<!doctype linuxdoc system>

<article>
<title>ca65 Users Guide
<author><url url="mailto:uz@cc65.org" name="Ullrich von Bassewitz">,<newline>
<url url="mailto:greg.king5@verizon.net" name="Greg King">

<abstract>
ca65 is a powerful macro assembler for the 6502, 65C02, and 65816 CPUs. It is
used as a companion assembler for the cc65 crosscompiler, but it may also be
used as a standalone product.
</abstract>

<!-- Table of contents -->
<toc>

<!-- Begin the document -->

<sect>Overview<p>

ca65 is a replacement for the ra65 assembler that was part of the cc65 C
compiler, originally developed by John R. Dunning. I had some problems with
ra65 and the copyright does not permit some things which I wanted to be
possible, so I decided to write a completely new assembler/linker/archiver
suite for the cc65 compiler. ca65 is part of this suite.

Some parts of the assembler (code generation and some routines for symbol
table handling) are taken from an older crossassembler named a816 written
by me a long time ago.


<sect1>Design criteria<p>

Here's a list of the design criteria, that I considered important for the
development:

<itemize>

<item>  The assembler must support macros. Macros are not essential, but they
        make some things easier, especially when you use the assembler in the
        backend of a compiler.
<item>  The assembler must support the newer 65C02 and 65816 CPUs. I have been
        thinking about a 65816 backend for the C compiler, and even my old
        a816 assembler had support for these CPUs, so this wasn't really a
        problem.
<item>  The assembler must produce relocatable code. This is necessary for the
        compiler support, and it is more convenient.
<item>  Conditional assembly must be supported. This is a must for bigger
        projects written in assembler (like Elite128).
<item>  The assembler must support segments, and it must support more than
        three segments (this is the count, most other assemblers support).
        Having more than one code segments helps developing code for systems
        with a divided ROM area (like the C64).
<item>  The linker must be able to resolve arbitrary expressions. It should
        be able to get things like
<tscreen><verb>
        .import S1, S2
        .export Special
        Special = 2*S1 + S2/7
</verb></tscreen>
        right.
<item>  True lexical nesting for symbols. This is very convenient for larger
        assembly projects.
<item>  "Cheap" local symbols without lexical nesting for those quick, late
        night hacks.
<item>  I liked the idea of "options" as Anre Fachats .o65 format has it, so I
        introduced the concept into the object file format use by the new cc65
        binutils.
<item>  The assembler will be a one pass assembler. There was no real need for
        this decision, but I've written several multipass assemblers, and it
        started to get boring. A one pass assembler needs much more elaborated
        data structures, and because of that it's much more fun:-)
<item>  Non-GPLed code that may be used in any project without restrictions or
        fear of "GPL infecting" other code.
</itemize>
<p>


<sect>Usage<p>


<sect1>Command line option overview<p>

The assembler accepts the following options:

<tscreen><verb>
---------------------------------------------------------------------------
Usage: ca65 [options] file
Short options:
  -D name[=value]               Define a symbol
  -I dir                        Set an include directory search path
  -U                            Mark unresolved symbols as import
  -V                            Print the assembler version
  -W n                          Set warning level n
  -d                            Debug mode
  -g                            Add debug info to object file
  -h                            Help (this text)
  -i                            Ignore case of symbols
  -l name                       Create a listing file if assembly was ok
  -mm model                     Set the memory model
  -o name                       Name the output file
  -s                            Enable smart mode
  -t sys                        Set the target system
  -v                            Increase verbosity

Long options:
  --auto-import                 Mark unresolved symbols as import
  --bin-include-dir dir         Set a search path for binary includes
  --cpu type                    Set cpu type
  --create-dep name             Create a make dependency file
  --create-full-dep name        Create a full make dependency file
  --debug                       Debug mode
  --debug-info                  Add debug info to object file
  --feature name                Set an emulation feature
  --help                        Help (this text)
  --ignore-case                 Ignore case of symbols
  --include-dir dir             Set an include directory search path
  --large-alignment             Don't warn about large alignments
  --listing name                Create a listing file if assembly was ok
  --list-bytes n                Maximum number of bytes per listing line
  --memory-model model          Set the memory model
  --pagelength n                Set the page length for the listing
  --relax-checks                Disables some error checks
  --smart                       Enable smart mode
  --target sys                  Set the target system
  --verbose                     Increase verbosity
  --version                     Print the assembler version
  --warnings-as-errors          Treat warnings as errors
---------------------------------------------------------------------------
</verb></tscreen>


<sect1>Command line options in detail<p>

Here is a description of all the command line options:

<descrip>

  <label id="option--bin-include-dir">
  <tag><tt>--bin-include-dir dir</tt></tag>

  Name a directory which is searched for binary include files. The option
  may be used more than once to specify more than one directory to search. The
  current directory is always searched first before considering any
  additional directories. See also the section about <ref id="search-paths"
  name="search paths">.


  <label id="option--cpu">
  <tag><tt>--cpu type</tt></tag>

  Set the default for the CPU type. The option takes a parameter, which
  may be one of
  <itemize>
  <item>6502 - NMOS 6502 (all legal instructions)
  <item>6502X - NMOS 6502 with all undocumented instructions
  <item>6502DTV - the emulated CPU of the C64DTV device
  <item>65SC02 - first CMOS instruction set (no bit manipulation, no wai/stp)
  <item>65C02 - CMOS with Rockwell extensions
  <item>W65C02 - full CMOS instruction set (has bit manipulation and wai/stp)
  <item>65CE02 - CMOS with CSG extensions
  <item>4510 - the CPU of the Commodore C65
  <item>45GS02 - the CPU of the Commodore MEGA65
  <item>HuC6280 - the CPU of the PC engine
  <item>M740 - a Microcontroller by Mitsubishi
  <item>65816 - the CPU of the SNES, and the SCPU
  <item>sweet16 - an interpreter for a pseudo 16 bit CPU
  </itemize>


  <label id="option-create-dep">
  <tag><tt>--create-dep name</tt></tag>

  Tells the assembler to generate a file containing the dependency list for
  the assembled module in makefile syntax. The output is written to a file
  with the given name. The output does not include files passed via debug
  information to the assembler.


  <label id="option-create-full-dep">
  <tag><tt>--create-full-dep name</tt></tag>

  Tells the assembler to generate a file containing the dependency list for
  the assembled module in makefile syntax. The output is written to a file
  with the given name. The output does include files passed via debug
  information to the assembler.


  <tag><tt>-d, --debug</tt></tag>

  Enables debug mode, something that should not be needed for mere
  mortals:-)


  <label id="option--feature">
  <tag><tt>--feature name</tt></tag>

  Enable an emulation feature. This is identical as using <tt/.FEATURE/
  in the source with two exceptions: Feature names must be lower case, and
  each feature must be specified by using a separate <tt/--feature/ option,
  comma separated lists are not allowed.

  See the discussion of the <tt><ref id=".FEATURE" name=".FEATURE"></tt>
  command for a list of emulation features.


  <label id="option-g">
  <tag><tt>-g, --debug-info</tt></tag>

  When this option (or the equivalent control command <tt/.DEBUGINFO/) is
  used, the assembler will add a section to the object file that contains
  all symbols (including local ones) together with the symbol values and
  source file positions. The linker will put these additional symbols into
  the VICE label file, so even local symbols can be seen in the VICE
  monitor.


  <label id="option-h">
  <tag><tt>-h, --help</tt></tag>

  Print the short option summary shown above.


  <label id="option-i">
  <tag><tt>-i, --ignore-case</tt></tag>

  This option makes the assembler case insensitive on identifiers and labels.
  This option will override the default, but may itself be overridden by the
  <tt><ref id=".CASE" name=".CASE"></tt> control command.


  <label id="option-l">
  <tag><tt>-l name, --listing name</tt></tag>

  Generate an assembler listing with the given name. A listing file will
  never be generated in case of assembly errors.


  <label id="option--large-alignment">
  <tag><tt>--large-alignment</tt></tag>

  Disable warnings about a large combined alignment. See the discussion of the
  <tt><ref id=".ALIGN" name=".ALIGN"></tt> directive for further information.


  <label id="option--list-bytes">
  <tag><tt>--list-bytes n</tt></tag>

  Set the maximum number of bytes printed in the listing for one line of
  input. See the <tt><ref id=".LISTBYTES" name=".LISTBYTES"></tt> directive
  for more information. The value zero can be used to encode an unlimited
  number of printed bytes.


  <label id="option-mm">
  <tag><tt>-mm model, --memory-model model</tt></tag>

  Define the default memory model. Possible model specifiers are near, far and
  huge.


  <label id="option-o">
  <tag><tt>-o name</tt></tag>

  The default output name is the name of the input file with the extension
  replaced by ".o". If you don't like that, you may give another name with
  the -o option. The output file will be placed in the same directory as
  the source file, or, if -o is given, the full path in this name is used.


  <label id="option--pagelength">
  <tag><tt>--pagelength n</tt></tag>

  sets the length of a listing page in lines. See the <tt><ref
  id=".PAGELENGTH" name=".PAGELENGTH"></tt> directive for more information.


  <label id="option--relax-checks">
  <tag><tt>--relax-checks</tt></tag>

  Disables some error checks done by the assembler. This will allow code that is an
  error in most cases and flagged as such by the assembler, but can be valid
  in special situations.

  Disabled checks are:
<itemize>
<item>Address vs. fragment size: a byte sized load from an non-zeropage
  address is truncated instead of producing an error.
<item>Indirect jump on page boundary: <tt>jmp (label)</tt> on a label that
  resides on a page boundary (<tt>$xxFF</tt>) fetches the second byte from the
  wrong address on 6502 CPUs, now allowed instead of producing an error.
</itemize>


  <label id="option-s">
  <tag><tt>-s, --smart-mode</tt></tag>

  In smart mode (enabled by -s or the <tt><ref id=".SMART" name=".SMART"></tt>
  pseudo instruction) the assembler will track usage of the <tt/REP/ and
  <tt/SEP/ instructions in 65816 mode and update the operand sizes
  accordingly. If the operand of such an instruction cannot be evaluated by
  the assembler (for example, because the operand is an imported symbol), a
  warning is issued.

  Beware: Since the assembler cannot trace the execution flow this may
  lead to false results in some cases. If in doubt, use the .ixx and .axx
  instructions to tell the assembler about the current settings. Smart
  mode is off by default.


  <label id="option-t">
  <tag><tt>-t sys, --target sys</tt></tag>

  Set the target system. This will enable translation of character strings and
  character constants into the character set of the target platform. The
  default for the target system is "none", which means that no translation
  will take place. The assembler supports the same target systems as the
  compiler, see <htmlurl url="ca65.html#option-t" name="there for a list">.

  Depending on the target, the default CPU type is also set. This can be
  overridden by using the <tt/<ref id="option--cpu" name="--cpu">/ option.


  <label id="option-v">
  <tag><tt>-v, --verbose</tt></tag>

  Increase the assembler verbosity. Usually only needed for debugging
  purposes. You may use this option more than one time for even more
  verbose output.


  <label id="option-D">
  <tag><tt>-D</tt></tag>

  This option allows you to define symbols on the command line. Without a
  value, the symbol is defined with the value zero. When giving a value,
  you may use the '&dollar;' prefix for hexadecimal symbols. Please note
  that for some operating systems, '&dollar;' has a special meaning, so
  you may have to quote the expression.


  <label id="option-I">
  <tag><tt>-I dir, --include-dir dir</tt></tag>

  Name a directory which is searched for include files. The option may be
  used more than once to specify more than one directory to search. The
  current directory is always searched first before considering any
  additional directories. See also the section about <ref id="search-paths"
  name="search paths">.


  <label id="option-U">
  <tag><tt>-U, --auto-import</tt></tag>

  Mark symbols that are not defined in the sources as imported symbols. This
  should be used with care since it delays error messages about typos and such
  until the linker is run. The compiler uses the equivalent of this switch
  (<tt><ref id=".AUTOIMPORT" name=".AUTOIMPORT"></tt>) to enable auto imported
  symbols for the runtime library. However, the compiler is supposed to
  generate code that runs through the assembler without problems, something
  which is not always true for assembler programmers.


  <label id="option-V">
  <tag><tt>-V, --version</tt></tag>

  Print the version number of the assembler. If you send any suggestions
  or bugfixes, please include the version number.


  <label id="option-W">
  <tag><tt>-Wn</tt></tag>

  Set the warning level for the assembler. Using -W2 the assembler will
  even warn about such things like unused imported symbols. The default
  warning level is 1, and it would probably be silly to set it to
  something lower.


  <label id="option--warnings-as-errors">
  <tag><tt>--warnings-as-errors</tt></tag>

  An error will be generated if any warnings were produced.


</descrip>
<p>



<sect>Search paths<label id="search-paths"><p>

Normal include files are searched in the following places:

<enum>
<item>The current file's directory.
<item>Any directory added with the <tt/<ref id="option-I" name="-I">/ option
on the command line.
<item>The value of the environment variable <tt/CA65_INC/ if it is defined.
<item>A subdirectory named <tt/asminc/ of the directory defined in the
      environment variable <tt/CC65_HOME/, if it is defined.
<item>An optionally compiled-in directory.
</enum>

Binary include files are searched in the following places:

<enum>
<item>The current file's directory.
<item>Any directory added with the <tt/<ref id="option--bin-include-dir"
name="--bin-include-dir">/ option on the command line.
</enum>



<sect>Input format<p><label id="input-format">

<sect1>Assembler syntax<p>

The assembler accepts the standard 6502/65816 assembler syntax. One line may
contain a label (which is identified by a colon), and, in addition to the
label, an assembler mnemonic, a macro, or a control command (see section <ref
id="control-commands" name="Control Commands"> for supported control
commands). Alternatively, the line may contain a symbol definition using
the '=' token. Everything after a semicolon is handled as a comment (that is,
it is ignored).

Here are some examples for valid input lines:

<tscreen><verb>
        Label:                          ; A label and a comment
                lda     #$20            ; A 6502 instruction plus comment
        L1:     ldx     #$20            ; Same with label
        L2:     .byte   "Hello world"   ; Label plus control command
                mymac   $20             ; Macro expansion
                MySym = 3*L1            ; Symbol definition
        MaSym   = Label                 ; Another symbol
</verb></tscreen>

The assembler accepts

<itemize>
<item>all valid 6502 mnemonics when in <ref id="6502-mode" name="6502 mode">
      (the default or after the
      <tt><ref id=".P02" name=".P02"></tt> command was given).
<item>all valid 6502 mnemonics, plus a set of illegal instructions, when in
      <ref id="6502X-mode" name="6502X mode"> (after the
      <tt><ref id=".P02X" name=".P02X"></tt> command was given).
<item>all valid 6502DTV mnemonics when in <ref id="DTV-mode" name="DTV mode"> (after the
      <tt><ref id=".PDTV" name=".PDTV"></tt> command was given).
<item>all valid 65SC02 mnemonics when in <ref id="65SC02-mode" name="65SC02 mode"> (after the
      <tt><ref id=".PSC02" name=".PSC02"></tt> command was given).
<item>all valid 65C02 mnemonics when in <ref id="65C02-mode" name="65C02 mode"> (after the
      <tt><ref id=".PC02" name=".PC02"></tt> command was given).
<item>all valid W65C02 mnemonics when in <ref id="W65C02-mode" name="W65C02 mode"> (after the
      <tt><ref id=".PWC02" name=".PWC02"></tt> command was given).
<item>all valid 65CE02 mnemonics when in <ref id="65CE02-mode" name="65CE02 mode"> (after the
      <tt><ref id=".PCE02" name=".PCE02"></tt> command was given).
<item>all valid 4510 mnemonics when in <ref id="4510-mode" name="4510 mode"> (after the
      <tt><ref id=".P4510" name=".P4510"></tt> command was given).
<item>all valid 45GS02 mnemonics when in <ref id="45GS02-mode" name="45GS02 mode"> (after the
      <tt><ref id=".P45GS02" name=".P45GS02"></tt> command was given).
<item>all valid HuC6280 mnemonics when in <ref id="HUC6280-mode" name="HuC6280 mode"> (after the
      <tt><ref id=".P6280" name=".P6280"></tt> command was given).
<item>all valid M740 mnemonics when in <ref id="M740-mode" name="M740 mode"> (after the
      <tt><ref id=".PM740" name=".PM740"></tt> command was given).
<item>all valid 65816 mnemonics when in <ref id="65816-mode" name="65816 mode"> (after the
      <tt><ref id=".P816" name=".P816"></tt> command was given).
</itemize>

for more details on the various CPUs, see <tt><htmlurl url="cpus.html" name="here"></tt>.

On 6502-derived platforms the <tt/BRK/ instruction has an optional signature
byte. If omitted, the assembler will only produce only 1 byte.

<tscreen><verb>
                brk                     ; 1-byte:  $00
                brk     $34             ; 2-bytes: $00 $34
                brk     #$34            ; 2-bytes: $00 $34
</verb></tscreen>

<sect2>6502 mode<label id="6502-mode"><p>

In 6502 mode (which is the default) the assembler accepts all regular "legal"
6502 mnemonics and addressing modes.

<sect2>6502X mode<label id="6502X-mode"><p>

6502X mode is an extension to the normal 6502 mode. In this mode, several
mnemonics for undocumented instructions of the NMOS 6502 CPUs are accepted.

Note: Since these instructions are undocumented, there are no official mnemonics
for them.

<itemize>
<item><tt>ALR: A:=(A and #{imm})/2;</tt>
<item><tt>ANC: A:= A and #{imm};</tt> Generates opcode &dollar;0B.
<item><tt>ANE: A:= (A or CONST) and X and #{imm};</tt>
<item><tt>ARR: A:=(A and #{imm})/2;</tt>
<item><tt>AXS: X:=A and X-#{imm};</tt>
<item><tt>DCP: {addr}:={addr}-1; A-{addr};</tt>
<item><tt>ISC: {addr}:={addr}+1; A:=A-{addr};</tt>
<item><tt>JAM:</tt>
<item><tt>LAS: A,X,S:={addr} and S;</tt>
<item><tt>LAX: A,X:={addr};</tt>
<item><tt>NOP: #{imm}; zp; zp,x; abs; abs,x</tt>
<item><tt>RLA: {addr}:={addr}rol; A:=A and {addr};</tt>
<item><tt>RRA: {addr}:={addr}ror; A:=A adc {addr};</tt>
<item><tt>SAX: {addr}:=A and X;</tt>
<item><tt>SHA: {addr}:=A and X and {addr hi +1};</tt>
<item><tt>SHX: {addr}:=X and {addr hi +1};</tt>
<item><tt>SHY: {addr}:=Y and {addr hi +1};</tt>
<item><tt>SLO: {addr}:={addr}*2; A:=A or {addr};</tt>
<item><tt>SRE: {addr}:={addr}/2; A:=A xor {addr};</tt>
<item><tt>TAS: {addr}:=A and X and {addr hi +1}; SP:=A and X;</tt>
</itemize>


<sect2>DTV mode<label id="DTV-mode"><p>

The C64DTV CPU is based on the 6510, but adds some instructions, and does not
support all undocumented instructions.

<itemize>
<item><tt>bra {rel}</tt> Generates opcode &dollar;12.
<item><tt>sac #{imm}</tt> Generates opcode &dollar;32.
<item><tt>sir #{imm}</tt> Generates opcode &dollar;42.
</itemize>

Supported undocumented instructions:

<itemize>
<item><tt>ALR: A:=(A and #{imm})/2;</tt>
<item><tt>ANC: A:=A and #{imm};</tt> Generates opcode &dollar;0B.
<item><tt>ARR: A:=(A and #{imm})/2;</tt>
<item><tt>AXS: X:=A and X-#{imm};</tt>
<item><tt>LAS: A,X,S:={addr} and S;</tt>
<item><tt>LAX: A,X:={addr};</tt>
<item><tt>NOP: #{imm}; zp; zp,x; abs; abs,x</tt>
<item><tt>RLA: {addr}:={addr}rol; A:=A and {addr};</tt>
<item><tt>RRA: {addr}:={addr}ror; A:=A adc {addr};</tt>
<item><tt>SHX: {addr}:=X and {addr hi +1};</tt>
<item><tt>SHY: {addr}:=y and {addr hi +1};</tt>
</itemize>


<sect2>65SC02 mode<label id="65SC02-mode"><p>

65SC02 mode supports all regular 6502 instructions, plus the original CMOS
instructions.


<sect2>65C02 mode (CMOS with Rockwell extensions)<label id="65C02-mode"><p>

65C02 mode supports all original CMOS instructions, plus the Rockwell (bit
manipulation instructions) extensions.


<sect2>W65C02 mode (CMOS with WDC extensions)<label id="W65C02-mode"><p>

W65C02 mode supports the Rockwell extensions, plus wai and stp.


<sect2>65CE02 mode<label id="65CE02-mode"><p>

All 65CE02 instructions are accepted, plus the Rockwell extensions.


<sect2>4510 mode<label id="4510-mode"><p>

The 4510 is a microcontroller that is the core of the Commodore C65 aka C64DX.
It contains among other functions a slightly modified 65CE02/4502 CPU, to allow
address mapping for 20 bits of address space (1 megabyte addressable area).

As compared to the description of the CPU in the
<url url="http://www.zimmers.net/anonftp/pub/cbm/c65/c65manualupdated.txt.gz"
name="C65 System Specification">
<url url="https://raw.githubusercontent.com/MEGA65/c65-specifications/master/c65manualupdated.txt"
name="(updated version)"> uses these changes:
<itemize>
<item><tt>LDA (d,SP),Y</tt> may also be written as <tt>LDA (d,S),Y</tt>
(matching the 65816 notation).
<item>All branch instruction allow now 16 bit offsets. To use a 16 bit
branch you have to prefix these with an "L" (e.g. "<tt>LBNE</tt>" instead of
"<tt>BNE</tt>"). This might change at a later implementation of the assembler.
</itemize>

For more information about the Commodore C65/C64DX and the 4510 CPU, see
<url url="http://www.zimmers.net/anonftp/pub/cbm/c65/"> and
<url url="https://en.wikipedia.org/wiki/Commodore_65" name="Wikipedia">.

<sect2>45GS02 mode<label id="45GS02-mode"><p>

The 45GS02 is a microcontroller that is the core of the MEGA65.
It is an extension of the 4510 CPU and adds 32-bit addressing and a 32-bit
pseudo register Q that is comprised of the four registers A, X, Y, and Z.

<sect2>HUC6280 mode (CMOS with Hudson extensions)<label id="HUC6280-mode"><p>

The HUC6280 is a superset of 65C02, used in the PC Engine.


<sect2>M740 mode<label id="M740-mode"><p>

The M740 is a microcontroller by Mitsubishi, which was marketed for embedded
devices in the mid 80s. It is a superset of 6502, and a subset of 65SC02, plus
some new instructions.

For more information about the M740 Controllers, see
<url url="https://en.wikipedia.org/wiki/Mitsubishi_740" name="Wikipedia">.


<sect2>65816 mode<label id="65816-mode"><p><p>

In 65816 mode, several aliases are accepted, in addition to the official
mnemonics:

<itemize>
<item><tt>CPA</tt> is an alias for <tt>CMP</tt>
<item><tt>DEA</tt> is an alias for <tt>DEC A</tt>
<item><tt>INA</tt> is an alias for <tt>INC A</tt>
<item><tt>SWA</tt> is an alias for <tt>XBA</tt>
<item><tt>TAD</tt> is an alias for <tt>TCD</tt>
<item><tt>TAS</tt> is an alias for <tt>TCS</tt>
<item><tt>TDA</tt> is an alias for <tt>TDC</tt>
<item><tt>TSA</tt> is an alias for <tt>TSC</tt>
</itemize>

The <tt/MVN/ and <tt/MVP/ instructions accept two different argument forms.
Either two bank bytes may be given with a <tt/#/ prefix,
or two far addresses whose high byte will be used.

<tscreen><verb>
                mvn     #^src, #^dst       ; bank of src to bank of dst
                mvn     src, dst           ; bank of src to bank of dst
                mvp     #$12, #$78         ; bank $12 to $78
                mvp     $123456, $789ABC   ; bank $12 to $78
</verb></tscreen>

also see <ref id="long_jsr_jmp_rts" name="long_jsr_jmp_rts">
 <ref id=".SMART" name=".SMART">
 <ref id=".A8" name=".A8">
 <ref id=".A16" name=".A16">
 <ref id=".I8" name=".I8">
 <ref id=".I16" name=".I16">


<sect2>sweet16 mode<label id="sweet16-mode"><p>

SWEET 16 is an interpreter for a pseudo 16 bit CPU written by Steve Wozniak
for the Apple ][ machines. It is available in the Apple ][ ROM. ca65 can
generate code for this pseudo CPU when switched into sweet16 mode. The
following is special in sweet16 mode:

<itemize>

<item>The '@' character denotes indirect addressing and is no longer available
for cheap local labels. If you need cheap local labels, you will have to
switch to another lead character using the <tt/<ref id=".LOCALCHAR"
name=".LOCALCHAR">/ command.

<item>Registers are specified using <tt/R0/ .. <tt/R15/. In sweet16 mode,
these identifiers are reserved words.

</itemize>

Please note that the assembler does neither supply the interpreter needed for
SWEET 16 code, nor the zero page locations needed for the SWEET 16 registers,
nor does it call the interpreter. All this must be done by your program. Apple
][ programmers do probably know how to use sweet16 mode.

For more information about SWEET 16, see
<url url="http://www.6502.org/source/interpreters/sweet16.htm">.


<sect1>Number format<p>

For literal values, the assembler accepts the widely used number formats: A
preceding '&dollar;' or a trailing 'h' denotes a hex value, a preceding '%'
denotes a binary value, and a bare number is interpreted as a decimal. There
are currently no octal values and no floats.


<sect1>Conditional assembly<p>

Please note that when using the conditional directives (<tt/.IF/ and friends),
the input must consist of valid assembler tokens, even in <tt/.IF/ branches
that are not assembled. The reason for this behaviour is that the assembler
must still be able to detect the ending tokens (like <tt/.ENDIF/), so
conversion of the input stream into tokens still takes place. As a consequence
conditional assembly directives may <bf/not/ be used to prevent normal text
(used as a comment or similar) from being assembled. <p>


<sect>Expressions<p>


<sect1>Expression evaluation<p>

All expressions are evaluated with (at least) 32 bit precision. An
expression may contain constant values and any combination of internal and
external symbols. Expressions that cannot be evaluated at assembly time
are stored inside the object file for evaluation by the linker.
Expressions referencing imported symbols must always be evaluated by the
linker.


<sect1>Size of an expression result<p>

Sometimes, the assembler must know about the size of the value that is the
result of an expression. This is usually the case, if a decision has to be
made, to generate a zero page or an absolute memory references. In this
case, the assembler has to make some assumptions about the result of an
expression:

<itemize>
<item>  If the result of an expression is constant, the actual value is
        checked to see if it's a byte sized expression or not.
<item>  If the expression is explicitly casted to a byte sized expression by
        one of the '&gt;', '&lt;' or '^' operators, it is a byte expression.
<item>  If this is not the case, and the expression contains a symbol,
        explicitly declared as zero page symbol (by one of the .importzp or
        .exportzp instructions), then the whole expression is assumed to be
        byte sized.
<item>  If the expression contains symbols that are not defined, and these
        symbols are local symbols, the enclosing scopes are searched for a
        symbol with the same name. If one exists and this symbol is defined,
        its attributes are used to determine the result size.
<item>  In all other cases the expression is assumed to be word sized.
</itemize>

Note: If the assembler is not able to evaluate the expression at assembly
time, the linker will evaluate it and check for range errors as soon as
the result is known.


<sect1>Boolean expressions<p>

In the context of a boolean expression, any non zero value is evaluated as
true, any other value to false. The result of a boolean expression is 1 if
it's true, and zero if it's false. There are boolean operators with extreme
low precedence with version 2.x (where x &gt; 0). The <tt/.AND/ and <tt/.OR/
operators are shortcut operators. That is, if the result of the expression is
already known, after evaluating the left hand side, the right hand side is
not evaluated.


<sect1>Constant expressions<p>

Sometimes an expression must evaluate to a constant without looking at any
further input. One such example is the <tt/<ref id=".IF" name=".IF">/ command
that decides if parts of the code are assembled or not. An expression used in
the <tt/.IF/ command cannot reference a symbol defined later, because the
decision about the <tt/.IF/ must be made at the point when it is read. If the
expression used in such a context contains only constant numerical values,
there is no problem. When unresolvable symbols are involved it may get harder
for the assembler to determine if the expression is actually constant, and it
is even possible to create expressions that aren't recognized as constant.
Simplifying the expressions will often help.

In cases where the result of the expression is not needed immediately, the
assembler will delay evaluation until all input is read, at which point all
symbols are known. So using arbitrary complex constant expressions is no
problem in most cases.



<sect1>Available operators<label id="operators"><p>

<table>
<tabular ca="clc">
<bf/Operator/| <bf/Description/| <bf/Precedence/@<hline>
| Built-in string functions| 0@
~|~|~@
| Built-in pseudo-variables| 1@
| Built-in pseudo-functions| 1@
+| Unary positive| 1@
-| Unary negative| 1@
&tilde;<newline>
.BITNOT| Unary bitwise not| 1@
&lt;<newline>
.LOBYTE| Unary low-byte operator| 1@
&gt;<newline>
.HIBYTE| Unary high-byte operator| 1@
^<newline>
.BANKBYTE| Unary bank-byte operator| 1@
~|~|~@
*| Multiplication| 2@
/| Division| 2@
.MOD| Modulo operator| 2@
&amp;<newline>
.BITAND| Bitwise and| 2@
^<newline>
.BITXOR| Binary bitwise xor| 2@
&lt;&lt;<newline>
.SHL| Shift-left operator| 2@
&gt;&gt;<newline>
.SHR| Shift-right operator| 2@
~|~|~@
+| Binary addition| 3@
-| Binary subtraction| 3@
&verbar;<newline>
.BITOR| Bitwise or| 3@
~|~|~@
= | Compare operator (equal)| 4@
&lt;&gt;| Compare operator (not equal)| 4@
&lt;| Compare operator (less)| 4@
&gt;| Compare operator (greater)| 4@
&lt;=| Compare operator (less or equal)| 4@
&gt;=| Compare operator (greater or equal)| 4@
~|~|~@
&amp;&amp;<newline>
.AND| Boolean and| 5@
.XOR| Boolean xor| 5@
~|~|~@
&verbar;&verbar;<newline>
.OR| Boolean or| 6@
~|~|~@
!<newline>
.NOT| Boolean not| 7
</tabular>
<caption>Available operators, sorted by precedence
</table>

To force a specific order of evaluation, parentheses may be used, as usual.



<sect>Symbols and labels<p>

A symbol or label is an identifier that starts with a letter and is followed
by letters and digits. Depending on some features enabled (see
<tt><ref id="at_in_identifiers" name="at_in_identifiers"></tt>,
<tt><ref id="dollar_in_identifiers" name="dollar_in_identifiers"></tt> and
<tt><ref id="leading_dot_in_identifiers" name="leading_dot_in_identifiers"></tt>)
other characters may be present. Use of identifiers consisting of a single
character will not work in all cases, because some of these identifiers are
reserved keywords (for example "A" is not a valid identifier for a label,
because it is the keyword for the accumulator).

The assembler allows you to use symbols instead of naked values to make
the source more readable. There are a lot of different ways to define and
use symbols and labels, giving a lot of flexibility.

<sect1>Numeric constants<p>

Numeric constants are defined using the equal sign or the label assignment
operator. After doing

<tscreen><verb>
        two = 2
</verb></tscreen>

may use the symbol "two" in every place where a number is expected, and it is
evaluated to the value 2 in this context. The label assignment operator is
almost identical, but causes the symbol to be marked as a label, so it may be
handled differently in a debugger:

<tscreen><verb>
        io := $d000
</verb></tscreen>

The right side can of course be an expression:

<tscreen><verb>
        four = two * two
</verb></tscreen>


<label id="variables">
<sect1>Numeric variables<p>

Within macros and other control structures (<tt><ref id=".REPEAT"
name=".REPEAT"></tt>, ...) it is sometimes useful to have some sort of
variable. This can be achieved by the <tt>.SET</tt> operator. It creates a
symbol that may get assigned a different value later:

<tscreen><verb>
        four .set 4
        lda     #four           ; Loads 4 into A
        four .set 3
        lda     #four           ; Loads 3 into A
</verb></tscreen>

Since the value of the symbol can change later, it must be possible to
evaluate it when used (no delayed evaluation as with normal symbols). So the
expression used as the value must be constant.

Following is an example for a macro that generates a different label each time
it is used. It uses the <tt><ref id=".SPRINTF" name=".SPRINTF"></tt> function
and a numeric variable named <tt>lcount</tt>.

<tscreen><verb>
        .lcount .set 0          ; Initialize the counter

        .macro  genlab
                .ident (.sprintf ("L%04X", lcount)):
                lcount .set lcount + 1
        .endmacro
</verb></tscreen>


<sect1>Standard labels<p>

A label is defined by writing the name of the label at the start of the line
(before any instruction mnemonic, macro or pseudo directive), followed by a
colon. This will declare a symbol with the given name and the value of the
current program counter.


<sect1>Local labels and symbols<p>

Using the <tt><ref id=".PROC" name=".PROC"></tt> directive, it is possible to
create regions of code where the names of labels and symbols are local to this
region. They are not known outside of this region and cannot be accessed from
there. Such regions may be nested like PROCEDUREs in Pascal.

See the description of the <tt><ref id=".PROC" name=".PROC"></tt>
directive for more information.


<sect1>Cheap local labels<p>

Cheap local labels are defined like standard labels, but the name of the
label must begin with a special symbol (usually '@', but this can be
changed by the <tt><ref id=".LOCALCHAR" name=".LOCALCHAR"></tt>
directive).

Cheap local labels are visible only between two non cheap labels. As soon as a
standard symbol is encountered (this may also be a local symbol if inside a
region defined with the <tt><ref id=".PROC" name=".PROC"></tt> directive), the
cheap local symbol goes out of scope.

You may use cheap local labels as an easy way to reuse common label
names like "Loop". Here is an example:

<tscreen><verb>
        Clear:  lda    #$00             ; Global label
                ldy    #$20
        @Loop:  sta    Mem,y            ; Local label
                dey
                bne    @Loop            ; Ok
                rts
        Sub:    ...                     ; New global label
                bne    @Loop            ; ERROR: Unknown identifier!
</verb></tscreen>


<sect1>Unnamed labels<p>

If you really want to write messy code, there are also unnamed labels. To define
an unnamed label, use sole <tt>:</tt>.

To reference an unnamed label, use <tt>:</tt> with several <tt>-</tt> or <tt>+</tt> characters.
The <tt>-</tt> characters will create a back reference (n'th label backwards),
the <tt>+</tt> will create a forward reference (n'th label in forward direction).
As an alternative, angle brackets <tt>&lt;</tt> and <tt>&gt;</tt> may be used
instead of <tt>-</tt> and <tt>+</tt> with the same meaning.

Example:

<tscreen><verb>
        cpy #0
        beq :++
    :
        sta $2007
        dey
        bne :-
    :
        rts
</verb></tscreen>

Unnamed labels may make even short sections of code hard to understand, because
you have to count labels to find branch targets. It's better to prefer the
"cheap" local labels. Nevertheless, unnamed labels are convenient in some
situations, so it's up to your discretion.

<em/Note:/ <ref id="scopes" name="Scopes"> organize named symbols, not
unnamed ones, so scopes don't have an effect on unnamed labels.


<sect1>Using macros to define labels and constants<p>

While there are drawbacks with this approach, it may be handy in a few rare
situations. Using <tt><ref id=".DEFINE" name=".DEFINE"></tt>, it is possible
to define symbols or constants that may be used elsewhere. One of the
advantages is that you can use it to define string constants (this is not
possible with the other symbol types).

Please note: <tt/.DEFINE/ style macros do token replacements on a low level,
so the names do not adhere to scoping, diagnostics may be misleading, there
are no symbols to look up in the map file, and there is no debug info.
Especially the first problem in the list can lead to very nasty programming
errors. Because of these problems, the general advice is, <bf/NOT/ do use
<tt/.DEFINE/ if you don't have to.

Example:

<tscreen><verb>
        .DEFINE two     2
        .DEFINE version "SOS V2.3"

        four = two * two        ; Ok
        .byte   version         ; Ok

        .PROC                   ; Start local scope
        two = 3                 ; Will give "2 = 3" - invalid!
        .ENDPROC
</verb></tscreen>


<sect1>Symbols and <tt>.DEBUGINFO</tt><p>

If <tt><ref id=".DEBUGINFO" name=".DEBUGINFO"></tt> is enabled (or <ref
id="option-g" name="-g"> is given on the command line), global, local and
cheap local labels are written to the object file and will be available in the
symbol file via the linker. Unnamed labels are not written to the object file,
because they don't have a name which would allow to access them.



<sect>Scopes<label id="scopes"><p>

ca65 implements several sorts of scopes for symbols.

<sect1>Global scope<p>

All (non cheap local) symbols that are declared outside of any nested scopes
are in global scope.


<sect1>Cheap locals<p>

A special scope is the scope for cheap local symbols. It lasts from one non
local symbol to the next one, without any provisions made by the programmer.
All other scopes differ in usage but use the same concept internally.


<sect1>Generic nested scopes<p>

A nested scoped for generic use is started with <tt/<ref id=".SCOPE"
name=".SCOPE">/ and closed with <tt/<ref id=".ENDSCOPE" name=".ENDSCOPE">/.
The scope can have a name, in which case it is accessible from the outside by
using <ref id="scopesyntax" name="explicit scopes">. If the scope does not
have a name, all symbols created within the scope are local to the scope, and
aren't accessible from the outside.

A nested scope can access symbols from the local or from enclosing scopes by
name without using explicit scope names. In some cases there may be
ambiguities, for example if there is a reference to a local symbol that is not
yet defined, but a symbol with the same name exists in outer scopes:

<tscreen><verb>
        .scope  outer
                foo     = 2
                .scope  inner
                        lda     #foo
                        foo     = 3
                .endscope
        .endscope
</verb></tscreen>

In the example above, the <tt/lda/ instruction will load the value 3 into the
accumulator, because <tt/foo/ is redefined in the scope. However:

<tscreen><verb>
        .scope  outer
                foo     = $1234
                .scope  inner
                        lda     foo,x
                        foo     = $12
                .endscope
        .endscope
</verb></tscreen>

Here, <tt/lda/ will still load from <tt/$12,x/, but since it is unknown to the
assembler that <tt/foo/ is a zeropage symbol when translating the instruction,
absolute mode is used instead. In fact, the assembler will not use absolute
mode by default, but it will search through the enclosing scopes for a symbol
with the given name. If one is found, the address size of this symbol is used.
This may lead to errors:

<tscreen><verb>
        .scope  outer
                foo     = $12
                .scope  inner
                        lda     foo,x
                        foo     = $1234
                .endscope
        .endscope
</verb></tscreen>

In this case, when the assembler sees the symbol <tt/foo/ in the <tt/lda/
instruction, it will search for an already defined symbol <tt/foo/. It will
find <tt/foo/ in scope <tt/outer/, and a close look reveals that it is a
zeropage symbol. So the assembler will use zeropage addressing mode. If
<tt/foo/ is redefined later in scope <tt/inner/, the assembler tries to change
the address in the <tt/lda/ instruction already translated, but since the new
value needs absolute addressing mode, this fails, and an error message "Range
error" is output.

Of course the most simple solution for the problem is to move the definition
of <tt/foo/ in scope <tt/inner/ upwards, so it precedes its use. There may be
rare cases when this cannot be done. In these cases, you can use one of the
address size override operators:

<tscreen><verb>
        .scope  outer
                foo     = $12
                .scope  inner
                        lda     a:foo,x
                        foo     = $1234
                .endscope
        .endscope
</verb></tscreen>

This will cause the <tt/lda/ instruction to be translated using absolute
addressing mode, which means changing the symbol reference later does not
cause any errors.


<sect1>Nested procedures<p>

A nested procedure is created by use of <tt/<ref id=".PROC" name=".PROC">/. It
differs from a <tt/<ref id=".SCOPE" name=".SCOPE">/ in that it must have a
name, and a it will introduce a symbol with this name in the enclosing scope.
So

<tscreen><verb>
        .proc   foo
                ...
        .endproc
</verb></tscreen>

is actually the same as

<tscreen><verb>
        foo:
        .scope  foo
                ...
        .endscope
</verb></tscreen>

This is the reason why a procedure must have a name. If you want a scope
without a name, use <tt/<ref id=".SCOPE" name=".SCOPE">/.

<em/Note:/ As you can see from the example above, scopes and symbols live in
different namespaces. There can be a symbol named <tt/foo/ and a scope named
<tt/foo/ without any conflicts (but see the section titled <ref
id="scopesearch" name="&quot;Scope search order&quot;">).


<sect1>Structs, unions and enums<p>

Structs, unions and enums are explained in a <ref id="structs" name="separate
section">, I do only cover them here, because if they are declared with a
name, they open a nested scope, similar to <tt/<ref id=".SCOPE"
name=".SCOPE">/. However, when no name is specified, the behaviour is
different: In this case, no new scope will be opened, symbols declared within
a struct, union, or enum declaration will then be added to the enclosing scope
instead.


<sect1>Explicit scope specification<label id="scopesyntax"><p>

Accessing symbols from other scopes is possible by using an explicit scope
specification, provided that the scope where the symbol lives in has a name.
The namespace token (<tt/::/) is used to access other scopes:

<tscreen><verb>
        .scope  foo
        bar:    .word   0
        .endscope

                ...
                lda     #foo::bar        ; Access bar in scope foo
</verb></tscreen>

The only way to deny access to a scope from the outside is to declare a scope
without a name (using the <tt/<ref id=".SCOPE" name=".SCOPE">/ command).

A special syntax is used to specify the global scope: If a symbol or scope is
preceded by the namespace token, the global scope is searched:

<tscreen><verb>
        bar     = 3

        .scope  foo
                bar     = 2
                lda     #::bar  ; Access the global bar (which is 3)
        .endscope
</verb></tscreen>


<sect1>Scope search order<label id="scopesearch"><p>

The assembler searches for a scope in a similar way as for a symbol. First, it
looks in the current scope, and then it walks up the enclosing scopes until
the scope is found.

However, one important thing to note when using explicit scope syntax is, that
a symbol may be accessed before it is defined, but a scope may <bf/not/ be
used without a preceding definition. This means that in the following
example:

<tscreen><verb>
        .scope  foo
                bar     = 3
        .endscope

        .scope  outer
                lda     #foo::bar  ; Will load 3, not 2!
                .scope  foo
                        bar     = 2
                .endscope
        .endscope
</verb></tscreen>

the reference to the scope <tt/foo/ will use the global scope, and not the
local one, because the local one is not visible at the point where it is
referenced.

Things get more complex if a complete chain of scopes is specified:

<tscreen><verb>
        .scope  foo
                .scope  outer
                        .scope  inner
                                bar = 1
                        .endscope
                .endscope
                .scope  another
                        .scope  nested
                                lda     #outer::inner::bar      ; 1
                        .endscope
                .endscope
        .endscope

        .scope  outer
                .scope  inner
                        bar = 2
                .endscope
        .endscope
</verb></tscreen>

When <tt/outer::inner::bar/ is referenced in the <tt/lda/ instruction, the
assembler will first search in the local scope for a scope named <tt/outer/.
Since none is found, the enclosing scope (<tt/another/) is checked. There is
still no scope named <tt/outer/, so scope <tt/foo/ is checked, and finally
scope <tt/outer/ is found. Within this scope, <tt/inner/ is searched, and in
this scope, the assembler looks for a symbol named <tt/bar/.

Please note that once the anchor scope is found, all following scopes
(<tt/inner/ in this case) are expected to be found exactly in this scope. The
assembler will search the scope tree only for the first scope (if it is not
anchored in the root scope). Starting from there on, there is no flexibility,
so if the scope named <tt/outer/ found by the assembler does not contain a
scope named <tt/inner/, this would be an error, even if such a pair does exist
(one level up in global scope).

Ambiguities that may be introduced by this search algorithm may be removed by
anchoring the scope specification in the global scope. In the example above,
if you want to access the "other" symbol <tt/bar/, you would have to write:

<tscreen><verb>
        .scope  foo
                .scope  outer
                        .scope  inner
                                bar = 1
                        .endscope
                .endscope
                .scope  another
                        .scope  nested
                                lda     #::outer::inner::bar    ; 2
                        .endscope
                .endscope
        .endscope

        .scope  outer
                .scope  inner
                        bar = 2
                .endscope
        .endscope
</verb></tscreen>


<sect>Address sizes and memory models<label id="address-sizes"><p>

<sect1>Address sizes<p>

ca65 assigns each segment and each symbol an address size. This is true, even
if the symbol is not used as an address. You may also think of a value range
of the symbol instead of an address size.

Possible address sizes are:

<itemize>
<item>Zeropage or direct (8 bits)
<item>Absolute (16 bits)
<item>Far (24 bits)
<item>Long (32 bits)
</itemize>

Since the assembler uses default address sizes for the segments and symbols,
it is usually not necessary to override the default behaviour. In cases, where
it is necessary, the following keywords may be used to specify address sizes:

<itemize>
<item>DIRECT, ZEROPAGE or ZP for zeropage addressing (8 bits).
<item>ABSOLUTE, ABS or NEAR for absolute addressing (16 bits).
<item>FAR for far addressing (24 bits).
<item>LONG or DWORD for long addressing (32 bits).
</itemize>


<sect1>Address sizes of segments<p>

The assembler assigns an address size to each segment. Since the
representation of a label within this segment is "segment start + offset",
labels will inherit the address size of the segment they are declared in.

The address size of a segment may be changed, by using an optional address
size modifier. See the <tt/<ref id=".SEGMENT" name="segment directive">/ for
an explanation on how this is done.


<sect1>Address sizes of symbols<p>

The address size of a symbol can be specified with a prefix:

<itemize>
<item>z: zeropage addressing (8 bits).
<item>a: absolute addressing (16 bits).
<item>f: far addressing (24 bits).
</itemize>

The zeropage addressing override can be used to ensure the use of optimal
zeropage instructions, or correct cases where the size isn't yet known
due to the single-pass assembly model.

The larger addressing overrides can be used to promote a smaller address
to absolute or far addressing, instead of being automatically fit into
a smaller addressing type.


<sect1>Memory models<p>

The default address size of a segment depends on the memory model used. Since
labels inherit the address size from the segment they are declared in,
changing the memory model is an easy way to change the address size of many
symbols at once.




<sect>Pseudo variables<label id="pseudo-variables"><p>

Pseudo variables are readable in all cases, and in some special cases also
writable.

<sect1><tt>*</tt><p>

  Reading this pseudo variable will return the program counter at the start
  of the current input line.

  Assignment to this variable is possible when <tt/<ref id=".FEATURE"
  name=".FEATURE pc_assignment">/ is used. Note: You should not use
  assignments to <tt/*/, use <tt/<ref id=".ORG" name=".ORG">/ instead.


<sect1><tt>.ASIZE</tt><label id=".ASIZE"><p>

  Reading this pseudo variable will return the current size of the
  Accumulator in bits.

  For the 65816 instruction set .ASIZE will return either 8 or 16, depending
  on the current size of the operand in immediate accu addressing mode.

  For all other CPU instruction sets, .ASIZE will always return 8.

  Example:

  <tscreen><verb>
        ; Reverse Subtract with Accumulator
        ; A = memory - A
        .macro rsb param
                .if .asize = 8
                        eor     #$ff
                .else
                        eor     #$ffff
                .endif
                sec
                adc     param
        .endmacro
  </verb></tscreen>

  See also: <tt><ref id=".ISIZE" name=".ISIZE"></tt>


<sect1><tt>.CPU</tt><label id=".CPU"><p>

  Reading this pseudo variable will give a constant integer value that
  tells which CPU is currently enabled. It can also tell which instruction
  set the CPU is able to translate. The value read from the pseudo variable
  should be further examined by using one of the following constants:

<tscreen><verb>
    CPU_6502
    CPU_65SC02
    CPU_65C02
    CPU_65816
    CPU_SWEET16
    CPU_HUC6280
    CPU_4510
    CPU_45GS02
    CPU_6502DTV
    CPU_M740
</verb></tscreen>

Above constants may be used to determine the exact type of the currently
enabled CPU. In addition to that, for each CPU instruction set, another
constant is defined:

<tscreen><verb>
    CPU_ISET_6502
    CPU_ISET_65SC02
    CPU_ISET_65C02
    CPU_ISET_65816
    CPU_ISET_SWEET16
    CPU_ISET_HUC6280
    CPU_ISET_4510
    CPU_ISET_45GS02
    CPU_ISET_6502DTV
    CPU_ISET_M740
</verb></tscreen>

<!-- Sorry but explaining these with the changes from #2751 is too cringy for
     me - must be done by someone else. The remainder is from the old
     ".macpack cpu" section"

The value read from the <tt/<ref id=".CPU" name=".CPU">/ pseudo variable may
be checked with <tt/<ref id="operators" name=".BITAND">/ to determine if the
currently enabled CPU supports a specific instruction set. For example the
65C02 supports all instructions of the 65SC02 CPU, so it has the
<tt/CPU_ISET_65SC02/ bit set in addition to its native <tt/CPU_ISET_65C02/
bit. Using

<tscreen><verb>
        .if (.cpu .bitand CPU_ISET_65SC02)
                lda     (c_sp)
        .else
                ldy     #$00
                lda     (c_sp),y
        .endif
</verb></tscreen>

it is possible to determine if the

<tscreen><verb>
                lda     (c_sp)
</verb></tscreen>

instruction is supported, which is the case for the 65SC02, 65C02 and 65816
CPUs (the latter two are upwards compatible to the 65SC02).

see section <ref id="6502-mode" name="6502 format"> and following.
-->

  <tt/.CPU/ may be used to replace the .IFPxx pseudo instructions or to
  construct even more complex expressions.

  Example:

  <tscreen><verb>
        .if     (.cpu .bitand CPU_ISET_65816)
                phx
                phy
        .else
                txa
                pha
                tya
                pha
        .endif
  </verb></tscreen>

  See also: <tt><ref id=".CAP" name=".CAP"></tt>



<sect1><tt>.ISIZE</tt><label id=".ISIZE"><p>

  Reading this pseudo variable will return the current size of the Index
  register in bits.

  For the 65816 instruction set .ISIZE will return either 8 or 16, depending
  on the current size of the operand in immediate index addressing mode.

  For all other CPU instruction sets, .ISIZE will always return 8.

  See also: <tt><ref id=".ASIZE" name=".ASIZE"></tt>


<sect1><tt>.PARAMCOUNT</tt><label id=".PARAMCOUNT"><p>

  This builtin pseudo variable is only available in macros. It is replaced by
  the actual number of parameters that were given in the macro invocation.

  Example:

  <tscreen><verb>
        .macro  foo     arg1, arg2, arg3
        .if     .paramcount <> 3
        .error  "Too few parameters for macro foo"
        .endif
        ...
        .endmacro
  </verb></tscreen>

  See section <ref id="macros" name="Macros">.


<sect1><tt>.TIME</tt><label id=".TIME"><p>

  Reading this pseudo variable will give a constant integer value that
  represents the current time in POSIX standard (as seconds since the
  Epoch).

  It may be used to encode the time of translation somewhere in the created
  code.

  Example:

  <tscreen><verb>
        .dword  .time   ; Place time here
  </verb></tscreen>


<sect1><tt>.VERSION</tt><label id=".VERSION"><p>

  Reading this pseudo variable will give the assembler version according to
  the following formula:

        <tt>(VER_MAJOR * 0x100) + VER_MINOR</tt>

  The upper 8 bits are the major-, the lower 8 bits are the  minor version.

  Example:

  For example, version 47.11 of the assembler would have this macro defined as
  <tt/0x2f0b/.

  Note: until 2.19 this pseudo variable was defined as <tt>(VER_MAJOR * 0x100) + VER_MINOR * 0x10</tt> -
  which resulted in broken values starting at version 2.16 of the assembler. For
  this reason the value of this pseudo variable is considered purely informal - you should
  not use it to check for a specific assembler version and use different code
  according to the detected version - please update your code to work with the
  recent version of the assembler instead (There is very little reason to not use
  the most recent version - and even less to support older versions in your code).

<sect>Pseudo functions<label id="pseudo-functions"><p>

Pseudo functions expect their arguments in parentheses, and they have a result,
either a string or an expression value.


<sect1><tt>.ADDRSIZE</tt><label id=".ADDRSIZE"><p>

  The <tt/.ADDRSIZE/ function is used to return the internal address size
  associated with a symbol. This can be helpful in macros when knowing the address
  size of a symbol can help with custom instructions.

  Example:

  <tscreen><verb>
        .macro myLDA foo
                .if .ADDRSIZE(foo) = 1
                        ;do custom command based on zeropage addressing:
                        .byte 0A5h, foo
                .elseif .ADDRSIZE(foo) = 2
                        ;do custom command based on absolute addressing:
                        .byte 0ADh
                        .word foo
                .elseif .ADDRSIZE(foo) = 0
                        ; no address size defined for this symbol:
                        .out .sprintf("Error, address size unknown for symbol %s", .string(foo))
                .endif
        .endmacro
  </verb></tscreen>


<sect1><tt>.BANK</tt><label id=".BANK"><p>

  The <tt/.BANK/ function is used to support systems with banked memory. The
  argument is an expression with exactly one segment reference -- usually a
  label. The function result is the value of the <tt/bank/ attribute assigned
  to the run memory area of the segment. Please see the linker documentation
  for more information about memory areas and their attributes.

  The value of <tt/.BANK/ can be used to switch memory so that a memory bank
  containing specific data is available.

  The <tt/bank/ attribute is a 32-bit integer, and so is the result of the
  <tt/.BANK/ function. You will have to use <tt><ref id=".LOBYTE"
  name=".LOBYTE"></tt> or similar functions to address just part of it.

  Please note that <tt/.BANK/ always will get evaluated in the link stage, so
  an expression containing <tt/.BANK/ never can be used where a constant, known
  result is expected (for example, with <tt/.RES/).

  Example:

  <tscreen><verb>
        .segment "BANK1"
        .proc   banked_func_1
                ...
        .endproc

        .segment "BANK2"
        .proc   banked_func_2
                ...
        .endproc

        .proc   bank_table
                .addr   banked_func_1
                .byte   <.BANK (banked_func_1)

                .addr   banked_func_2
                .byte   <.BANK (banked_func_2)
        .endproc
  </verb></tscreen>



<sect1><tt>.BANKBYTE</tt><label id=".BANKBYTE"><p>

  The function returns the bank byte (that is, bits 16-23) of its argument.
  It works identical to the '^' operator.

  See: <tt><ref id=".HIBYTE" name=".HIBYTE"></tt>,
       <tt><ref id=".LOBYTE" name=".LOBYTE"></tt>


<sect1><tt>.BLANK</tt><label id=".BLANK"><p>

  Builtin function. The function evaluates its argument in parentheses and yields
  "false" if the argument is non blank (there is an argument), and "true" if
  there is no argument.  The token list that makes up the function argument
  may optionally be enclosed in curly braces. This allows the inclusion of
  tokens that would otherwise terminate the list (the closing right
  parenthesis). The curly braces are not considered part of the list, a list
  just consisting of curly braces is considered to be empty.

  As an example, the <tt/.IFBLANK/ statement may be replaced by

  <tscreen><verb>
        .if     .blank({arg})
  </verb></tscreen>



<sect1><tt>.CAP, .CAPABILITY</tt><label id=".CAP"><p>

  Builtin function. The function allows to check for capabilities of the
  currently selected CPU or target system. It must be called with a comma
  separated list of identifiers and returns non zero if all of the given
  capabilities are available. Otherwise it returns zero.

  Existing capabilities are:

<descrip>

  <tag><tt>CPU_HAS_BITIMM</tt></tag>
  Checks for the availability of the "bit #imm" instruction.

  <tag><tt>CPU_HAS_BRA8</tt></tag>
  Checks for the availability of a short (8 bit) branch.

  <tag><tt>CPU_HAS_INA</tt></tag>
  Checks for the availability of accu inc/dec instructions.

  <tag><tt>CPU_HAS_PUSHXY</tt></tag>
  Checks for the capability to push and pop the X and Y registers.

  <tag><tt>CPU_HAS_ZPIND</tt></tag>
  Checks for the availability of the "zeropage indirect" addressing mode as it
  is implemented in the 65SC02 CPU.

  <tag><tt>CPU_HAS_STZ</tt></tag>
  Checks for the availability of the "store zero" instruction as it is
  implemented in the 65SC02 CPU.

</descrip>

  Case is ignored when checking the identifiers. The <tt/.cap/ function is
  easier to use than checking <tt/.cpu/ and requires no intimate knowledge
  of all instruction sets. For more detailed checking <tt/.cpu/ is still
  available.

  Example:

  <tscreen><verb>
        .if     .cap(CPU_HAS_BRA, CPU_HAS_PUSHXY)
                phx
                bra     L1
        .else
                txa
                pha
                jmp     L1
        .endif
  </verb></tscreen>

  See also: <tt><ref id=".CPU" name=".CPU"></tt>



<sect1><tt>.CONCAT</tt><label id=".CONCAT"><p>

  Builtin string function. The function allows to concatenate a list of string
  constants separated by commas. The result is a string constant that is the
  concatenation of all arguments. This function is most useful in macros and
  when used together with the <tt/.STRING/ builtin function. The function may
  be used in any case where a string constant is expected.

  Example:

  <tscreen><verb>
        .include        .concat ("myheader", ".", "inc")
  </verb></tscreen>

  This is the same as the command

  <tscreen><verb>
        .include        "myheader.inc"
  </verb></tscreen>


<sect1><tt>.CONST</tt><label id=".CONST"><p>

  Builtin function. The function evaluates its argument in parentheses and
  yields "true" if the argument is a constant expression (that is, an
  expression that yields a constant value at assembly time) and "false"
  otherwise. As an example, the .IFCONST statement may be replaced by

  <tscreen><verb>
        .if     .const(a + 3)
  </verb></tscreen>


<sect1><tt>.DEF, .DEFINED</tt><label id=".DEFINED"><p>

  Builtin function. The function expects an identifier as argument in parentheses.
  The argument is evaluated, and the function yields "true" if the identifier
  is a symbol that already is defined somewhere in the source file up to the
  current position. Otherwise, the function yields false. As an example, the
  <tt><ref id=".IFDEF" name=".IFDEF"></tt> statement may be replaced by

  <tscreen><verb>
        .if     .defined(a)
  </verb></tscreen>


<sect1><tt>.DEFINEDMACRO</tt><label id=".DEFINEDMACRO"><p>

  Builtin function. The function expects an identifier as argument in parentheses.
  The argument is evaluated, and the function yields "true" if the identifier
  already has been defined as the name of a macro. Otherwise, the function yields
  false. Example:

  <tscreen><verb>
        .macro add foo
                clc
                adc foo
        .endmacro

        .if     .definedmacro(add)
                add #$01
        .else
                clc
                adc #$01
        .endif
  </verb></tscreen>


<sect1><tt>.HIBYTE</tt><label id=".HIBYTE"><p>

  The function returns the high byte (that is, bits 8-15) of its argument.
  It works identical to the '>' operator.

  See: <tt><ref id=".LOBYTE" name=".LOBYTE"></tt>,
       <tt><ref id=".BANKBYTE" name=".BANKBYTE"></tt>


<sect1><tt>.HIWORD</tt><label id=".HIWORD"><p>

  The function returns the high word (that is, bits 16-31) of its argument.

  See: <tt><ref id=".LOWORD" name=".LOWORD"></tt>


<sect1><tt>.IDENT</tt><label id=".IDENT"><p>

  The function expects a string as its argument, and converts this argument
  into an identifier. If the string starts with the current <tt/<ref
  id=".LOCALCHAR" name=".LOCALCHAR">/, it will be converted into a cheap local
  identifier, otherwise it will be converted into a normal identifier.

  Example:

  <tscreen><verb>
        .macro  makelabel       arg1, arg2
                .ident (.concat (arg1, arg2)):
        .endmacro

                makelabel       "foo", "bar"

                .word           foobar          ; Valid label
  </verb></tscreen>


<sect1><tt>.ISMNEM, .ISMNEMONIC</tt><label id=".ISMNEMONIC"><p>

  Builtin function. The function expects an identifier as argument in parentheses.
  The argument is evaluated, and the function yields "true" if the identifier
  is defined as an instruction mnemonic that is recognized by the assembler.
  Example:

  <tscreen><verb>
        .if     .not .ismnemonic(ina)
                .macro ina
                        clc
                        adc #$01
                .endmacro
        .endif
  </verb></tscreen>


<sect1><tt>.LEFT</tt><label id=".LEFT"><p>

  Builtin function. Extracts the left part of a given token list.

  Syntax:

  <tscreen><verb>
        .LEFT (&lt;int expr&gt;, &lt;token list&gt;)
  </verb></tscreen>

  The first integer expression gives the number of tokens to extract from
  the token list. The second argument is the token list itself. The token
  list may optionally be enclosed into curly braces. This allows the
  inclusion of tokens that would otherwise terminate the list (the closing
  right paren in the given case).

  Example:

  To check in a macro if the given argument has a '#' as first token
  (immediate addressing mode), use something like this:

  <tscreen><verb>
        .macro  ldax    arg
                ...
                .if (.match (.left (1, {arg}), #))

                ; ldax called with immediate operand
                ...

                .endif
                ...
        .endmacro
  </verb></tscreen>

  See also the <tt><ref id=".MID" name=".MID"></tt> and <tt><ref id=".RIGHT"
  name=".RIGHT"></tt> builtin functions.


<sect1><tt>.LOBYTE</tt><label id=".LOBYTE"><p>

  The function returns the low byte (that is, bits 0-7) of its argument.
  It works identical to the '<' operator.

  See: <tt><ref id=".HIBYTE" name=".HIBYTE"></tt>,
       <tt><ref id=".BANKBYTE" name=".BANKBYTE"></tt>


<sect1><tt>.LOWORD</tt><label id=".LOWORD"><p>

  The function returns the low word (that is, bits 0-15) of its argument.

  See: <tt><ref id=".HIWORD" name=".HIWORD"></tt>


<sect1><tt>.MATCH</tt><label id=".MATCH"><p>

  Builtin function. Matches two token lists against each other. This is
  most useful within macros, since macros are not stored as strings, but
  as lists of tokens.

  The syntax is

  <tscreen><verb>
        .MATCH(&lt;token list #1&gt;, &lt;token list #2&gt;)
  </verb></tscreen>

  Both token list may contain arbitrary tokens with the exception of the
  terminator token (comma resp. right parenthesis) and

  <itemize>
  <item>end-of-line
  <item>end-of-file
  </itemize>

  The token lists may optionally be enclosed into curly braces. This allows
  the inclusion of tokens that would otherwise terminate the list (the closing
  right paren in the given case). Often a macro parameter is used for any of
  the token lists.

  Please note that the function does only compare tokens, not token
  attributes. So any number is equal to any other number, regardless of the
  actual value. The same is true for strings. If you need to compare tokens
  <em/and/ token attributes, use the <tt><ref id=".XMATCH"
  name=".XMATCH"></tt> function.

  Example:

  Assume the macro <tt/ASR/, that will shift right the accumulator by one,
  while honoring the sign bit. The builtin processor instructions will allow
  an optional "A" for accu addressing for instructions like <tt/ROL/ and
  <tt/ROR/. We will use the <tt><ref id=".MATCH" name=".MATCH"></tt> function
  to check for this and print and error for invalid calls.

  <tscreen><verb>
        .macro  asr     arg

                .if (.not .blank(arg)) .and (.not .match ({arg}, a))
                .error "Syntax error"
                .endif

                cmp     #$80            ; Bit 7 into carry
                lsr     a               ; Shift carry into bit 7

        .endmacro
  </verb></tscreen>

  The macro will only accept no arguments, or one argument that must be the
  reserved keyword "A".

  See: <tt><ref id=".XMATCH" name=".XMATCH"></tt>


<sect1><tt>.MAX</tt><label id=".MAX"><p>

  Builtin function. The result is the larger of two values.

  The syntax is

  <tscreen><verb>
        .MAX (&lt;value #1&gt;, &lt;value #2&gt;)
  </verb></tscreen>

  Example:

  <tscreen><verb>
        ; Reserve space for the larger of two data blocks
        savearea:       .res .max (.sizeof (foo), .sizeof (bar))
  </verb></tscreen>

  See: <tt><ref id=".MIN" name=".MIN"></tt>


<sect1><tt>.MID</tt><label id=".MID"><p>

  Builtin function. Takes a starting index, a count and a token list as
  arguments. Will return part of the token list.

  Syntax:

  <tscreen><verb>
        .MID (&lt;int expr&gt;, &lt;int expr&gt;, &lt;token list&gt;)
  </verb></tscreen>

  The first integer expression gives the starting token in the list (the first
  token has index 0). The second integer expression gives the number of tokens
  to extract from the token list. The third argument is the token list itself.
  The token list may optionally be enclosed into curly braces. This allows the
  inclusion of tokens that would otherwise terminate the list (the closing
  right paren in the given case).

  Example:

  To check in a macro if the given argument has a '<tt/#/' as first token
  (immediate addressing mode), use something like this:

    <tscreen><verb>
        .macro  ldax    arg
                ...
                .if (.match (.mid (0, 1, {arg}), #))

                ; ldax called with immediate operand
                ...

                .endif
                ...
        .endmacro
  </verb></tscreen>

  See also the <tt><ref id=".LEFT" name=".LEFT"></tt> and <tt><ref id=".RIGHT"
  name=".RIGHT"></tt> builtin functions.


<sect1><tt>.MIN</tt><label id=".MIN"><p>

  Builtin function. The result is the smaller of two values.

  The syntax is

  <tscreen><verb>
        .MIN (&lt;value #1&gt;, &lt;value #2&gt;)
  </verb></tscreen>

  Example:

  <tscreen><verb>
        ; Reserve space for some data, but 256 bytes maximum
        savearea:       .res .min (.sizeof (foo), 256)
  </verb></tscreen>

  See: <tt><ref id=".MAX" name=".MAX"></tt>


<sect1><tt>.REF, .REFERENCED</tt><label id=".REFERENCED"><p>

  Builtin function. The function expects an identifier as argument in parentheses.
  The argument is evaluated, and the function yields "true" if the identifier
  is a symbol that has already been referenced somewhere in the source file up
  to the current position. Otherwise the function yields false. As an example,
  the <tt><ref id=".IFREF" name=".IFREF"></tt> statement may be replaced by

  <tscreen><verb>
        .if     .referenced(a)
  </verb></tscreen>

  See: <tt><ref id=".DEFINED" name=".DEFINED"></tt>


<sect1><tt>.RIGHT</tt><label id=".RIGHT"><p>

  Builtin function. Extracts the right part of a given token list.

  Syntax:

  <tscreen><verb>
        .RIGHT (&lt;int expr&gt;, &lt;token list&gt;)
  </verb></tscreen>

  The first integer expression gives the number of tokens to extract from the
  token list. The second argument is the token list itself.  The token list
  may optionally be enclosed into curly braces. This allows the inclusion of
  tokens that would otherwise terminate the list (the closing right paren in
  the given case).

  See also the <tt><ref id=".LEFT" name=".LEFT"></tt> and <tt><ref id=".MID"
  name=".MID"></tt> builtin functions.


<sect1><tt>.SIZEOF</tt><label id=".SIZEOF"><p>

  <tt/.SIZEOF()/ is a pseudo function that returns the size of its argument.
  The argument can be a struct/union, a struct member, a scope/procedure, or a
  label. In the case of a procedure or label, its size is defined by the
  amount of data placed in the segment where the label is relative to. If a
  line of code switches segments (for example, in a macro), data placed in
  other segments does not count for the size.

  Please note that a symbol or scope must exist before it can be used together
  with <tt/.SIZEOF()/ (that may get relaxed later, but always will be true for
  scopes). A scope has preference over a symbol with the same name; so, if the
  last part of a name represents both a scope and a symbol, then the scope is
  chosen over the symbol.

  After the following code:

  <tscreen><verb>
        .struct Point                   ; Struct size = 4
                xcoord  .word
                ycoord  .word
        .endstruct

        P:      .tag    Point           ; Declare a point
        @P:     .tag    Point           ; Declare another point

        .code
        .proc   Code
                nop
                .proc   Inner
                        nop
                .endproc
                nop
        .endproc

        .proc   Data
        .data                           ; Segment switch!!!
                .res    4
        .endproc
  </verb></tscreen>

  <descrip>
    <tag><tt/.sizeof(Point)/</tag>
    will have the value 4, because this is the size of struct <tt/Point/.

    <tag><tt/.sizeof(Point::xcoord)/</tag>
    will have the value 2, because this is the size of the member <tt/xcoord/
    in struct <tt/Point/.

    <tag><tt/.sizeof(P)/</tag>
    will have the value 4, this is the size of the data declared on the same
    source line as the label <tt/P/, which is in the same segment that <tt/P/
    is relative to.

    <tag><tt/.sizeof(@P)/</tag>
    will have the value 4, see above. The example demonstrates that <tt/.SIZEOF/
    does also work for cheap local symbols.

    <tag><tt/.sizeof(Code)/</tag>
    will have the value 3, since this is amount of data emitted into the code
    segment, the segment that was active when <tt/Code/ was entered. Note that
    this value includes the amount of data emitted in child scopes (in this
    case <tt/Code::Inner/).

    <tag><tt/.sizeof(Code::Inner)/</tag>
    will have the value 1 as expected.

    <tag><tt/.sizeof(Data)/</tag>
    will have the value 0. Data is emitted within the scope <tt/Data/, but since
    the segment is switched after entry, this data is emitted into another
    segment.
  </descrip>


<sect1><tt>.SPRINTF</tt><label id=".SPRINTF"><p>

  Builtin function. It expects a format string as first argument. The number
  and type of the following arguments depend on the format string. The format
  string is similar to the one of the C <tt/printf/ function. Missing things
  are: Length modifiers, variable width.

  The result of the function is a string.

  Example:

  <tscreen><verb>
        num     = 3

        ; Generate an identifier:
        .ident (.sprintf ("%s%03d", "label", num)):
  </verb></tscreen>


<sect1><tt>.STRAT</tt><label id=".STRAT"><p>

  Builtin function. The function accepts a string and an index as
  arguments and returns the value of the character at the given position
  as an integer value. The index is zero based.

  Example:

  <tscreen><verb>
        .macro  M       Arg
                ; Check if the argument string starts with '#'
                .if (.strat (Arg, 0) = '#')
                ...
                .endif
        .endmacro
  </verb></tscreen>


<sect1><tt>.STRING</tt><label id=".STRING"><p>

  Builtin function. The function accepts an argument in parentheses and converts
  this argument into a string constant. The argument may be an identifier, or
  a constant numeric value.

  Since you can use a string in the first place, the use of the function may
  not be obvious. However, it is useful in macros, or more complex setups.

  Example:

  <tscreen><verb>
        ; Emulate other assemblers:
        .macro  section name
                .segment        .string(name)
        .endmacro
  </verb></tscreen>


<sect1><tt>.STRLEN</tt><label id=".STRLEN"><p>

  Builtin function. The function accepts a string argument in parentheses and
  evaluates to the length of the string.

  Example:

  The following macro encodes a string as a pascal style string with
  a leading length byte.

  <tscreen><verb>
        .macro  PString Arg
                .byte   .strlen(Arg), Arg
        .endmacro
  </verb></tscreen>


<sect1><tt>.TCOUNT</tt><label id=".TCOUNT"><p>

  Builtin function. The function accepts a token list in parentheses. The function
  result is the number of tokens given as argument. The token list may
  optionally be enclosed into curly braces which are not considered part of
  the list and not counted. Enclosement in curly braces allows the inclusion
  of tokens that would otherwise terminate the list (the closing right paren
  in the given case).

  Example:

  The <tt/ldax/ macro accepts the '#' token to denote immediate addressing (as
  with the normal 6502 instructions). To translate it into two separate 8 bit
  load instructions, the '#' token has to get stripped from the argument:

  <tscreen><verb>
        .macro  ldax    arg
                .if (.match (.mid (0, 1, {arg}), #))
                ; ldax called with immediate operand
                lda     #<(.right (.tcount ({arg})-1, {arg}))
                ldx     #>(.right (.tcount ({arg})-1, {arg}))
                .else
                ...
                .endif
        .endmacro
  </verb></tscreen>


<sect1><tt>.XMATCH</tt><label id=".XMATCH"><p>

  Builtin function. Matches two token lists against each other. This is
  most useful within macros, since macros are not stored as strings, but
  as lists of tokens.

  The syntax is

  <tscreen><verb>
        .XMATCH(&lt;token list #1&gt;, &lt;token list #2&gt;)
  </verb></tscreen>

  Both token list may contain arbitrary tokens with the exception of the
  terminator token (comma resp. right parenthesis) and

  <itemize>
  <item>end-of-line
  <item>end-of-file
  </itemize>

  The token lists may optionally be enclosed into curly braces. This allows
  the inclusion of tokens that would otherwise terminate the list (the closing
  right paren in the given case). Often a macro parameter is used for any of
  the token lists.

  The function compares tokens <em/and/ token values. If you need a function
  that just compares the type of tokens, have a look at the <tt><ref
  id=".MATCH" name=".MATCH"></tt> function.

  See: <tt><ref id=".MATCH" name=".MATCH"></tt>



<sect>Control commands<label id="control-commands"><p>

Here's a list of all control commands and a description, what they do:


<sect1><tt>.A16</tt><label id=".A16"><p>

  Valid only in 65816 mode. Assume the accumulator is 16 bit.

  Note: This command will not emit any code, it will tell the assembler to
  create 16 bit operands for immediate accumulator addressing mode.

  See also: <tt><ref id=".SMART" name=".SMART"></tt>


<sect1><tt>.A8</tt><label id=".A8"><p>

  Valid only in 65816 mode. Assume the accumulator is 8 bit.

  Note: This command will not emit any code, it will tell the assembler to
  create 8 bit operands for immediate accu addressing mode.

  See also: <tt><ref id=".SMART" name=".SMART"></tt>


<sect1><tt>.ADDR</tt><label id=".ADDR"><p>

  Define word sized data. In 6502 mode, this is an alias for <tt/.WORD/ and
  may be used for better readability if the data words are address values. In
  65816 mode, the address is forced to be 16 bit wide to fit into the current
  segment. See also <tt><ref id=".FARADDR" name=".FARADDR"></tt>. The command
  must be followed by a sequence of (not necessarily constant) expressions.

  Example:

  <tscreen><verb>
        .addr   $0D00, $AF13, _Clear
  </verb></tscreen>

  See: <tt><ref id=".FARADDR" name=".FARADDR"></tt>, <tt><ref id=".WORD"
       name=".WORD"></tt>


<sect1><tt>.ALIGN</tt><label id=".ALIGN"><p>

  Align data to a given boundary. The command expects a constant integer
  argument in the range 1 ... 65536, plus an optional second argument
  in byte range. If there is a second argument, it is used as fill value,
  otherwise the value defined in the linker configuration file is used
  (the default for this value is zero).

  <tt/.ALIGN/ will insert fill bytes, and the number of fill bytes depend of
  the final address of the segment. <tt/.ALIGN/ cannot insert a variable
  number of bytes, since that would break address calculations within the
  module. So each <tt/.ALIGN/ expects the segment to be aligned to a multiple
  of the alignment, because that allows the number of fill bytes to be
  calculated in advance by the assembler. You are therefore required to
  specify a matching alignment for the segment in the linker config. The
  linker will output a warning if the alignment of the segment is less than
  what is necessary to have a correct alignment in the object file.

  Example:

  <tscreen><verb>
        .align  256
  </verb></tscreen>

  Some unexpected behaviour might occur if there are multiple <tt/.ALIGN/
  commands with different arguments. To allow the assembler to calculate the
  number of fill bytes in advance, the alignment of the segment must be a
  multiple of each of the alignment factors. This may result in unexpectedly
  large alignments for the segment within the module.

  Example:

  <tscreen><verb>
        .align  15
        .byte   15
        .align  18
        .byte   18
  </verb></tscreen>

  For the assembler to be able to align correctly, the segment must be aligned
  to the least common multiple of 15 and 18 which is 90. The assembler will
  calculate this automatically and will mark the segment with this value.

  Unfortunately, the combined alignment may get rather large without the user
  knowing about it, wasting space in the final executable. If we add another
  alignment to the example above

  <tscreen><verb>
        .align  15
        .byte   15
        .align  18
        .byte   18
        .align  251
        .byte   0
  </verb></tscreen>

  the assembler will force a segment alignment to the least common multiple of
  15, 18 and 251 - which is 22590. To protect the user against errors, when the
  combined alignment is larger than the explicitly requested alignments,
  the assembler will issue a warning if it also exceeds 256. The command line
  option <tt><ref id="option--large-alignment" name="--large-alignment"></tt>
  will disable this warning.

  Please note that with only alignments that are a power of two, a warning will
  never occur, because the least common multiple of powers to the same base is
  always simply the larger one.



<sect1><tt>.ASCIIZ</tt><label id=".ASCIIZ"><p>

  Define a string with a trailing zero.

  Example:

  <tscreen><verb>
        Msg:    .asciiz "Hello world"
  </verb></tscreen>

  This will put the string "Hello world" followed by a binary zero into
  the current segment. There may be more strings separated by commas, but
  the binary zero is only appended once (after the last one). Strings will
  be translated using the current character mapping definition.

See: <tt><ref id=".BYTE" name=".BYTE"></tt>,<tt><ref id=".CHARMAP" name=".CHARMAP"></tt>,
     <tt><ref id=".LITERAL" name=".LITERAL"></tt>


<sect1><tt>.ASSERT</tt><label id=".ASSERT"><p>

  Add an assertion. The command is followed by an expression, an action
  specifier, and an optional message that is output in case the assertion
  fails. If no message was given, the string "Assertion failed" is used. The
  action specifier may be one of <tt/warning/, <tt/error/, <tt/ldwarning/ or
  <tt/lderror/. In the former two cases, the assertion is evaluated by the
  assembler if possible, and in any case, it's also passed to the linker in
  the object file (if one is generated). The linker will then evaluate the
  expression when segment placement has been done.

  Example:

  <tscreen><verb>
        .assert         * = $8000, error, "Code not at $8000"
  </verb></tscreen>

  The example assertion will check that the current location is at $8000,
  when the output file is written, and abort with an error if this is not
  the case. More complex expressions are possible. The action specifier
  <tt/warning/ outputs a warning, while the <tt/error/ specifier outputs
  an error message. In the latter case, generation of the output file is
  suppressed in both the assembler and linker.


<sect1><tt>.AUTOIMPORT</tt><label id=".AUTOIMPORT"><p>

  Is followed by a plus or a minus character. When switched on (using a
  +), undefined symbols are automatically marked as import instead of
  giving errors. When switched off (which is the default so this does not
  make much sense), this does not happen and an error message is
  displayed. The state of the autoimport flag is evaluated when the
  complete source was translated, before outputting actual code, so it is
  <em/not/ possible to switch this feature on or off for separate sections
  of code. The last setting is used for all symbols.

  You should probably not use this switch because it delays error
  messages about undefined symbols until the link stage. The cc65
  compiler (which is supposed to produce correct assembler code in all
  circumstances, something which is not true for most assembler
  programmers) will insert this command to avoid importing each and every
  routine from the runtime library.

  Example:

  <tscreen><verb>
        .autoimport     +       ; Switch on auto import
  </verb></tscreen>

<sect1><tt>.BANKBYTES</tt><label id=".BANKBYTES"><p>

  Define byte sized data by extracting only the bank byte (that is, bits 16-23) from
  each expression.  This is equivalent to <tt><ref id=".BYTE" name=".BYTE"></tt> with
  the operator '^' prepended to each expression in its list.

  Example:

  <tscreen><verb>
        .define MyTable TableItem0, TableItem1, TableItem2, TableItem3

        TableLookupLo:   .lobytes   MyTable
        TableLookupHi:   .hibytes   MyTable
        TableLookupBank: .bankbytes MyTable
  </verb></tscreen>

  which is equivalent to

  <tscreen><verb>
        TableLookupLo:   .byte &lt;TableItem0, &lt;TableItem1, &lt;TableItem2, &lt;TableItem3
        TableLookupHi:   .byte &gt;TableItem0, &gt;TableItem1, &gt;TableItem2, &gt;TableItem3
        TableLookupBank: .byte ^TableItem0, ^TableItem1, ^TableItem2, ^TableItem3
  </verb></tscreen>

  See also: <tt><ref id=".BYTE" name=".BYTE"></tt>,
            <tt><ref id=".HIBYTES" name=".HIBYTES"></tt>,
            <tt><ref id=".LOBYTES" name=".LOBYTES"></tt>


<sect1><tt>.BSS</tt><label id=".BSS"><p>

  Switch to the BSS segment. The name of the BSS segment is always "BSS",
  so this is a shortcut for

  <tscreen><verb>
        .segment  "BSS"
  </verb></tscreen>

  See also the <tt><ref id=".SEGMENT" name=".SEGMENT"></tt> command.


<sect1><tt>.BYT, .BYTE</tt><label id=".BYTE"><p>

  Define byte sized data. Must be followed by a sequence of (byte ranged)
  expressions or strings. Strings will be translated using the current
  character mapping definition.

  Example:

  <tscreen><verb>
        .byte   "Hello "
        .byt    "world", $0D, $00
  </verb></tscreen>

See: <tt><ref id=".ASCIIZ" name=".ASCIIZ"></tt>,<tt><ref id=".CHARMAP" name=".CHARMAP"></tt>
     <tt><ref id=".LITERAL" name=".LITERAL"></tt>


<sect1><tt>.CASE</tt><label id=".CASE"><p>

  Switch on or off case sensitivity on identifiers. The default is off
  (that is, identifiers are case sensitive), but may be changed by the
  -i switch on the command line.
  The command can be followed by a '+' or '-' character to switch the
  option on or off respectively.

  Example:

  <tscreen><verb>
        .case   -               ; Identifiers are not case sensitive
  </verb></tscreen>


<sect1><tt>.CHARMAP</tt><label id=".CHARMAP"><p>

  Apply a custom mapping for characters for the commands <tt><ref id=".ASCIIZ"
  name=".ASCIIZ"></tt> and <tt><ref id=".BYTE" name=".BYTE"></tt>. The command
  is followed by two numbers. The first one is the index of the source character
  (range 0..255);
  the second one is the mapping (range 0..255). The mapping applies to all
  character and string constants <em/when/ they generate output; and, overrides
  a mapping table specified with the <tt><ref id="option-t" name="-t"></tt>
  command line switch.

  Example:
  <tscreen><verb>
  .charmap        $41, $61        ; Map 'A' to 'a'
  </verb></tscreen>


<sect1><tt>.CODE</tt><label id=".CODE"><p>

  Switch to the CODE segment. The name of the CODE segment is always
  "CODE", so this is a shortcut for

  <tscreen><verb>
        .segment  "CODE"
  </verb></tscreen>

  See also the <tt><ref id=".SEGMENT" name=".SEGMENT"></tt> command.


<sect1><tt>.CONDES</tt><label id=".CONDES"><p>

  Export a symbol and mark it in a special way. The linker is able to build
  tables of all such symbols. This may be used to automatically create a list
  of functions needed to initialize linked library modules.

  Note: The linker has a feature to build a table of marked routines, but it
  is your code that must call these routines, so just declaring a symbol with
  <tt/.CONDES/ does nothing by itself.

  All symbols are exported as an absolute (16 bit) symbol. You don't need to
  use an additional <tt><ref id=".EXPORT" name=".EXPORT"></tt> statement, this
  is implied by <tt/.CONDES/.

  <tt/.CONDES/ is followed by the type, which may be <tt/constructor/,
  <tt/destructor/ or a numeric value between 0 and 6 (where 0 is the same as
  specifying <tt/constructor/ and 1 is equal to specifying <tt/destructor/).
  The <tt><ref id=".CONSTRUCTOR" name=".CONSTRUCTOR"></tt>, <tt><ref
  id=".DESTRUCTOR" name=".DESTRUCTOR"></tt> and <tt><ref id=".INTERRUPTOR"
  name=".INTERRUPTOR"></tt> commands are actually shortcuts for <tt/.CONDES/
  with a type of <tt/constructor/ resp. <tt/destructor/ or <tt/interruptor/.

  After the type, an optional priority may be specified. Higher numeric values
  mean higher priority. If no priority is given, the default priority of 7 is
  used. Be careful when assigning priorities to your own module constructors
  so they won't interfere with the ones in the cc65 library.

  Example:

  <tscreen><verb>
        .condes         ModuleInit, constructor
        .condes         ModInit, 0, 16
  </verb></tscreen>

  See the <tt><ref id=".CONSTRUCTOR" name=".CONSTRUCTOR"></tt>, <tt><ref
  id=".DESTRUCTOR" name=".DESTRUCTOR"></tt> and <tt><ref id=".INTERRUPTOR"
  name=".INTERRUPTOR"></tt> commands and the separate section <ref id="condes"
  name="Module constructors/destructors"> explaining the feature in more
  detail.


<sect1><tt>.CONSTRUCTOR</tt><label id=".CONSTRUCTOR"><p>

  Export a symbol and mark it as a module constructor. This may be used
  together with the linker to build a table of constructor subroutines that
  are called by the startup code.

  Note: The linker has a feature to build a table of marked routines, but it
  is your code that must call these routines, so just declaring a symbol as
  constructor does nothing by itself.

  A constructor is always exported as an absolute (16 bit) symbol. You don't
  need to use an additional <tt/.export/ statement, this is implied by
  <tt/.constructor/. It may have an optional priority that is separated by a
  comma. Higher numeric values mean a higher priority. If no priority is
  given, the default priority of 7 is used. Be careful when assigning
  priorities to your own module constructors so they won't interfere with the
  ones in the cc65 library.

  Example:

  <tscreen><verb>
        .constructor    ModuleInit
        .constructor    ModInit, 16
  </verb></tscreen>

  See the <tt><ref id=".CONDES" name=".CONDES"></tt> and <tt><ref
  id=".DESTRUCTOR" name=".DESTRUCTOR"></tt> commands and the separate section
  <ref id="condes" name="Module constructors/destructors"> explaining the
  feature in more detail.


<sect1><tt>.DATA</tt><label id=".DATA"><p>

  Switch to the DATA segment. The name of the DATA segment is always
  "DATA", so this is a shortcut for

  <tscreen><verb>
        .segment  "DATA"
  </verb></tscreen>

  See also the <tt><ref id=".SEGMENT" name=".SEGMENT"></tt> command.


<sect1><tt>.DBYT</tt><label id=".DBYT"><p>

  Define word sized data with the hi and lo bytes swapped (use <tt/.WORD/ to
  create word sized data in native 65XX format). Must be followed by a
  sequence of (word ranged) expressions.

  Example:

  <tscreen><verb>
        .dbyt   $1234, $4512
  </verb></tscreen>

  This will emit the bytes

  <tscreen><verb>
        $12 $34 $45 $12
  </verb></tscreen>

  into the current segment in that order.


<sect1><tt>.DEBUGINFO</tt><label id=".DEBUGINFO"><p>

  Switch on or off debug info generation. The default is off (that is,
  the object file will not contain debug infos), but may be changed by the
  -g switch on the command line.
  The command can be followed by a '+' or '-' character to switch the
  option on or off respectively.

  Example:

  <tscreen><verb>
        .debuginfo      +       ; Generate debug info
  </verb></tscreen>


<sect1><tt>.DEFINE</tt><label id=".DEFINE"><p>

  Start a define style macro definition. The command is followed by an
  identifier (the macro name) and optionally by a list of formal arguments
  in parentheses.

  Please note that <tt/.DEFINE/ shares most disadvantages with its C
  counterpart, so the general advice is, <bf/NOT/ do use <tt/.DEFINE/ if you
  don't have to.

  See also the <tt><ref id=".UNDEFINE" name=".UNDEFINE"></tt> command and
  section <ref id="macros" name="Macros">.


<sect1><tt>.DELMAC, .DELMACRO</tt><label id=".DELMACRO"><p>

  Delete a classic macro (defined with <tt><ref id=".MACRO"
  name=".MACRO"></tt>) . The command is followed by the name of an
  existing macro. Its definition will be deleted together with the name.
  If necessary, another macro with this name may be defined later.

  See: <tt><ref id=".ENDMACRO" name=".ENDMACRO"></tt>,
       <tt><ref id=".EXITMACRO" name=".EXITMACRO"></tt>,
       <tt><ref id=".MACRO" name=".MACRO"></tt>

  See also section <ref id="macros" name="Macros">.


<sect1><tt>.DESTRUCTOR</tt><label id=".DESTRUCTOR"><p>

  Export a symbol and mark it as a module destructor. This may be used
  together with the linker to build a table of destructor subroutines that
  are called by the startup code.

  Note: The linker has a feature to build a table of marked routines, but it
  is your code that must call these routines, so just declaring a symbol as
  constructor does nothing by itself.

  A destructor is always exported as an absolute (16 bit) symbol. You don't
  need to use an additional <tt/.export/ statement, this is implied by
  <tt/.destructor/. It may have an optional priority that is separated by a
  comma. Higher numerical values mean a higher priority. If no priority is
  given, the default priority of 7 is used. Be careful when assigning
  priorities to your own module destructors so they won't interfere with the
  ones in the cc65 library.

  Example:

  <tscreen><verb>
        .destructor     ModuleDone
        .destructor     ModDone, 16
  </verb></tscreen>

  See the <tt><ref id=".CONDES" name=".CONDES"></tt> and <tt><ref
  id=".CONSTRUCTOR" name=".CONSTRUCTOR"></tt> commands and the separate
  section <ref id="condes" name="Module constructors/destructors"> explaining
  the feature in more detail.


<sect1><tt>.DWORD</tt><label id=".DWORD"><p>

  Define dword sized data (4 bytes) Must be followed by a sequence of
  expressions.

  Example:

  <tscreen><verb>
        .dword  $12344512, $12FA489
  </verb></tscreen>


<sect1><tt>.ELSE</tt><label id=".ELSE"><p>

  Conditional assembly: Reverse the current condition.


<sect1><tt>.ELSEIF</tt><label id=".ELSEIF"><p>

  Conditional assembly: Reverse current condition and test a new one.


<sect1><tt>.END</tt><label id=".END"><p>

  Forced end of assembly. Assembly stops at this point, even if the command
  is read from an include file.


<sect1><tt>.ENDENUM</tt><label id=".ENDENUM"><p>

  End a <tt><ref id=".ENUM" name=".ENUM"></tt> declaration.


<sect1><tt>.ENDIF</tt><label id=".ENDIF"><p>

  Conditional assembly: Close a <tt><ref id=".IF" name=".IF..."></tt> or
  <tt><ref id=".ELSE" name=".ELSE"></tt> branch.


<sect1><tt>.ENDMAC, .ENDMACRO</tt><label id=".ENDMACRO"><p>

  Marks the end of a macro definition. Note, <tt>.ENDMACRO</tt> should be on
  its own line to successfully end the macro definition. It is possible to use
  <tt><ref id=".DEFINE" name=".DEFINE"></tt> to create a symbol that references
  <tt>.ENDMACRO</tt> without ending the macro definition.

  Example:

  <tscreen><verb>
        .macro  new_mac
                .define startmac .macro
                .define endmac .endmacro
        .endmacro
  </verb></tscreen>

  See: <tt><ref id=".DELMACRO" name=".DELMACRO"></tt>,
       <tt><ref id=".EXITMACRO" name=".EXITMACRO"></tt>,
       <tt><ref id=".MACRO" name=".MACRO"></tt>

  See also section <ref id="macros" name="Macros">.


<sect1><tt>.ENDPROC</tt><label id=".ENDPROC"><p>

  End of the local lexical level (see <tt><ref id=".PROC" name=".PROC"></tt>).


<sect1><tt>.ENDREP, .ENDREPEAT</tt><label id=".ENDREPEAT"><p>

  End a <tt><ref id=".REPEAT" name=".REPEAT"></tt> block.


<sect1><tt>.ENDSCOPE</tt><label id=".ENDSCOPE"><p>

  End of the local lexical level (see <tt/<ref id=".SCOPE" name=".SCOPE">/).


<sect1><tt>.ENDSTRUCT</tt><label id=".ENDSTRUCT"><p>

  Ends a struct definition. See the <tt/<ref id=".STRUCT" name=".STRUCT">/
  command and the separate section named <ref id="structs" name="&quot;Structs
  and unions&quot;">.


<sect1><tt>.ENDUNION</tt><label id=".ENDUNION"><p>

  Ends a union definition. See the <tt/<ref id=".UNION" name=".UNION">/
  command and the separate section named <ref id="structs" name="&quot;Structs
  and unions&quot;">.


<sect1><tt>.ENUM</tt><label id=".ENUM"><p>

  Start an enumeration. This directive is very similar to the C <tt/enum/
  keyword. If a name is given, a new scope is created for the enumeration,
  otherwise the enumeration members are placed in the enclosing scope.

  In the enumeration body, symbols are declared. The first symbol has a value
  of zero, and each following symbol will get the value of the preceding, plus
  one. That behaviour may be overridden by an explicit assignment. Two symbols
  may have the same value.

  Example:

  <tscreen><verb>
        .enum   errorcodes
                no_error
                file_error
                parse_error
        .endenum
  </verb></tscreen>

  The above example will create a new scope named <tt/errorcodes/ with three
  symbols in it that get the values 0, 1, and 2 respectively. Another way
  to write that would have been:

  <tscreen><verb>
        .scope  errorcodes
                no_error        = 0
                file_error      = 1
                parse_error     = 2
        .endscope
  </verb></tscreen>

  Please note that explicit scoping must be used to access the identifiers:

  <tscreen><verb>
        .word   errorcodes::no_error
  </verb></tscreen>

  A more complex example:

  <tscreen><verb>
        .enum
                EUNKNOWN        = -1
                EOK
                EFILE
                EBUSY
                EAGAIN
                EWOULDBLOCK     = EAGAIN
        .endenum
  </verb></tscreen>

  In that example, the enumeration does not have a name, which means that the
  members will be visible in the enclosing scope, and can be used in that scope
  without explicit scoping. The first member (<tt/EUNKNOWN/) has the value -1.
  The values for the following members are incremented by one; so, <tt/EOK/
  would be zero, and so on. <tt/EWOULDBLOCK/ is an alias for <tt/EAGAIN/; so,
  it has an override for the value, using an already defined symbol.


<sect1><tt>.ERROR</tt><label id=".ERROR"><p>

  Force an assembly error. The assembler will output an error message
  preceded by "User error". Assembly is continued but no object file will
  generated.

  This command may be used to check for initial conditions that must be
  set before assembling a source file.

  Example:

  <tscreen><verb>
        .if     foo = 1
        ...
        .elseif bar = 1
        ...
        .else
        .error  "Must define foo or bar!"
        .endif
  </verb></tscreen>

  See also: <tt><ref id=".FATAL" name=".FATAL"></tt>,
            <tt><ref id=".OUT" name=".OUT"></tt>,
            <tt><ref id=".WARNING" name=".WARNING"></tt>


<sect1><tt>.EXITMAC, .EXITMACRO</tt><label id=".EXITMACRO"><p>

  Abort a macro expansion immediately. This command is often useful in
  recursive macros.

  See: <tt><ref id=".DELMACRO" name=".DELMACRO"></tt>,
       <tt><ref id=".ENDMACRO" name=".ENDMACRO"></tt>,
       <tt><ref id=".MACRO" name=".MACRO"></tt>

  See also section <ref id="macros" name="Macros">.


<sect1><tt>.EXPORT</tt><label id=".EXPORT"><p>

  Make symbols accessible from other modules. Must be followed by a comma
  separated list of symbols to export, with each one optionally followed by an
  address specification and (also optional) an assignment. Using an additional
  assignment in the export statement allows to define and export a symbol in
  one statement. The default is to export the symbol with the address size it
  actually has. The assembler will issue a warning, if the symbol is exported
  with an address size smaller than the actual address size.

  Examples:

  <tscreen><verb>
        .export foo
        .export bar: far
        .export foobar: far = foo * bar
        .export baz := foobar, zap: far = baz - bar
  </verb></tscreen>

  As with constant definitions, using <tt/:=/ instead of <tt/=/ marks the
  symbols as a label.

  See: <tt><ref id=".EXPORTZP" name=".EXPORTZP"></tt>


<sect1><tt>.EXPORTZP</tt><label id=".EXPORTZP"><p>

  Make symbols accessible from other modules. Must be followed by a comma
  separated list of symbols to export. The exported symbols are explicitly
  marked as zero page symbols. An assignment may be included in the
  <tt/.EXPORTZP/ statement. This allows to define and export a symbol in one
  statement.

  Examples:

  <tscreen><verb>
        .exportzp  foo, bar
        .exportzp  baz := &dollar;02
  </verb></tscreen>

  See: <tt><ref id=".EXPORT" name=".EXPORT"></tt>


<sect1><tt>.FARADDR</tt><label id=".FARADDR"><p>

  Define far (24 bit) address data. The command must be followed by a
  sequence of (not necessarily constant) expressions.

  Example:

  <tscreen><verb>
        .faraddr        DrawCircle, DrawRectangle, DrawHexagon
  </verb></tscreen>

  See: <tt><ref id=".ADDR" name=".ADDR"></tt>


<sect1><tt>.FATAL</tt><label id=".FATAL"><p>

  Force an assembly error and terminate assembly. The assembler will output an
  error message preceded by "User error" and will terminate assembly
  immediately.

  This command may be used to check for initial conditions that must be
  set before assembling a source file.

  Example:

  <tscreen><verb>
        .if     foo = 1
        ...
        .elseif bar = 1
        ...
        .else
        .fatal  "Must define foo or bar!"
        .endif
  </verb></tscreen>

  See also: <tt><ref id=".ERROR" name=".ERROR"></tt>,
            <tt><ref id=".OUT" name=".OUT"></tt>,
            <tt><ref id=".WARNING" name=".WARNING"></tt>


<sect1><tt>.FEATURE</tt><label id=".FEATURE"><p>

  This directive may be used to enable one or more compatibility features
  of the assembler. While the use of <tt/.FEATURE/ should be avoided when
  possible, it may be useful when porting sources written for other
  assemblers. After the feature name an optional '+' or '-' may specify whether
  to enable or disable the feature (enable if omitted). Multiple features may be
  enabled, separated by commas. Examples:

  <tscreen><verb>
        ; enable c_comments
        .feature   c_comments
        .feature   c_comments +
        ; enable force_range, disable underline_in_numbers, enable labels_without_colons
        .feature   force_range, underline_in_numbers -, labels_without_colons +
        .feature   force_range +, underline_in_numbers off, labels_without_colons on
  </verb></tscreen>

  The following features are available:

  <descrip>

  <tag><tt>at_in_identifiers</tt><label id="at_in_identifiers"></tag>

    Accept the at character ('@') as a valid character in identifiers. The
    at character is not allowed to start an identifier, even with this
    feature enabled.

  <tag><tt>bracket_as_indirect</tt><label id="bracket_as_indirect"></tag>

    Use <tt>[]</tt> instead of <tt>()</tt> for the indirect addressing modes.
    Example:

    <tscreen><verb>
        lda     [$82]
        lda     [$82,x]
        lda     [$82],y
        jmp     [$fffe]
        jmp     [table,x]
    </verb></tscreen>
    <em/Note:/ This should not be used in 65186 mode because it conflicts with
    the 65816 instruction syntax for far addressing. See the section covering
    <tt/<ref id="address-sizes" name="address sizes">/ for more information.

  <tag><tt>c_comments</tt><label id="c_comments"></tag>

    Allow C like comments using <tt>/*</tt> and <tt>*/</tt> as left and right
    comment terminators. Note that C comments may not be nested. There's also a
    pitfall when using C like comments: All statements must be terminated by
    "end-of-line". Using C like comments, it is possible to hide the newline,
    which results in error messages. See the following non working example:

    <tscreen><verb>
        lda     #$00  /* This comment hides the newline
*/      sta     $82
    </verb></tscreen>

  <tag><tt>dollar_in_identifiers</tt><label id="dollar_in_identifiers"></tag>

    Accept the dollar sign ('&dollar;') as a valid character in identifiers. The
    dollar character is not allowed to start an identifier, even with this
    feature enabled.

  <tag><tt>dollar_is_pc</tt><label id="dollar_is_pc"></tag>

    The dollar sign may be used as an alias for the star ('*'), which
    gives the value of the current PC in expressions.
    Note: Assignment to the pseudo variable is not allowed.

  <tag><tt>force_range</tt><label id="force_range"></tag>

    Force expressions into their valid range for immediate addressing and
    storage operators like <tt><ref id=".BYTE" name=".BYTE"></tt> and
    <tt><ref id=".WORD" name=".WORD"></tt>. Be very careful with this one,
    since it will completely disable error checks.

  <tag><tt>labels_without_colons</tt><label id="labels_without_colons"></tag>

    Allow labels without a trailing colon. These labels are only accepted,
    if they start at the beginning of a line (no leading white space).

  <tag><tt>leading_dot_in_identifiers</tt><label id="leading_dot_in_identifiers"></tag>

    Accept the dot ('.') as the first character of an identifier. This may be
    used for example to create macro names that start with a dot emulating
    control directives of other assemblers. Note however, that none of the
    reserved keywords built into the assembler, that starts with a dot, may be
    overridden. When using this feature, you may also get into trouble if
    later versions of the assembler define new keywords starting with a dot.

  <tag><tt>line_continuations</tt><label id="line_continuations"></tag>

    Switch on or off line continuations using the backslash character
    before a newline. The option is off by default.
    Note: Line continuations do not work in a comment. A backslash at the
    end of a comment is treated as part of the comment and does not trigger
    line continuation.

  Example:

    <tscreen><verb>
          .feature line_continuations +   ; Allow line continuations

          lda     \
                  #$20                    ; This is legal now
    </verb></tscreen>

    For backward compatibility reasons, the <tt>.LINECONT +</tt> control command
    is also supported and enables the same feature.

  <tag><tt>long_jsr_jmp_rts</tt><label id="long_jsr_jmp_rts"></tag>

    Affects 65816 mode only.

    Allows <tt>jsr</tt> and <tt>jmp</tt> to produce long jumps if the target
    address has been previously declared in a <tt>far</tt> segment,
    or imported as <tt>far</tt>.
    Otherwise <tt>jsl</tt> and <tt>jml</tt> must be used instead.

    Also allows <tt><ref id=".SMART" name=".SMART"></tt> to convert <tt>rts</tt>
    to a long return <tt>rtl</tt> when the enclosing scope or memory model
    indicates returning from a <tt>far</tt> procedure.

    This permits compatibility with the old behavior of this assembler, or other
    assemblers which similarly allowed <tt>jsr</tt> and <tt>jmp</tt> to be used
    this way.

  <tag><tt>loose_char_term</tt><label id="loose_char_term"></tag>

    Accept single quotes as well as double quotes as terminators for char
    constants.

  <tag><tt>loose_string_term</tt><label id="loose_string_term"></tag>

    Accept single quotes as well as double quotes as terminators for string
    constants.

  <tag><tt>missing_char_term</tt><label id="missing_char_term"></tag>

    Accept single quoted character constants where the terminating quote is
    missing.
    <tscreen><verb>
        lda     #'a
    </verb></tscreen>
    <em/Note:/ This does not work in conjunction with <tt/.FEATURE
    loose_string_term/, since in this case the input would be ambiguous.

  <tag><tt>org_per_seg</tt><label id="org_per_seg"></tag>

    This feature makes relocatable/absolute mode local to the current segment.
    Using <tt><ref id=".ORG" name=".ORG"></tt> when <tt/org_per_seg/ is in
    effect will only enable absolute mode for the current segment. Dito for
    <tt><ref id=".RELOC" name=".RELOC"></tt>.

  <tag><tt>pc_assignment</tt><label id="pc_assignment"></tag>

    Allow assignments to the PC symbol ('*' or '&dollar;' if <tt/dollar_is_pc/
    is enabled). Such an assignment is handled identical to the <tt><ref
    id=".ORG" name=".ORG"></tt> command (which is usually not needed, so just
    removing the lines with the assignments may also be an option when porting
    code written for older assemblers).

  <tag><tt>string_escapes</tt><label id="string_escapes"></tag>

    Allow C-style backslash escapes within string constants to embed
    special characters. The following escapes are accepted:
    <itemize>
    <item><tt>\\</tt> backslash (<tt>$5C</tt>)
    <item><tt>\'</tt> single quote (<tt>$27</tt>)
    <item><tt>\&quot;</tt> double quote (<tt>$22</tt>)
    <item><tt>\t</tt> tab (<tt>$09</tt>)
    <item><tt>\r</tt> carriage return (<tt>$0D</tt>)
    <item><tt>\n</tt> newline (<tt>$0A</tt>)
    <item><tt>\xNN</tt>  (<tt>$NN</tt>)
    </itemize>

    Note that string escapes are converted to platform-specific characters in
    the same way that other characters are converted.

  <tag><tt>ubiquitous_idents</tt><label id="ubiquitous_idents"></tag>

    Allow the use of instructions names as names for macros and symbols. This
    makes it possible to "overload" instructions by defining a macro with the
    same name. This does also make it possible to introduce hard to find errors
    in your code, so be careful!

  <tag><tt>underline_in_numbers</tt><label id="underline_in_numbers"></tag>

    Allow underlines within numeric constants. These may be used for grouping
    the digits of numbers for easier reading.
    Example:
    <tscreen><verb>
        .feature        underline_in_numbers
        .word           %1100001110100101
        .word           %1100_0011_1010_0101    ; Identical but easier to read
    </verb></tscreen>

  </descrip>

  It is also possible to specify features on the command line using the
  <tt><ref id="option--feature" name="--feature"></tt> command line option.
  This is useful when translating sources written for older assemblers, when
  you don't want to change the source code.

  As an example, to translate sources written for Andre Fachats xa65
  assembler, the features

  <verb>
        labels_without_colons, pc_assignment, loose_char_term
  </verb>

  may be helpful. They do not make ca65 completely compatible, so you may not
  be able to translate the sources without changes, even when enabling these
  features. However, I have found several sources that translate without
  problems when enabling these features on the command line.


<sect1><tt>.FILEOPT, .FOPT</tt><label id=".FOPT"><p>

  Insert an option string into the object file. There are two forms of
  this command, one specifies the option by a keyword, the second
  specifies it as a number. Since usage of the second one needs knowledge
  of the internal encoding, its use is not recommended and I will only
  describe the first form here.

  The command is followed by one of the keywords

  <tscreen><verb>
        author
        comment
        compiler
  </verb></tscreen>

  a comma and a string. The option is written into the object file
  together with the string value. This is currently unidirectional and
  there is no way to actually use these options once they are in the
  object file.

  Examples:

  <tscreen><verb>
        .fileopt        comment, "Code stolen from my brother"
        .fileopt        compiler, "BASIC 2.0"
        .fopt           author, "J. R. User"
  </verb></tscreen>


<sect1><tt>.FORCEIMPORT</tt><label id=".FORCEIMPORT"><p>

  Import an absolute symbol from another module. The command is followed by a
  comma separated list of symbols to import. The command is similar to <tt>
  <ref id=".IMPORT" name=".IMPORT"></tt>, but the import reference is always
  written to the generated object file, even if the symbol is never referenced
  (<tt><ref id=".IMPORT" name=".IMPORT"></tt> will not generate import
  references for unused symbols).

  Example:

  <tscreen><verb>
        .forceimport    needthisone, needthistoo
  </verb></tscreen>

  See: <tt><ref id=".IMPORT" name=".IMPORT"></tt>


<sect1><tt>.GLOBAL</tt><label id=".GLOBAL"><p>

  Declare symbols as global. Must be followed by a comma separated list of
  symbols to declare. Symbols from the list, that are defined somewhere in the
  source, are exported, all others are imported. Additional <tt><ref
  id=".IMPORT" name=".IMPORT"></tt> or <tt><ref id=".EXPORT"
  name=".EXPORT"></tt> commands for the same symbol are allowed.

  Example:

  <tscreen><verb>
        .global foo, bar
  </verb></tscreen>


<sect1><tt>.GLOBALZP</tt><label id=".GLOBALZP"><p>

  Declare symbols as global. Must be followed by a comma separated list of
  symbols to declare. Symbols from the list, that are defined somewhere in the
  source, are exported, all others are imported. Additional <tt><ref
  id=".IMPORTZP" name=".IMPORTZP"></tt> or <tt><ref id=".EXPORTZP"
  name=".EXPORTZP"></tt> commands for the same symbol are allowed. The symbols
  in the list are explicitly marked as zero page symbols.

  Example:

  <tscreen><verb>
        .globalzp foo, bar
  </verb></tscreen>

<sect1><tt>.HIBYTES</tt><label id=".HIBYTES"><p>

  Define byte sized data by extracting only the high byte (that is, bits 8-15) from
  each expression.  This is equivalent to <tt><ref id=".BYTE" name=".BYTE"></tt> with
  the operator '>' prepended to each expression in its list.

  Example:

  <tscreen><verb>
        .lobytes         $1234, $2345, $3456, $4567
        .hibytes         $fedc, $edcb, $dcba, $cba9
  </verb></tscreen>

  which is equivalent to

  <tscreen><verb>
        .byte            $34, $45, $56, $67
        .byte            $fe, $ed, $dc, $cb
  </verb></tscreen>

  Example:

  <tscreen><verb>
        .define MyTable TableItem0, TableItem1, TableItem2, TableItem3

        TableLookupLo:   .lobytes MyTable
        TableLookupHi:   .hibytes MyTable
  </verb></tscreen>

  which is equivalent to

  <tscreen><verb>
        TableLookupLo:   .byte &lt;TableItem0, &lt;TableItem1, &lt;TableItem2, &lt;TableItem3
        TableLookupHi:   .byte &gt;TableItem0, &gt;TableItem1, &gt;TableItem2, &gt;TableItem3
  </verb></tscreen>

  See also: <tt><ref id=".BYTE" name=".BYTE"></tt>,
            <tt><ref id=".LOBYTES" name=".LOBYTES"></tt>,
            <tt><ref id=".BANKBYTES" name=".BANKBYTES"></tt>


<sect1><tt>.I16</tt><label id=".I16"><p>

  Valid only in 65816 mode. Assume the index registers are 16 bit.

  Note: This command will not emit any code, it will tell the assembler to
  create 16 bit operands for immediate operands.

  See also the <tt><ref id=".I8" name=".I8"></tt> and <tt><ref id=".SMART"
  name=".SMART"></tt> commands.


<sect1><tt>.I8</tt><label id=".I8"><p>

  Valid only in 65816 mode. Assume the index registers are 8 bit.

  Note: This command will not emit any code, it will tell the assembler to
  create 8 bit operands for immediate operands.

  See also the <tt><ref id=".I16" name=".I16"></tt> and <tt><ref id=".SMART"
  name=".SMART"></tt> commands.


<sect1><tt>.IF</tt><label id=".IF"><p>

  Conditional assembly: Evaluate an expression and switch assembler output
  on or off depending on the expression. The expression must be a constant
  expression, that is, all operands must be defined.

  A expression value of zero evaluates to FALSE, any other value evaluates
  to TRUE.


<sect1><tt>.IFBLANK</tt><label id=".IFBLANK"><p>

  Conditional assembly: Check if there are any remaining tokens in this line,
  and evaluate to FALSE if this is the case, and to TRUE otherwise. If the
  condition is not true, further lines are not assembled until an <tt><ref
  id=".ELSE" name=".ELSE"></tt>, <tt><ref id=".ELSEIF" name=".ELSEIF"></tt> or
  <tt><ref id=".ENDIF" name=".ENDIF"></tt> directive.

  This command is often used to check if a macro parameter was given. Since an
  empty macro parameter will evaluate to nothing, the condition will evaluate
  to TRUE if an empty parameter was given.

  Example:

  <tscreen><verb>
        .macro     arg1, arg2
        .ifblank   arg2
                   lda     #arg1
        .else
                   lda     #arg2
        .endif
        .endmacro
  </verb></tscreen>

  See also: <tt><ref id=".BLANK" name=".BLANK"></tt>


<sect1><tt>.IFCONST</tt><label id=".IFCONST"><p>

  Conditional assembly: Evaluate an expression and switch assembler output
  on or off depending on the constness of the expression.

  A const expression evaluates to to TRUE, a non const expression (one
  containing an imported or currently undefined symbol) evaluates to
  FALSE.

  See also: <tt><ref id=".CONST" name=".CONST"></tt>


<sect1><tt>.IFDEF</tt><label id=".IFDEF"><p>

  Conditional assembly: Check if a symbol is defined. Must be followed by
  a symbol name. The condition is true if the given symbol is already
  defined, and false otherwise.

  See also: <tt><ref id=".DEFINED" name=".DEFINED"></tt>


<sect1><tt>.IFNBLANK</tt><label id=".IFNBLANK"><p>

  Conditional assembly: Check if there are any remaining tokens in this line,
  and evaluate to TRUE if this is the case, and to FALSE otherwise. If the
  condition is not true, further lines are not assembled until an <tt><ref
  id=".ELSE" name=".ELSE"></tt>, <tt><ref id=".ELSEIF" name=".ELSEIF"></tt> or
  <tt><ref id=".ENDIF" name=".ENDIF"></tt> directive.

  This command is often used to check if a macro parameter was given.
  Since an empty macro parameter will evaluate to nothing, the condition
  will evaluate to FALSE if an empty parameter was given.

  Example:

  <tscreen><verb>
        .macro     arg1, arg2
                   lda     #arg1
        .ifnblank  arg2
                   lda     #arg2
        .endif
        .endmacro
  </verb></tscreen>

  See also: <tt><ref id=".BLANK" name=".BLANK"></tt>


<sect1><tt>.IFNDEF</tt><label id=".IFNDEF"><p>

  Conditional assembly: Check if a symbol is defined. Must be followed by
  a symbol name. The condition is true if the given symbol is not
  defined, and false otherwise.

  See also: <tt><ref id=".DEFINED" name=".DEFINED"></tt>


<sect1><tt>.IFNREF</tt><label id=".IFNREF"><p>

  Conditional assembly: Check if a symbol is referenced. Must be followed
  by a symbol name. The condition is true if the given symbol was
  not referenced before, and false otherwise.

  See also: <tt><ref id=".REFERENCED" name=".REFERENCED"></tt>


<sect1><tt>.IFP02</tt><label id=".IFP02"><p>

  Conditional assembly: Check if the assembler is currently in 6502 mode
  (see <tt><ref id=".P02" name=".P02"></tt> command).


<sect1><tt>.IFP02X</tt><label id=".IFP02X"><p>

  Conditional assembly: Check if the assembler is currently in 6502X mode
  (see <tt><ref id=".P02X" name=".P02X"></tt> command).


<sect1><tt>.IFP4510</tt><label id=".IFP4510"><p>

  Conditional assembly: Check if the assembler is currently in 4510 mode
  (see <tt><ref id=".P4510" name=".P4510"></tt> command).


<sect1><tt>.IFP45GS02</tt><label id=".IFP45GS02"><p>

  Conditional assembly: Check if the assembler is currently in 45GS02 mode
  (see <tt><ref id=".P45GS02" name=".P45GS02"></tt> command).


<sect1><tt>.IFP6280</tt><label id=".IFP816"><p>

  Conditional assembly: Check if the assembler is currently in HuC6280 mode
  (see <tt><ref id=".P6280" name=".P6280"></tt> command).


<sect1><tt>.IFP816</tt><label id=".IFP816"><p>

  Conditional assembly: Check if the assembler is currently in 65816 mode
  (see <tt><ref id=".P816" name=".P816"></tt> command).


<sect1><tt>.IFPC02</tt><label id=".IFPC02"><p>

  Conditional assembly: Check if the assembler is currently in 65C02 mode
  (see <tt><ref id=".PC02" name=".PC02"></tt> command).


<sect1><tt>.IFPCE02</tt><label id=".IFPCE02"><p>

  Conditional assembly: Check if the assembler is currently in 65CE02 mode
  (see <tt><ref id=".PCE02" name=".PCE02"></tt> command).


<sect1><tt>.IFPDTV</tt><label id=".IFPDTV"><p>

  Conditional assembly: Check if the assembler is currently in 6502DTV mode
  (see <tt><ref id=".PDTV" name=".PDTV"></tt> command).


<sect1><tt>.IFPM740</tt><label id=".IFPM740"><p>

  Conditional assembly: Check if the assembler is currently in M740 mode
  (see <tt><ref id=".PM740" name=".PM740"></tt> command).


<sect1><tt>.IFPSC02</tt><label id=".IFPSC02"><p>

  Conditional assembly: Check if the assembler is currently in 65SC02 mode
  (see <tt><ref id=".PSC02" name=".PSC02"></tt> command).


<sect1><tt>.IFPSWEET16</tt><label id=".IFPSWEET16"><p>

  Conditional assembly: Check if the assembler is currently in Sweet16 mode
  (see <tt><ref id=".PSWEET16" name=".PSWEET16"></tt> command).


<sect1><tt>.IFREF</tt><label id=".IFREF"><p>

  Conditional assembly: Check if a symbol is referenced. Must be followed
  by a symbol name. The condition is true if the given symbol was
  referenced before, and false otherwise.

  This command may be used to build subroutine libraries in include files
  (you may use separate object modules for this purpose too).

  Example:

  <tscreen><verb>
        .ifref  ToHex                   ; If someone used this subroutine
        ToHex:  tay                     ; Define subroutine
                lda     HexTab,y
                rts
        .endif
  </verb></tscreen>

  See also: <tt><ref id=".REFERENCED" name=".REFERENCED"></tt>, and
  <tt><ref id=".REFERTO" name=".REFERTO"></tt>


<sect1><tt>.IFPWC02</tt><label id=".IFPWC02"><p>

  Conditional assembly: Check if the assembler is currently in 65WC02 mode
  (see <tt><ref id=".PWC02" name=".PWC02"></tt> command).


<sect1><tt>.IMPORT</tt><label id=".IMPORT"><p>

  Import a symbol from another module. The command is followed by a comma
  separated list of symbols to import, with each one optionally followed by
  an address specification.

  Example:

  <tscreen><verb>
        .import foo
        .import bar: zeropage
  </verb></tscreen>

  See: <tt><ref id=".IMPORTZP" name=".IMPORTZP"></tt>


<sect1><tt>.IMPORTZP</tt><label id=".IMPORTZP"><p>

  Import a symbol from another module. The command is followed by a comma
  separated list of symbols to import. The symbols are explicitly imported
  as zero page symbols (that is, symbols with values in byte range).

  Example:

  <tscreen><verb>
        .importzp       foo, bar
  </verb></tscreen>

  See: <tt><ref id=".IMPORT" name=".IMPORT"></tt>


<sect1><tt>.INCBIN</tt><label id=".INCBIN"><p>

  Include a file as binary data. The command expects a string argument
  that is the name of a file to include literally in the current segment.
  In addition to that, a start offset and a size value may be specified,
  separated by commas. If no size is specified, all of the file from the
  start offset to end-of-file is used. If no start position is specified
  either, zero is assumed (which means that the whole file is inserted).

  Example:

  <tscreen><verb>
        ; Include whole file
        .incbin         "sprites.dat"

        ; Include file starting at offset 256
        .incbin         "music.dat", $100

        ; Read 100 bytes starting at offset 200
        .incbin         "graphics.dat", 200, 100
  </verb></tscreen>


<sect1><tt>.INCLUDE</tt><label id=".INCLUDE"><p>

  Include another file. Include files may be nested up to a depth of 16.

  Example:

  <tscreen><verb>
        .include        "subs.inc"
  </verb></tscreen>


<sect1><tt>.INTERRUPTOR</tt><label id=".INTERRUPTOR"><p>

  Export a symbol and mark it as an interruptor. This may be used together
  with the linker to build a table of interruptor subroutines that are called
  in an interrupt.

  Note: The linker has a feature to build a table of marked routines, but it
  is your code that must call these routines, so just declaring a symbol as
  interruptor does nothing by itself.

  An interruptor is always exported as an absolute (16 bit) symbol. You don't
  need to use an additional <tt/.export/ statement, this is implied by
  <tt/.interruptor/. It may have an optional priority that is separated by a
  comma. Higher numeric values mean a higher priority. If no priority is
  given, the default priority of 7 is used. Be careful when assigning
  priorities to your own module constructors so they won't interfere with the
  ones in the cc65 library.

  Example:

  <tscreen><verb>
        .interruptor    IrqHandler
        .interruptor    Handler, 16
  </verb></tscreen>

  See the <tt><ref id=".CONDES" name=".CONDES"></tt> command and the separate
  section <ref id="condes" name="Module constructors/destructors"> explaining
  the feature in more detail.


<sect1><tt>.LIST</tt><label id=".LIST"><p>

  Enable output to the listing. The command can be followed by a boolean
  switch ("on", "off", "+" or "-") and will enable or disable listing
  output.
  The option has no effect if the listing is not enabled by the command line
  switch -l. If -l is used, an internal counter is set to 1. Lines are output
  to the listing file, if the counter is greater than zero, and suppressed if
  the counter is zero. Each use of <tt/.LIST/ will increment or decrement the
  counter.

  Example:

  <tscreen><verb>
        .list   on              ; Enable listing output
  </verb></tscreen>


<sect1><tt>.LISTBYTES</tt><label id=".LISTBYTES"><p>

  Set, how many bytes are shown in the listing for one source line. The
  default is 12, so the listing will show only the first 12 bytes for any
  source line that generates more than 12 bytes of code or data.
  The directive needs an argument, which is either "unlimited", or an
  integer constant in the range 4..255.

  Examples:

  <tscreen><verb>
        .listbytes      unlimited       ; List all bytes
        .listbytes      12              ; List the first 12 bytes
        .incbin         "data.bin"      ; Include large binary file
  </verb></tscreen>


<sect1><tt>.LITERAL</tt><label id=".LITERAL"><p>

  Define byte sized data. Must be followed by a sequence of (byte ranged)
  expressions or strings. Strings will disregard the current character
  mapping definition and will be interpreted literally.

  Example:

  <tscreen><verb>
        .literal    "Hello "
        .literal    "world", $0D, $00
  </verb></tscreen>

See: <tt><ref id=".ASCIIZ" name=".ASCIIZ"></tt>,<tt><ref id=".BYTE" name=".BYTE"></tt>


<sect1><tt>.LOBYTES</tt><label id=".LOBYTES"><p>

  Define byte sized data by extracting only the low byte (that is, bits 0-7) from
  each expression.  This is equivalent to <tt><ref id=".BYTE" name=".BYTE"></tt> with
  the operator '<' prepended to each expression in its list.

  Example:

  <tscreen><verb>
        .lobytes         $1234, $2345, $3456, $4567
        .hibytes         $fedc, $edcb, $dcba, $cba9
  </verb></tscreen>

  which is equivalent to

  <tscreen><verb>
        .byte            $34, $45, $56, $67
        .byte            $fe, $ed, $dc, $cb
  </verb></tscreen>

  Example:

  <tscreen><verb>
        .define MyTable TableItem0, TableItem1, TableItem2, TableItem3

        TableLookupLo:   .lobytes MyTable
        TableLookupHi:   .hibytes MyTable
  </verb></tscreen>

  which is equivalent to

  <tscreen><verb>
        TableLookupLo:   .byte &lt;TableItem0, &lt;TableItem1, &lt;TableItem2, &lt;TableItem3
        TableLookupHi:   .byte &gt;TableItem0, &gt;TableItem1, &gt;TableItem2, &gt;TableItem3
  </verb></tscreen>

  See also: <tt><ref id=".BYTE" name=".BYTE"></tt>,
            <tt><ref id=".HIBYTES" name=".HIBYTES"></tt>,
            <tt><ref id=".BANKBYTES" name=".BANKBYTES"></tt>


<sect1><tt>.LOCAL</tt><label id=".LOCAL"><p>

  This command may only be used inside a macro definition. It declares a
  list of identifiers as local to the macro expansion.

  A problem when using macros are labels: Since they don't change their name,
  you get a "duplicate symbol" error if the macro is expanded the second time.
  Labels declared with <tt><ref id=".LOCAL" name=".LOCAL"></tt> have their
  name mapped to an internal unique name (<tt/___ABCD__/) with each macro
  invocation.

  Some other assemblers start a new lexical block inside a macro expansion.
  This has some drawbacks however, since that will not allow <em/any/ symbol
  to be visible outside a macro, a feature that is sometimes useful. The
  <tt><ref id=".LOCAL" name=".LOCAL"></tt> command is in my eyes a better way
  to address the problem.

  You get an error when using <tt><ref id=".LOCAL" name=".LOCAL"></tt> outside
  a macro.


<sect1><tt>.LOCALCHAR</tt><label id=".LOCALCHAR"><p>

  Defines the character that start "cheap" local labels. You may use one
  of '@' and '?' as start character. The default is '@'.

  Cheap local labels are labels that are visible only between two non
  cheap labels. This way you can reuse identifiers like "<tt/loop/" without
  using explicit lexical nesting.

  Example:

  <tscreen><verb>
        .localchar      '?'

        Clear:  lda     #$00            ; Global label
        ?Loop:  sta     Mem,y           ; Local label
                dey
                bne     ?Loop           ; Ok
                rts
        Sub:    ...                     ; New global label
                bne     ?Loop           ; ERROR: Unknown identifier!
  </verb></tscreen>


<sect1><tt>.MACPACK</tt><label id=".MACPACK"><p>

  Insert a predefined macro package. The command is followed by an
  identifier specifying the macro package to insert. Available macro
  packages are:

  <tscreen><verb>
        atari           Defines the scrcode macro.
        cbm             Defines the scrcode macro.
        cpu             Defines constants for the .CPU variable.
        generic         Defines generic macros like add, sub, and blt.
        longbranch      Defines conditional long-jump macros.
  </verb></tscreen>

  Including a macro package twice, or including a macro package that
  redefines already existing macros will lead to an error.

  Example:

  <tscreen><verb>
        .macpack        longbranch      ; Include macro package

                cmp     #$20            ; Set condition codes
                jne     Label           ; Jump long on condition
  </verb></tscreen>

  Macro packages are explained in more detail in section <ref
  id="macropackages" name="Macro packages">.


<sect1><tt>.MAC, .MACRO</tt><label id=".MACRO"><p>

  Start a classic macro definition. The command is followed by an identifier
  (the macro name) and optionally by a comma separated list of identifiers
  that are macro parameters. A macro definition is terminated by <tt><ref
  id=".ENDMACRO" name=".ENDMACRO"></tt>.

  Example:

  <tscreen><verb>
        .macro  ldax    arg             ; Define macro ldax
                lda     arg
                ldx     arg+1
  </verb></tscreen>

  See: <tt><ref id=".DELMACRO" name=".DELMACRO"></tt>,
       <tt><ref id=".ENDMACRO" name=".ENDMACRO"></tt>,
       <tt><ref id=".EXITMACRO" name=".EXITMACRO"></tt>

  See also section <ref id="macros" name="Macros">.


<sect1><tt>.ORG</tt><label id=".ORG"><p>

  Start a section of absolute code. The command is followed by a constant
  expression that gives the new PC counter location for which the code is
  assembled. Use <tt><ref id=".RELOC" name=".RELOC"></tt> to switch back to
  relocatable code.

  By default, absolute/relocatable mode is global (valid even when switching
  segments). Using <tt>.FEATURE <ref id="org_per_seg" name="org_per_seg"></tt>
  it can be made segment local.

  Please note that you <em/do not need/ <tt/.ORG/ in most cases. Placing
  code at a specific address is the job of the linker, not the assembler, so
  there is usually no reason to assemble code to a specific address.

  Example:

  <tscreen><verb>
        .org    $7FF            ; Emit code starting at $7FF
  </verb></tscreen>


<sect1><tt>.OUT</tt><label id=".OUT"><p>

  Output a string to the console without producing an error. This command
  is similar to <tt/.ERROR/, however, it does not force an assembler error
  that prevents the creation of an object file.

  Example:

  <tscreen><verb>
        .out    "This code was written by the codebuster(tm)"
  </verb></tscreen>

  See also: <tt><ref id=".ERROR" name=".ERROR"></tt>,
            <tt><ref id=".FATAL" name=".FATAL"></tt>,
            <tt><ref id=".WARNING" name=".WARNING"></tt>


<sect1><tt>.P02</tt><label id=".P02"><p>

  Enable the 6502 instruction set, disable 65SC02, 65C02 and 65816
  instructions. This is the default if not overridden by the
  <tt><ref id="option--cpu" name="--cpu"></tt> command line option.

  See: <tt><ref id=".PC02" name=".PC02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".P816" name=".P816"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.P02X</tt><label id=".P02X"><p>

  Enable the 6502X instruction set, disable 65SC02, 65C02 and 65816
  instructions.

  See: <tt><ref id=".PC02" name=".PC02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".P816" name=".P816"></tt> and
  <tt><ref id=".P4510" name=".P4510"></tt>


<sect1><tt>.P4510</tt><label id=".P4510"><p>

  Enable the 4510 instruction set. This is a superset of the 65C02 and
  6502 instruction sets.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".PC02" name=".PC02"></tt>,
  <tt><ref id=".P816" name=".P816"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.P45GS02</tt><label id=".P45GS02"><p>

  Enable the 45GS02 instruction set. This is a superset of the 4510, 65C02, and
  6502 instruction sets.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".PC02" name=".PC02"></tt>,
  <tt><ref id=".P816" name=".P816"></tt>, and
  <tt><ref id=".P4510" name=".P4510"></tt>


<sect1><tt>.P6280</tt><label id=".P6280"><p>

  Enable the HuC6280 instruction set. This is a superset of the 65C02 and
  6502 instruction sets.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".PC02" name=".PC02"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.P816</tt><label id=".P816"><p>

  Enable the 65816 instruction set. This is a superset of the 65SC02 and
  6502 instruction sets.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".PC02" name=".PC02"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.PAGELEN, .PAGELENGTH</tt><label id=".PAGELENGTH"><p>

  Set the page length for the listing. Must be followed by an integer
  constant. The value may be "unlimited", or in the range 32 to 127. The
  statement has no effect if no listing is generated. The default value is -1
  (unlimited) but may be overridden by the <tt/--pagelength/ command line
  option. Beware: Since ca65 is a one pass assembler, the listing is generated
  after assembly is complete, you cannot use multiple line lengths with one
  source. Instead, the value set with the last <tt/.PAGELENGTH/ is used.

  Examples:

  <tscreen><verb>
        .pagelength     66              ; Use 66 lines per listing page

        .pagelength     unlimited       ; Unlimited page length
  </verb></tscreen>


<sect1><tt>.PC02</tt><label id=".PC02"><p>

  Enable the 65C02 instructions set. This instruction set includes all
  6502 and 65SC02 instructions.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".P816" name=".P816"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>

<sect1><tt>.PCE02</tt><label id=".PCE02"><p>

  Enable the 65CE02 instructions set. This instruction set includes all
  6502 and extended 65CE02 instructions.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".P816" name=".P816"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.PDTV</tt><label id=".PDTV"><p>

  Enable the 6502DTV instruction set. This is a superset of the 6502
  instruction set.

  See: <tt><ref id=".P02" name=".P02"></tt>


<sect1><tt>.PM740</tt><label id=".PM740"><p>

  Enable the M740 instruction set. This is a superset of the 6502
  instruction set.

  See: <tt><ref id=".P02" name=".P02"></tt>


<sect1><tt>.POPCHARMAP</tt><label id=".POPCHARMAP"><p>

  Pop the last character mapping from the stack, and activate it.

  This command will switch back to the character mapping that was last pushed onto the
  character mapping stack using the <tt><ref id=".PUSHCHARMAP" name=".PUSHCHARMAP"></tt>
  command, and remove this entry from the stack.

  The assembler will print an error message if the mappting stack is empty when
  this command is issued.

  See: <tt><ref id=".CHARMAP" name=".CHARMAP"></tt>, <tt><ref id=".PUSHCHARMAP"
  name=".PUSHCHARMAP"></tt>


<sect1><tt>.POPCPU</tt><label id=".POPCPU"><p>

  Pop the last CPU setting from the stack, and activate it.

  This command will switch back to the CPU that was last pushed onto the CPU
  stack using the <tt><ref id=".PUSHCPU" name=".PUSHCPU"></tt> command, and
  remove this entry from the stack.

  The assembler will print an error message if the CPU stack is empty when
  this command is issued.

  See: <tt><ref id=".CPU" name=".CPU"></tt>, <tt><ref id=".PUSHCPU"
  name=".PUSHCPU"></tt>, <tt><ref id=".SETCPU" name=".SETCPU"></tt>


<sect1><tt>.POPSEG</tt><label id=".POPSEG"><p>

  Pop the last pushed segment from the stack, and set it.

  This command will switch back to the segment that was last pushed onto the
  segment stack using the <tt><ref id=".PUSHSEG" name=".PUSHSEG"></tt>
  command, and remove this entry from the stack.

  The assembler will print an error message if the segment stack is empty
  when this command is issued.

  See: <tt><ref id=".PUSHSEG" name=".PUSHSEG"></tt>


<sect1><tt>.PROC</tt><label id=".PROC"><p>

  Start a nested lexical level with the given name and adds a symbol with this
  name to the enclosing scope. All new symbols from now on are in the local
  lexical level and are accessible from outside only via <ref id="scopesyntax"
  name="explicit scope specification">. Symbols defined outside this local
  level may be accessed as long as their names are not used for new symbols
  inside the level. Symbols names in other lexical levels do not clash, so you
  may use the same names for identifiers. The lexical level ends when the
  <tt><ref id=".ENDPROC" name=".ENDPROC"></tt> command is read. Lexical levels
  may be nested up to a depth of 16 (this is an artificial limit to protect
  against errors in the source).

  Note: Macro names are always in the global level and in a separate name
  space. There is no special reason for this, it's just that I've never
  had any need for local macro definitions.

  Example:

  <tscreen><verb>
        .proc   Clear           ; Define Clear subroutine, start new level
                lda     #$00
        L1:     sta     Mem,y   ; L1 is local and does not cause a
                                ; duplicate symbol error if used in other
                                ; places
                dey
                bne     L1      ; Reference local symbol
                rts
        .endproc                ; Leave lexical level
  </verb></tscreen>

  See: <tt/<ref id=".ENDPROC" name=".ENDPROC">/ and <tt/<ref id=".SCOPE"
  name=".SCOPE">/


<sect1><tt>.PSC02</tt><label id=".PSC02"><p>

  Enable the 65SC02 instructions set. This instruction set includes all
  6502 instructions.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PC02"
  name=".PC02"></tt>, <tt><ref id=".P816" name=".P816"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.PSWEET16</tt><label id=".PSWEET16"><p>

  Enable the Sweet16 instructions set.

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PC02"
  name=".PC02"></tt>, <tt><ref id=".P816" name=".P816"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.PUSHCHARMAP</tt><label id=".PUSHCHARMAP"><p>

  Push the currently active character mapping onto a stack. The stack has a size of 16
  entries.

  <tt/.PUSHCHARMAP/ allows together with <tt><ref id=".POPCHARMAP"
  name=".POPCHARMAP"></tt> to switch to another character mapping and to restore the old
  character mapping later, without knowledge of the current mapping.

  The assembler will print an error message if the character mapping stack is already full,
  when this command is issued.

  See: <tt><ref id=".CHARMAP" name=".CHARMAP"></tt>, <tt><ref id=".POPCHARMAP"
  name=".POPCHARMAP"></tt>


<sect1><tt>.PUSHCPU</tt><label id=".PUSHCPU"><p>

  Push the currently active CPU onto a stack. The stack has a size of 8
  entries.

  <tt/.PUSHCPU/ allows together with <tt><ref id=".POPCPU"
  name=".POPCPU"></tt> to switch to another CPU and to restore the old CPU
  later, without knowledge of the current CPU setting.

  The assembler will print an error message if the CPU stack is already full,
  when this command is issued.

  See: <tt><ref id=".CPU" name=".CPU"></tt>, <tt><ref id=".POPCPU"
  name=".POPCPU"></tt>, <tt><ref id=".SETCPU" name=".SETCPU"></tt>


<sect1><tt>.PUSHSEG</tt><label id=".PUSHSEG"><p>

  Push the currently active segment onto a stack. The entries on the stack
  include the name of the segment and the segment type. The stack has a size
  of 16 entries.

  <tt/.PUSHSEG/ allows together with <tt><ref id=".POPSEG" name=".POPSEG"></tt>
  to switch to another segment and to restore the old segment later, without
  even knowing the name and type of the current segment.

  The assembler will print an error message if the segment stack is already
  full, when this command is issued.

  See: <tt><ref id=".POPSEG" name=".POPSEG"></tt>


<sect1><tt>.PWC02</tt><label id=".PWC02"><p>

  Enable the W65C02 instructions set. This instruction set includes all
  6502, 65SC02, 65C02 and two extra instructions (wai and stp)

  See: <tt><ref id=".P02" name=".P02"></tt>, <tt><ref id=".PSC02"
  name=".PSC02"></tt>, <tt><ref id=".P816" name=".P816"></tt>,
  <tt><ref id=".P4510" name=".P4510"></tt>, and
  <tt><ref id=".P45GS02" name=".P45GS02"></tt>


<sect1><tt>.REFERTO, .REFTO</tt><label id=".REFERTO"><p>

  Mark a symbol as referenced.

  It is useful in combination with the <tt><ref id=".IFREF" name=".IFREF"></tt>
  command. A subroutine with two entry points can be created. When the first
  entry point is called, it sets some default value as an argument, and falls
  through into the second entry point. <tt>.REFERTO</tt> helps to ensure that
  the second part is included into binary when only the first entry point is
  actually used from the code.

  Example:

  <tscreen><verb>
        .ifref NegateValue              ; If this subroutine is used
        NegateValue:                    ; Define it
                lda     #0
                sec
                sbc     Value
            .ifref ResetValue           ; If the ResetValue is also used
                jmp     SetValue        ; Jump over it
            .else
                .refto  SetValue        ; Ensure that SetValue will be included
            .endif
        .endif

        .ifref ResetValue               ; If this subroutine is used
        ResetValue:                     ; Define it
                lda     #0              ; Set a default value
                .refto  SetValue        ; Ensure that SetValue will be included
        .endif

        .ifref SetValue                 ; If this or previous subroutine is used
        SetValue:
                sta     Value
                rts
        .endif
  </verb></tscreen>


<sect1><tt>.RELOC</tt><label id=".RELOC"><p>

  Switch back to relocatable mode. See the <tt><ref id=".ORG"
  name=".ORG"></tt> command.


<sect1><tt>.REPEAT</tt><label id=".REPEAT"><p>

  Repeat all commands between <tt/.REPEAT/ and <tt><ref id=".ENDREPEAT"
  name=".ENDREPEAT"></tt> constant number of times. The command is followed by
  a constant expression that tells how many times the commands in the body
  should get repeated. Optionally, a comma and an identifier may be specified.
  If this identifier is found in the body of the repeat statement, it is
  replaced by the current repeat count (starting with zero for the first time
  the body is repeated).

  <tt/.REPEAT/ statements may be nested. If you use the same repeat count
  identifier for a nested <tt/.REPEAT/ statement, the one from the inner
  level will be used, not the one from the outer level.

  Example:

  The following macro will emit a string that is "encrypted" in that all
  characters of the string are XORed by the value $55.

  <tscreen><verb>
        .macro  Crypt   Arg
                .repeat .strlen(Arg), I
                .byte   .strat(Arg, I) ^ $55
                .endrep
        .endmacro
  </verb></tscreen>

  See: <tt><ref id=".ENDREPEAT" name=".ENDREPEAT"></tt>


<sect1><tt>.RES</tt><label id=".RES"><p>

  Reserve storage. The command is followed by one or two constant
  expressions. The first one is mandatory and defines, how many bytes of
  storage should be defined. The second, optional expression must be a
  constant byte value that will be used as value of the data. If there
  is no fill value given, the linker will use the value defined in the
  linker configuration file (default: zero).

  Example:

  <tscreen><verb>
        ; Reserve 12 bytes of memory with value $AA
        .res    12, $AA
  </verb></tscreen>


<sect1><tt>.RODATA</tt><label id=".RODATA"><p>

  Switch to the RODATA segment. The name of the RODATA segment is always
  "RODATA", so this is a shortcut for

  <tscreen><verb>
        .segment  "RODATA"
  </verb></tscreen>

  The RODATA segment is a segment that is used by the compiler for
  readonly data like string constants.

  See also the <tt><ref id=".SEGMENT" name=".SEGMENT"></tt> command.


<sect1><tt>.SCOPE</tt><label id=".SCOPE"><p>

  Start a nested lexical level with the given name. All new symbols from now
  on are in the local lexical level and are accessible from outside only via
  <ref id="scopesyntax" name="explicit scope specification">. Symbols defined
  outside this local level may be accessed as long as their names are not used
  for new symbols inside the level. Symbols names in other lexical levels do
  not clash, so you may use the same names for identifiers. The lexical level
  ends when the <tt><ref id=".ENDSCOPE" name=".ENDSCOPE"></tt> command is
  read. Lexical levels may be nested up to a depth of 16 (this is an
  artificial limit to protect against errors in the source).

  Note: Macro names are always in the global level and in a separate name
  space. There is no special reason for this, it's just that I've never
  had any need for local macro definitions.

  Example:

  <tscreen><verb>
        .scope  Error                   ; Start new scope named Error
                None = 0                ; No error
                File = 1                ; File error
                Parse = 2               ; Parse error
        .endscope                       ; Close lexical level

                ...
                lda #Error::File        ; Use symbol from scope Error
  </verb></tscreen>

  See: <tt/<ref id=".ENDSCOPE" name=".ENDSCOPE">/ and <tt/<ref id=".PROC"
  name=".PROC">/


<sect1><tt>.SEGMENT</tt><label id=".SEGMENT"><p>

  Switch to another segment. Code and data is always emitted into a
  segment, that is, a named section of data. The default segment is
  "CODE". There may be up to 254 different segments per object file
  (and up to 65534 per executable). There are shortcut commands for
  the most common segments ("ZEROPAGE", "CODE", "RODATA", "DATA", and "BSS").

  The command is followed by a string containing the segment name (there are
  some constraints for the name - as a rule of thumb use only those segment
  names that would also be valid identifiers). There may also be an optional
  address size separated by a colon. See the section covering <tt/<ref
  id="address-sizes" name="address sizes">/ for more information.

  The default address size for a segment depends on the memory model specified
  on the command line. The default is "absolute", which means that you don't
  have to use an address size modifier in most cases.

  "absolute" means that the is a segment with 16 bit (absolute) addressing.
  That is, the segment will reside somewhere in core memory outside the zero
  page. "zeropage" (8 bit) means that the segment will be placed in the zero
  page and direct (short) addressing is possible for data in this segment.

  Beware: Only labels in a segment with the zeropage attribute are marked
  as reachable by short addressing. The '*' (PC counter) operator will
  work as in other segments and will create absolute variable values.

  Please note that a segment cannot have two different address sizes. A
  segment specified as zeropage cannot be declared as being absolute later.

  Examples:

  <tscreen><verb>
        .segment "ROM2"                 ; Switch to ROM2 segment
        .segment "ZP2": zeropage        ; New direct segment
        .segment "ZP2"                  ; Ok, will use last attribute
        .segment "ZP2": absolute        ; Error, redecl mismatch
  </verb></tscreen>

  See: <tt><ref id=".BSS" name=".BSS"></tt>, <tt><ref id=".CODE"
  name=".CODE"></tt>, <tt><ref id=".DATA" name=".DATA"></tt>, <tt><ref
  id=".RODATA" name=".RODATA"></tt>, and <tt><ref id=".ZEROPAGE"
  name=".ZEROPAGE"></tt>


<sect1><tt>.SET</tt><label id=".SET"><p>

  <tt/.SET/ is used to assign a value to a variable. See <ref id="variables"
  name="Numeric variables"> for a full description.


<sect1><tt>.SETCPU</tt><label id=".SETCPU"><p>

  Switch the CPU instruction set. The command is followed by a string that
  specifies the CPU. Possible values are those that can also be supplied to
  the <tt><ref id="option--cpu" name="--cpu"></tt> command line option,
  namely: 6502, 6502X, 6502DTV, 65SC02, 65C02, 65816, 4510, 45GS02, HuC6280 and m740.

  See: <tt><ref id=".CPU" name=".CPU"></tt>,
       <tt><ref id=".IFP02" name=".IFP02"></tt>,
       <tt><ref id=".IFP02X" name=".IFP02X"></tt>,
       <tt><ref id=".IFPDTV" name=".IFPDTV"></tt>,
       <tt><ref id=".IFP816" name=".IFP816"></tt>,
       <tt><ref id=".IFPC02" name=".IFPC02"></tt>,
       <tt><ref id=".IFPM740" name=".IFPM740"></tt>,
       <tt><ref id=".IFPSC02" name=".IFPSC02"></tt>,
       <tt><ref id=".P02" name=".P02"></tt>,
       <tt><ref id=".P02X" name=".P02X"></tt>,
       <tt><ref id=".P816" name=".P816"></tt>,
       <tt><ref id=".P4510" name=".P4510"></tt>,
       <tt><ref id=".P45GS02" name=".P45GS02"></tt>,
       <tt><ref id=".PC02" name=".PC02"></tt>,
       <tt><ref id=".PM740" name=".PM740"></tt>,
       <tt><ref id=".PSC02" name=".PSC02"></tt>


<sect1><tt>.SMART</tt><label id=".SMART"><p>

  Switch on or off smart mode. The command can be followed by a '+' or '-'
  character to switch the option on or off respectively. The default is off
  (that is, the assembler doesn't try to be smart), but this default may be
  changed by the -s switch on the command line.

  In smart mode the assembler will do the following:

  <itemize>
  <item>Track usage of the <tt/REP/ and <tt/SEP/ instructions in 65816 mode
        and update the operand sizes accordingly. If the operand of such an
        instruction cannot be evaluated by the assembler (for example, because
        the operand is an imported symbol), a warning is issued. Beware: Since
        the assembler cannot trace the execution flow this may lead to false
        results in some cases. If in doubt, use the <tt/.Inn/ and <tt/.Ann/
        instructions to tell the assembler about the current settings.
  <item>In 65816 mode, if the <tt><ref id="long_jsr_jmp_rts"
        name="long_jsr_jmp_rts"></tt> feature is enabled,
        smart mode will replace a <tt/RTS/ instruction by <tt/RTL/ if it is
        used within a procedure declared as <tt/far/, or if the procedure has
        no explicit address specification, but it is <tt/far/ because of the
        memory model used.
  </itemize>

  Example:

  <tscreen><verb>
        .smart                          ; Be smart
        .smart  -                       ; Stop being smart
  </verb></tscreen>

  See: <tt><ref id=".A16" name=".A16"></tt>,
       <tt><ref id=".A8" name=".A8"></tt>,
       <tt><ref id=".I16" name=".I16"></tt>,
       <tt><ref id=".I8" name=".I8"></tt>


<sect1><tt>.STRUCT</tt><label id=".STRUCT"><p>

  Starts a struct definition. Structs are covered in a separate section named
  <ref id="structs" name="&quot;Structs and unions&quot;">.

  See also: <tt><ref id=".ENDSTRUCT" name=".ENDSTRUCT"></tt>,
            <tt><ref id=".ENDUNION" name=".ENDUNION"></tt>,
            <tt><ref id=".UNION" name=".UNION"></tt>


<sect1><tt>.TAG</tt><label id=".TAG"><p>

  Allocate space for a struct or union. This is equivalent to
  <tt><ref id=".RES" name=".RES"></tt> with the
  <tt><ref id=".SIZEOF" name=".SIZEOF"></tt> of a struct.

  Example:

  <tscreen><verb>
        .struct Point
                xcoord  .word
                ycoord  .word
        .endstruct

        .bss
                .tag    Point           ; Allocate 4 bytes
  </verb></tscreen>

  See: <ref id="structs" name="&quot;Structs and unions&quot;">

<sect1><tt>.UNDEF, .UNDEFINE</tt><label id=".UNDEFINE"><p>

  Delete a define style macro definition. The command is followed by an
  identifier which specifies the name of the macro to delete. Macro
  replacement is switched of when reading the token following the command
  (otherwise the macro name would be replaced by its replacement list).

  See also the <tt><ref id=".DEFINE" name=".DEFINE"></tt> command and
  section <ref id="macros" name="Macros">.


<sect1><tt>.UNION</tt><label id=".UNION"><p>

  Starts a union definition. Unions are covered in a separate section named
  <ref id="structs" name="&quot;Structs and unions&quot;">.

  See also: <tt><ref id=".ENDSTRUCT" name=".ENDSTRUCT"></tt>,
            <tt><ref id=".ENDUNION" name=".ENDUNION"></tt>,
            <tt><ref id=".STRUCT" name=".STRUCT"></tt>


<sect1><tt>.WARNING</tt><label id=".WARNING"><p>

  Force an assembly warning. The assembler will output a warning message
  preceded by "User warning". This warning will always be output, even if
  other warnings are disabled with the <tt><ref id="option-W" name="-W0"></tt>
  command line option.

  This command may be used to output possible problems when assembling
  the source file.

  Example:

  <tscreen><verb>
        .macro  jne     target
                .local L1
                .ifndef target
                .warning "Forward jump in jne, cannot optimize!"
                beq     L1
                jmp     target
        L1:
                .else
                ...
                .endif
        .endmacro
  </verb></tscreen>

  See also: <tt><ref id=".ERROR" name=".ERROR"></tt>,
            <tt><ref id=".FATAL" name=".FATAL"></tt>,
            <tt><ref id=".OUT" name=".OUT"></tt>


<sect1><tt>.WORD</tt><label id=".WORD"><p>

  Define word sized data. Must be followed by a sequence of (word ranged,
  but not necessarily constant) expressions.

  Example:

  <tscreen><verb>
        .word   $0D00, $AF13, _Clear
  </verb></tscreen>


<sect1><tt>.ZEROPAGE</tt><label id=".ZEROPAGE"><p>

  Switch to the ZEROPAGE segment and mark it as direct (zeropage) segment.
  The name of the ZEROPAGE segment is always "ZEROPAGE", so this is a
  shortcut for

  <tscreen><verb>
        .segment  "ZEROPAGE": zeropage
  </verb></tscreen>

  Because of the "zeropage" attribute, labels declared in this segment are
  addressed using direct addressing mode if possible. You <em/must/ instruct
  the linker to place this segment somewhere in the address range 0..$FF
  otherwise you will get errors.

  See: <tt><ref id=".SEGMENT" name=".SEGMENT"></tt>



<sect>Macros<label id="macros"><p>


<sect1>Introduction<p>

Macros may be thought of as "parametrized super instructions". Macros are
sequences of tokens that have a name. If that name is used in the source
file, the macro is "expanded", that is, it is replaced by the tokens that
were specified when the macro was defined.


<sect1>Macros without parameters<p>

In its simplest form, a macro does not have parameters. Here's an
example:

<tscreen><verb>
.macro  asr             ; Arithmetic shift right
        cmp     #$80    ; Put bit 7 into carry
        ror             ; Rotate right with carry
.endmacro
</verb></tscreen>

The macro above consists of two real instructions, that are inserted into
the code, whenever the macro is expanded. Macro expansion is simply done
by using the name, like this:

<tscreen><verb>
        lda     $2010
        asr
        sta     $2010
</verb></tscreen>


<sect1>Parametrized macros<p>

When using macro parameters, macros can be even more useful:

<tscreen><verb>
.macro  inc16   addr
        clc
        lda     addr
        adc     #<$0001
        sta     addr
        lda     addr+1
        adc     #>$0001
        sta     addr+1
.endmacro
</verb></tscreen>

When calling the macro, you may give a parameter, and each occurrence of
the name "addr" in the macro definition will be replaced by the given
parameter. So

<tscreen><verb>
        inc16   $1000
</verb></tscreen>

will be expanded to

<tscreen><verb>
        clc
        lda     $1000
        adc     #<$0001
        sta     $1000
        lda     $1000+1
        adc     #>$0001
        sta     $1000+1
</verb></tscreen>

A macro may have more than one parameter, in this case, the parameters
are separated by commas. You are free to give less parameters than the
macro actually takes in the definition. You may also leave intermediate
parameters empty. Empty parameters are replaced by empty space (that is,
they are removed when the macro is expanded). If you have a look at our
macro definition above, you will see, that replacing the "addr" parameter
by nothing will lead to wrong code in most lines.

The names "a", "x" and "y" should be avoided for macro parameters, as these
will usually conflict with the 6502 registers.

For writing macros with a variable parameter list, control commands are
available:

<tt><ref id=".IFBLANK" name=".IFBLANK"></tt> tests the rest of the line and
returns true, if there are any tokens on the remainder of the line. Since
empty parameters are replaced by nothing, this may be used to test if a given
parameter is empty. <tt><ref id=".IFNBLANK" name=".IFNBLANK"></tt> tests the
opposite.

Look at this example:

<tscreen><verb>
.macro  ldaxy   i, j, k
.ifnblank       i
        lda     #i
.endif
.ifnblank       j
        ldx     #j
.endif
.ifnblank       k
        ldy     #k
.endif
.endmacro
</verb></tscreen>

That macro may be called as follows:

<tscreen><verb>
        ldaxy   1, 2, 3         ; Load all three registers

        ldaxy   1, , 3          ; Load only a and y

        ldaxy   , , 3           ; Load y only
</verb></tscreen>

There's another helper command for determining which macro parameters are
valid: <tt><ref id=".PARAMCOUNT" name=".PARAMCOUNT"></tt>. That command is
replaced by the parameter count given, <em/including/ explicitly empty
parameters:

<tscreen><verb>
        ldaxy   1       ; .PARAMCOUNT = 1
        ldaxy   1,,3    ; .PARAMCOUNT = 3
        ldaxy   1,2     ; .PARAMCOUNT = 2
        ldaxy   1,      ; .PARAMCOUNT = 2
        ldaxy   1,2,3   ; .PARAMCOUNT = 3
</verb></tscreen>

Macro parameters may optionally be enclosed into curly braces. This allows the
inclusion of tokens that would otherwise terminate the parameter (the comma in
case of a macro parameter).

<tscreen><verb>
.macro  foo     arg1, arg2
        ...
.endmacro

        foo     ($00,x)         ; Two parameters passed
        foo     {($00,x)}       ; One parameter passed
</verb></tscreen>

In the first case, the macro is called with two parameters: '<tt/(&dollar;00/'
and '<tt/x)/'. The comma is not passed to the macro, because it is part of the
calling sequence, not the parameters.

In the second case, '<tt/(&dollar;00,x)/' is passed to the macro; this time,
including the comma.


<sect1>Detecting parameter types<p>

Sometimes it is nice to write a macro that acts differently depending on the
type of the argument supplied. An example would be a macro that loads a 16 bit
value from either an immediate operand, or from memory. The <tt/<ref
id=".MATCH" name=".MATCH">/ and <tt/<ref id=".XMATCH" name=".XMATCH">/
functions will allow you to do exactly this:

<tscreen><verb>
.macro  ldax    arg
        .if (.match (.left (1, {arg}), #))
            ; immediate mode
            lda     #<(.right (.tcount ({arg})-1, {arg}))
            ldx     #>(.right (.tcount ({arg})-1, {arg}))
        .else
            ; assume absolute or zero page
            lda     arg
            ldx     1+(arg)
        .endif
.endmacro
</verb></tscreen>

Using the <tt/<ref id=".MATCH" name=".MATCH">/ function, the macro is able to
check if its argument begins with a hash mark. If so, two immediate loads are
emitted, Otherwise a load from an absolute zero page memory location is
assumed. Please note how the curly braces are used to enclose parameters to
pseudo functions handling token lists. This is necessary, because the token
lists may include commas or parens, which would be treated by the assembler
as end-of-list.

The macro can be used as

<tscreen><verb>
foo:    .word   $5678
...
        ldax    #$1234          ; X=$12, A=$34
...
        ldax    foo             ; X=$56, A=$78
</verb></tscreen>


<sect1>Recursive macros<p>

Macros may be used recursively:

<tscreen><verb>
.macro  push    r1, r2, r3
        lda     r1
        pha
.ifnblank       r2
        push    r2, r3
.endif
.endmacro
</verb></tscreen>

There's also a special macro command to help with writing recursive macros:
<tt><ref id=".EXITMACRO" name=".EXITMACRO"></tt>. That command will stop macro
expansion immediately:

<tscreen><verb>
.macro  push    r1, r2, r3, r4, r5, r6, r7
.ifblank        r1
        ; First parameter is empty
        .exitmacro
.else
        lda     r1
        pha
.endif
        push    r2, r3, r4, r5, r6, r7
.endmacro
</verb></tscreen>

When expanding that macro, the expansion will push all given parameters
until an empty one is encountered. The macro may be called like this:

<tscreen><verb>
        push    $20, $21, $32   ; Push 3 ZP locations
        push    $21             ; Push one ZP location
</verb></tscreen>


<sect1>Local symbols inside macros<p>

Now, with recursive macros, <tt><ref id=".IFBLANK" name=".IFBLANK"></tt> and
<tt><ref id=".PARAMCOUNT" name=".PARAMCOUNT"></tt>, what else do you need?
Have a look at the inc16 macro above. Here is it again:

<tscreen><verb>
.macro  inc16   addr
        clc
        lda     addr
        adc     #<$0001
        sta     addr
        lda     addr+1
        adc     #>$0001
        sta     addr+1
.endmacro
</verb></tscreen>

If you have a closer look at the code, you will notice, that it could be
written more efficiently, like this:

<tscreen><verb>
.macro  inc16   addr
        inc     addr
        bne     Skip
        inc     addr+1
Skip:
.endmacro
</verb></tscreen>

But imagine what happens, if you use this macro twice? Since the label "Skip"
has the same name both times, you get a "duplicate symbol" error. Without a
way to circumvent this problem, macros are not as useful, as they could be.
One possible solution is the command <tt><ref id=".LOCAL" name=".LOCAL"></tt>.
It declares one or more symbols as local to the macro expansion. The names of
local variables are replaced by a unique name in each separate macro
expansion. So we can solve the problem above by using <tt/.LOCAL/:

<tscreen><verb>
.macro  inc16   addr
        .local  Skip            ; Make Skip a local symbol
        inc     addr
        bne     Skip
        inc     addr+1
Skip:                           ; Not visible outside
.endmacro
</verb></tscreen>

Another solution is of course to start a new lexical block inside the macro
that hides any labels:

<tscreen><verb>
.macro  inc16   addr
.proc
        inc     addr
        bne     Skip
        inc     addr+1
Skip:
.endproc
.endmacro
</verb></tscreen>


<sect1>C style macros<p>

Starting with version 2.5 of the assembler, there is a second macro type
available: C style macros using the <tt/.DEFINE/ directive. These macros are
similar to the classic macro type described above, but behaviour is sometimes
different:

<itemize>

<item>  Macros defined with <tt><ref id=".DEFINE" name=".DEFINE"></tt> may not
        span more than a line. You may use line continuation (see <tt><ref
        id="line_continuations" name="line_continuations"></tt>) to spread the
        definition over more than one line for increased readability, but the
        macro itself may not contain an end-of-line token.

<item>  Macros defined with <tt><ref id=".DEFINE" name=".DEFINE"></tt> share
        the name space with classic macros, but they are detected and replaced
        at the scanner level. While classic macros may be used in every place,
        where a mnemonic or other directive is allowed, <tt><ref id=".DEFINE"
        name=".DEFINE"></tt> style macros are allowed anywhere in a line. So
        they are more versatile in some situations.

<item>  <tt><ref id=".DEFINE" name=".DEFINE"></tt> style macros may take
        parameters. While classic macros may have empty parameters, this is
        not true for <tt><ref id=".DEFINE" name=".DEFINE"></tt> style macros.
        For this macro type, the number of actual parameters must match
        exactly the number of formal parameters.

        To make this possible, formal parameters are enclosed in parentheses when
        defining the macro. If there are no parameters, the empty parentheses may
        be omitted.

<item>  Since <tt><ref id=".DEFINE" name=".DEFINE"></tt> style macros may not
        contain end-of-line tokens, there are things that cannot be done. They
        may not contain several processor instructions for example. So, while
        some things may be done with both macro types, each type has special
        usages. The types complement each other.

<item>  Parentheses work differently from C macros.
        The common practice of wrapping C macros in parentheses may cause
        unintended problems here, such as accidentally implying an
        indirect addressing mode. While the definition of a macro requires
        parentheses around its argument list, when invoked they should not be
        included.

</itemize>

Let's look at a few examples to make the advantages and disadvantages
clear.

To emulate assemblers that use "<tt/EQU/" instead of "<tt/=/" you may use the
following <tt/.DEFINE/:

<tscreen><verb>
.define EQU     =

foo     EQU     $1234           ; This is accepted now
</verb></tscreen>

You may use the directive to define string constants used elsewhere:

<tscreen><verb>
; Define the version number
.define VERSION "12.3a"

        ; ... and use it
        .asciiz VERSION
</verb></tscreen>

Macros with parameters may also be useful:

<tscreen><verb>
.define DEBUG(message)  .out    message

        DEBUG   "Assembling include file #3"
</verb></tscreen>

Note that, while formal parameters have to be placed in parentheses,
the actual argument used when invoking the macro should not be.
The invoked arguments are separated by commas only; if parentheses are
used by accident, they will become part of the replaced token.

If you wish to have an expression follow the macro invocation, the
last parameter can be enclosed in curly braces {} to indicate the end of that
argument.

Examples:

<tscreen><verb>
.define COMBINE(ta,tb,tc) ta+tb*10+tc*100

.word COMBINE 5,6,7      ; 5+6*10+7*100 = 765
.word COMBINE(5,6,7)     ; (5+6*10+7)*100 = 7200 ; incorrect use of parentheses
.word COMBINE 5,6,7+1    ; 5+6*10+7+1*100 = 172
.word COMBINE 5,6,{7}+1  ; 5+6*10+7*100+1 = 766 ; {} encloses the argument
.word COMBINE 5,6-2,7    ; 5+6-2*10+7*100 = 691
.word COMBINE 5,(6-2),7  ; 5+(6-2)*10+7*100 = 745
.word COMBINE 5,6,7+COMBINE 0,1,2    ; 5+6*10+7+0+1*10+2*100*100 = 20082
.word COMBINE 5,6,{7}+COMBINE 0,1,2  ; 5+6*10+7*100+0+1*10+2*100 = 975
</verb></tscreen>

With C macros it is common to enclose the results in parentheses to
prevent unintended interactions with the text of the arguments, but
additional care must be taken in this assembly context where parentheses
may alter the meaning of a statement. In particular, indirect addressing modes
may be accidentally implied:

<tscreen><verb>
.define DUO(ta,tb) (ta+(tb*10))

        lda DUO(5,4), Y         ; LDA (indirect), Y
        lda 0+DUO(5,4), Y       ; LDA absolute indexed, Y
</verb></tscreen>


<sect1>Characters in macros<p>

When using the <ref id="option-t" name="-t"> option, characters are translated
into the target character set of the specific machine. However, this happens
as late as possible. This means that strings are translated if they are part
of a <tt><ref id=".BYTE" name=".BYTE"></tt> or <tt><ref id=".ASCIIZ"
name=".ASCIIZ"></tt> command. Characters are translated as soon as they are
used as part of an expression.

This behaviour is very intuitive outside of macros but may be confusing when
doing more complex macros. If you compare characters against numeric values,
be sure to take the translation into account.


<sect1>Deleting macros<p>

Macros can be deleted. This will not work if the macro that should be deleted
is currently expanded as in the following non-working example:

<tscreen><verb>
.macro  notworking
        .delmacro       notworking
.endmacro

        notworking              ; Will not work
</verb></tscreen>

The commands to delete classic and define style macros differ. Classic macros
can be deleted by use of <tt><ref id=".DELMACRO" name=".DELMACRO"></tt>, while
for <tt><ref id=".DEFINE" name=".DEFINE"></tt> style macros, <tt><ref
id=".UNDEFINE" name=".UNDEFINE"></tt> must be used. Example:

<tscreen><verb>
.define value   1
.macro  mac
        .byte   2
.endmacro

        .byte   value           ; Emit one byte with value 1
        mac                     ; Emit another byte with value 2

.undefine value
.delmacro mac

        .byte   value           ; Error: Unknown identifier
        mac                     ; Error: Missing ":"
</verb></tscreen>

A separate command for <tt>.DEFINE</tt> style macros was necessary, because
the name of such a macro is replaced by its replacement list on a very low
level. To get the actual name, macro replacement has to be switched off when
reading the argument to <tt>.UNDEFINE</tt>. This does also mean that the
argument to <tt>.UNDEFINE</tt> is not allowed to come from another
<tt>.DEFINE</tt>. All this is not necessary for classic macros, so having two
different commands increases flexibility.



<sect>Macro packages<label id="macropackages"><p>

Using the <tt><ref id=".MACPACK" name=".MACPACK"></tt> directive, predefined
macro packages may be included with just one command. Available macro packages
are:


<sect1><tt>.MACPACK generic</tt><p>

This macro package defines macros that are useful in almost any program.
Currently defined macros are:

<tscreen><verb>
        .macro  add     Arg     ; add without carry
                clc
                adc     Arg
        .endmacro

        .macro  sub     Arg     ; subtract without borrow
                sec
                sbc     Arg
        .endmacro

        .macro  bge     Arg     ; branch on greater-than or equal
                bcs     Arg
        .endmacro

        .macro  blt     Arg     ; branch on less-than
                bcc     Arg
        .endmacro

        .macro  bgt     Arg     ; branch on greater-than
                .local  L
                beq     L
                bcs     Arg
        L:
        .endmacro

        .macro  ble     Arg     ; branch on less-than or equal
                beq     Arg
                bcc     Arg
        .endmacro

        .macro  bnz     Arg     ; branch on not zero
                bne     Arg
        .endmacro

        .macro  bze     Arg     ; branch on zero
                beq     Arg
        .endmacro
</verb></tscreen>


<sect1><tt>.MACPACK longbranch</tt><p>

This macro package defines long conditional jumps. They are named like the
short counterpart but with the 'b' replaced by a 'j'. Here is a sample
definition for the "<tt/jeq/" macro, the other macros are built using the same
scheme:

<tscreen><verb>
        .macro  jeq     Target
                .if     .def(Target) .and ((*+2)-(Target) <= 127)
                beq     Target
                .else
                bne     *+5
                jmp     Target
                .endif
        .endmacro
</verb></tscreen>

All macros expand to a short branch, if the label is already defined (back
jump) and is reachable with a short jump. Otherwise the macro expands to a
conditional branch with the branch condition inverted, followed by an absolute
jump to the actual branch target.

The package defines the following macros:

<tscreen><verb>
        jeq, jne, jmi, jpl, jcs, jcc, jvs, jvc
</verb></tscreen>



<sect1><tt>.MACPACK apple2</tt><p>

This macro package defines a macro named <tt/scrcode/. It takes a string
as argument and places this string into memory translated into screen codes.


<sect1><tt>.MACPACK atari</tt><p>

This macro package defines a macro named <tt/scrcode/. It takes a string
as argument and places this string into memory translated into screen codes.


<sect1><tt>.MACPACK cbm</tt><p>

This macro package defines a macro named <tt/scrcode/. It takes a string
as argument and places this string into memory translated into screen codes.


<sect1><tt>.MACPACK module</tt><p>

This macro package defines a macro named <tt/module_header/. It takes an
identifier as argument and is used to define the header of a module both
in the dynamic and static variant.



<sect>Predefined constants<label id="predefined-constants"><p>

For better orthogonality, the assembler defines similar symbols as the
compiler, depending on the target system selected:

<itemize>
<item><tt/__APPLE2__/ - Target system is <tt/apple2/ or <tt/apple2enh/
<item><tt/__APPLE2ENH__/ - Target system is <tt/apple2enh/
<item><tt/__ATARI2600__/ - Target system is <tt/atari2600/
<item><tt/__ATARI5200__/ - Target system is <tt/atari5200/
<item><tt/__ATARI7800__/ - Target system is <tt/atari7800/
<item><tt/__ATARI__/ - Target system is <tt/atari/ or <tt/atarixl/
<item><tt/__ATARIXL__/ - Target system is <tt/atarixl/
<item><tt/__ATMOS__/ - Target system is <tt/atmos/
<item><tt/__BBC__/ - Target system is <tt/bbc/
<item><tt/__C128__/ - Target system is <tt/c128/
<item><tt/__C16__/ - Target system is <tt/c16/ or <tt/plus4/
<item><tt/__C64__/ - Target system is <tt/c64/
<item><tt/__CBM__/ - Target is a Commodore or Commodore-alike system
<item><tt/__CBM510__/ - Target system is <tt/cbm510/
<item><tt/__CBM610__/ - Target system is <tt/cbm610/
<item><tt/__CX16__/ - Target system is <tt/cx16/
<item><tt/__GEOS__/ - Target is a GEOS system
<item><tt/__GEOS_APPLE__/ - Target system is <tt/geos-apple/
<item><tt/__GEOS_CBM__/ - Target system is <tt/geos-cbm/
<item><tt/__LUNIX__/ - Target system is <tt/lunix/
<item><tt/__LYNX__/ - Target system is <tt/lynx/
<item><tt/__NES__/ - Target system is <tt/nes/
<item><tt/__OSIC1P__/ - Target system is <tt/osic1p/
<item><tt/__PET__/ - Target system is <tt/pet/
<item><tt/__PLUS4__/ - Target system is <tt/plus4/
<item><tt/__SIM6502__/ - Target system is <tt/sim6502/
<item><tt/__SIM65C02__/ - Target system is <tt/sim65c02/
<item><tt/__SUPERVISION__/ - Target system is <tt/supervision/
<item><tt/__SYM1__/ - Target system is <tt/sym1/
<item><tt/__VIC20__/ - Target system is <tt/vic20/
</itemize>



<sect>Structs and unions<label id="structs"><p>

<sect1>Structs and unions Overview<p>

Structs and unions are special forms of <ref id="scopes" name="scopes">.  They
are, to some degree, comparable to their C counterparts. Both have a list of
members. Each member allocates storage, and optionally may have a name.

Each named member has a constant value equal to the storage offset from the
beginning of the structure. In the case of a union, all members are placed at
the same offset, typically 0.

Each named member also has a storage size which can be accessed with the
<tt><ref id=".SIZEOF" name=".SIZEOF"></tt> operator. The struct or union itself
also has a <tt/.SIZEOF/ indicating its total storage size.

<sect1>Declaration<p>

Here is an example for a very simple struct with two members and a total size
of 4 bytes:
<tscreen><verb>
      .struct Point
              xcoord  .word
              ycoord  .word
      .endstruct
</verb></tscreen>

A union shares the total space between all its members; its size is the same
as that of the largest member. The offset of all members relative to the union
is zero.
<tscreen><verb>
      .union  Entry
              index   .word
              ptr     .addr
      .endunion
</verb></tscreen>

A struct or union may not necessarily have a name. If it is anonymous, no
local scope is opened; the identifiers used to name the members are placed
into the current scope instead.

Storage allocators may contain a multiplier. A struct may also contain members
and definitions of local structs/unions. Example:

<tscreen><verb>
      .struct Circle
              .struct Point
                      .word   2         ; Allocate two words
              .endstruct
              Radius  .word
      .endstruct
</verb></tscreen>

In this example the size of the Circle struct is 6 (three words).


<sect1>The storage allocator keywords<p>

  <descrip>

  <tag/.BYTE, .RES/
    Allocates multiples of 1 byte.  <tt/.RES/ requires an operand.

  <tag/.DBYT, .WORD, .ADDR/
    Allocates multiples of 2 bytes.

  <tag/.FARADDR/
    Allocates multiples of 3 bytes.

  <tag/.DWORD/
    Allocates multiples of 4 bytes.

  <tag/.TAG/
    Allocates a previously defined struct.

  <tag/.STRUCT, .UNION/
    Begins a nested .struct or .union definition, and allocates it.
    Note that its member offset values will begin at 0, unless this nested
    structure is anonymous, in which case they will instead become members of
    the enclosing scope.

  </descrip>


<sect1>The <tt/.ORG/ keyword<p>

The <tt/.ORG/ keyword changes the offset value that is assigned to subsequent
member names.  It's useful when using a struct to define the names of the
registers in an I/O chip.  Example:
<tscreen><verb>
; 6551
.struct ACIA            ; Asynchronous Communications Interface Adapter
        .org    $031C
DATA    .byte
STATUS  .byte
CMD     .byte           ; Command register
CTRL    .byte           ; Control register
.endstruct

        lda     ACIA::DATA      ; Get an RS-232 character
</verb></tscreen>


<sect1>The <tt/.TAG/ keyword<p>

By using the <ref id=".TAG" name=".TAG"> keyword, it is possible to reserve
space for an already defined struct or union within another struct:
<tscreen><verb>
      .struct Point
              xcoord  .word
              ycoord  .word
      .endstruct

      .struct Circle
              Origin  .tag    Point
              Radius  .byte
      .endstruct
</verb></tscreen>

Actual space for a struct or union may be allocated by using the <ref id=".TAG"
name=".TAG"> directive.
<tscreen><verb>
C:      .tag    Circle
</verb></tscreen>

Members are just offsets from the start of the struct or union. To
access a field of a struct, the member offset must be added to the address of
the struct variable itself:
<tscreen><verb>
        lda    C + Circle::Radius                    ; Load circle radius
        lda    C + Circle::Origin + Point::ycoord    ; Load circle origin.ycoord
</verb></tscreen>

Nested structures or unions are treated differently depending on whether they
are anonymous. If named, a new structure definition is created within the
enclosing scope, with its offsets beginning at 0. If anonymous, the members of
the new structure are added to the enclosing scope instead, with offsets
continuing through that scope. Example:

<tscreen><verb>
      .struct Object
              id .byte                ; Object::id = 0
              target .struct Point    ; Object::target = 1
                      xcoord  .word   ; Object::Point::xcoord = 0
                      ycoord  .word   ; Object::Point::ycoord = 2
              .endstruct
               cost .struct           ; Object::cost = 5
                      price  .word    ; Object::price = 5
                      tax  .word      ; Object::tax = 7
              .endstruct
              .struct
                      radius  .word   ; Object::radius = 9
              .endstruct
      .endstruct

O:    .tag   Object
      lda    O + Object::target + Object::Point::ycoord  ; Named struct
      lda    O + Object::tax                             ; Anonymous
      lda    O + Object::radius                          ; Anonymous

      ; Be careful not to use a named nested structure without also adding the
      ; offset to the nested structure itself.
      lda    O + Object::Point::ycoord                   ; Incorrect!
      lda    O + Object::target + Object::Point::ycoord  ; Correct
</verb></tscreen>

In this example, the first nested structure is named "Point", and its member
offsets begin at 0. On the other hand, the two anonymous structures simply
continue to add members to the enclosing "Object" structure.

Note that an anonymous structure does not need a member name, since all of its
members become part of the enclosing structure. The "cost" member in the
example is redundantly the same offset as its first member "price".


<sect1>Limitations<p>

Structs and unions currently are implemented as nested symbol tables (in fact,
they were a by-product of the improved scoping rules). Currently, the
assembler has no idea of types. That means that the <ref id=".TAG"
name=".TAG"> keyword only will allocate space. You won't be able to initialize
variables declared with <ref id=".TAG" name=".TAG">; and, adding an embedded
structure to another structure with <ref id=".TAG" name=".TAG"> will not make
that added structure accessible by using the '::' operator.



<sect>Module constructors/destructors<label id="condes"><p>

<em>Note:</em> This section applies mostly to C programs, so the explanation
below uses examples from the C libraries. However, the feature may also be
useful for assembler programs.


<sect1>Module constructors/destructors Overview<p>

Using the <tt><ref id=".CONSTRUCTOR" name=".CONSTRUCTOR"></tt>, <tt><ref
id=".DESTRUCTOR" name=".DESTRUCTOR"></tt> and <tt><ref id=".INTERRUPTOR"
name=".INTERRUPTOR"></tt> keywords it is possible to export functions in a
special way. The linker is able to generate tables with all functions of a
specific type. Such a table will <em>only</em> include symbols from object
files that are linked into a specific executable. This may be used to add
initialization and cleanup code for library modules, or a table of interrupt
handler functions.

The C heap functions are an example where module initialization code is used.
All heap functions (<tt>malloc</tt>, <tt>free</tt>, ...) work with a few
variables that contain the start and the end of the heap, pointers to the free
list and so on. Since the end of the heap depends on the size and start of the
stack, it must be initialized at runtime. However, initializing these
variables for programs that do not use the heap are a waste of time and
memory.

So the central module defines a function that contains initialization code and
exports this function using the <tt/.CONSTRUCTOR/ statement. If (and only if)
this module is added to an executable by the linker, the initialization
function will be placed into the table of constructors by the linker. The C
startup code will call all constructors before <tt/main/ and all destructors
after <tt/main/, so without any further work, the heap initialization code is
called once the module is linked in.

While it would be possible to add explicit calls to initialization functions
in the startup code, the new approach has several advantages:

<enum>
<item>
If a module is not included, the initialization code is not linked in and not
called. So you don't pay for things you don't need.

<item>
Adding another library that needs initialization does not mean that the
startup code has to be changed. Before we had module constructors and
destructors, the startup code for all systems had to be adjusted to call the
new initialization code.

<item>
The feature saves memory: Each additional initialization function needs just
two bytes in the table (a pointer to the function).

</enum>


<sect1>Calling order<p>

The symbols are sorted in increasing priority order by the linker when using
one of the builtin linker configurations, so the functions with lower
priorities come first and are followed by those with higher priorities. The C
library runtime subroutine that walks over the function tables calls the
functions starting from the top of the table - which means that functions with
a high priority are called first.

So when using the C runtime, functions are called with high priority functions
first, followed by low priority functions.


<sect1>Pitfalls<p>

When using these special symbols, please take care of the following:

<itemize>

<item>
The linker will only generate function tables, it will not generate code to
call these functions. If you're using the feature in some other than the
existing C environments, you have to write code to call all functions in a
linker generated table yourself. See the <tt/condes/ and <tt/callirq/ modules
in the C runtime for an example on how to do this.

<item>
The linker will only add addresses of functions that are in modules linked to
the executable. This means that you have to be careful where to place the
condes functions. If initialization or an irq handler is needed for a group of
functions, be sure to place the function into a module that is linked in
regardless of which function is called by the user.

<item>
The linker will generate the tables only when requested to do so by the
<tt/FEATURE CONDES/ statement in the linker config file. Each table has to
be requested separately.

<item>
Constructors and destructors may have priorities. These priorities determine
the order of the functions in the table. If your initialization or cleanup code
does depend on other initialization or cleanup code, you have to choose the
priority for the functions accordingly.

<item>
Besides the <tt><ref id=".CONSTRUCTOR" name=".CONSTRUCTOR"></tt>, <tt><ref
id=".DESTRUCTOR" name=".DESTRUCTOR"></tt> and <tt><ref id=".INTERRUPTOR"
name=".INTERRUPTOR"></tt> statements, there is also a more generic command:
<tt><ref id=".CONDES" name=".CONDES"></tt>. This allows to specify an
additional type. Predefined types are 0 (constructor), 1 (destructor) and 2
(interruptor). The linker generates a separate table for each type on request.

</itemize>


<sect>Porting sources from other assemblers<p>

Sometimes it is necessary to port code written for older assemblers to ca65.
In some cases, this can be done without any changes to the source code by
using the emulation features of ca65 (see <tt><ref id=".FEATURE"
name=".FEATURE"></tt>). In other cases, it is necessary to make changes to the
source code.

Probably the biggest difference is the handling of the <tt><ref id=".ORG"
name=".ORG"></tt> directive. ca65 generates relocatable code, and placement is
done by the linker. Most other assemblers generate absolute code, placement is
done within the assembler and there is no external linker.

In general it is not a good idea to write new code using the emulation
features of the assembler, but there may be situations where even this rule is
not valid.

<sect1>TASS<p>

You need to use some of the ca65 emulation features to simulate the behaviour
of such simple assemblers.

<enum>
<item>Prepare your sourcecode like this:

<tscreen><verb>
        ; if you want TASS style labels without colons
        .feature labels_without_colons

        ; if you want TASS style character constants
        ; ("a" instead of the default 'a')
        .feature loose_char_term

                .word *+2       ; the cbm load address

                [yourcode here]
</verb></tscreen>

notice that the two emulation features are mostly useful for porting
sources originally written in/for TASS, they are not needed for the
actual "simple assembler operation" and are not recommended if you are
writing new code from scratch.

<item>Replace all program counter assignments (which are not possible in ca65
by default, and the respective emulation feature works different from what
you'd expect) by another way to skip to memory locations, for example the
<tt><ref id=".RES" name=".RES"></tt> directive.

<tscreen><verb>
        ; *=$2000
        .res $2000-*    ; reserve memory up to $2000
</verb></tscreen>

Please note that other than the original TASS, ca65 can never move the program
counter backwards - think of it as if you are assembling to disk with TASS.

<item>Conditional assembly (<tt/.ifeq//<tt/.endif//<tt/.goto/ etc.) must be
rewritten to match ca65 syntax. Most importantly notice that due to the lack
of <tt/.goto/, everything involving loops must be replaced by
<tt><ref id=".REPEAT" name=".REPEAT"></tt>.

<item>To assemble code to a different address than it is executed at, use the
<tt><ref id=".ORG" name=".ORG"></tt> directive instead of
<tt/.offs/-constructs.

<tscreen><verb>
        .org $1800

        [floppy code here]

        .reloc  ; back to normal
</verb></tscreen>

<item>Then assemble like this:

<tscreen><verb>
        cl65 --start-addr 0x0ffe -t none myprog.s -o myprog.prg
</verb></tscreen>

Note that you need to use the actual start address minus two, since two bytes
are used for the cbm load address.

</enum>


<sect>Copyright<p>

ca65 (and all cc65 binutils) are (C) Copyright 1998-2003 Ullrich von
Bassewitz. For usage of the binaries and/or sources the following
conditions do apply:

This software is provided 'as-is', without any expressed or implied
warranty.  In no event will the authors be held liable for any damages
arising from the use of this software.

Permission is granted to anyone to use this software for any purpose,
including commercial applications, and to alter it and redistribute it
freely, subject to the following restrictions:

<enum>
<item>  The origin of this software must not be misrepresented; you must not
        claim that you wrote the original software. If you use this software
        in a product, an acknowledgment in the product documentation would be
        appreciated but is not required.
<item>  Altered source versions must be plainly marked as such, and must not
        be misrepresented as being the original software.
<item>  This notice may not be removed or altered from any source
        distribution.
</enum>



</article>
