(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "unconnected-(D1-K-Pad1)")
  (net 2 "unconnected-(D1-A-Pad2)")
  (net 3 "unconnected-(D2-K-Pad1)")
  (net 4 "unconnected-(D2-A-Pad2)")
  (net 5 "unconnected-(D3-K-Pad1)")
  (net 6 "unconnected-(D3-A-Pad2)")
  (net 7 "unconnected-(D4-K-Pad1)")
  (net 8 "unconnected-(D4-A-Pad2)")
  (net 9 "unconnected-(D5-K-Pad1)")
  (net 10 "unconnected-(D5-A-Pad2)")
  (net 11 "unconnected-(D6-K-Pad1)")
  (net 12 "unconnected-(D6-A-Pad2)")
  (net 13 "unconnected-(D7-K-Pad1)")
  (net 14 "unconnected-(D7-A-Pad2)")
  (net 15 "unconnected-(D8-K-Pad1)")
  (net 16 "unconnected-(D8-A-Pad2)")
  (net 17 "unconnected-(J1-Pad0)")
  (net 18 "unconnected-(J1-Pad1)")
  (net 19 "unconnected-(J1-Pad2)")
  (net 20 "unconnected-(J1-Pad3)")
  (net 21 "unconnected-(J1-Pad4)")
  (net 22 "unconnected-(J1-Pad5)")
  (net 23 "unconnected-(J1-Pad6)")
  (net 24 "unconnected-(J1-Pad7)")
  (net 25 "unconnected-(J1-Pad8)")
  (net 26 "unconnected-(J1-Pad9)")
  (net 27 "unconnected-(J1-Pad10)")
  (net 28 "unconnected-(J1-Pad11)")
  (net 29 "unconnected-(J1-Pad12)")
  (net 30 "unconnected-(J1-Pad13)")
  (net 31 "unconnected-(J1-Pad14)")
  (net 32 "unconnected-(J1-Pad15)")
  (net 33 "unconnected-(J2-Pad1)")
  (net 34 "unconnected-(J2-Pad2)")
  (net 35 "unconnected-(J2-Pad3)")
  (net 36 "unconnected-(J2-Pad4)")
  (net 37 "unconnected-(J2-Pad5)")
  (net 38 "unconnected-(J2-Pad6)")
  (net 39 "unconnected-(J2-Pad7)")
  (net 40 "unconnected-(J2-Pad8)")
  (net 41 "unconnected-(J2-Pad9)")
  (net 42 "unconnected-(J2-Pad10)")
  (net 43 "unconnected-(J2-Pad11)")
  (net 44 "unconnected-(J2-Pad12)")
  (net 45 "unconnected-(J2-Pad13)")
  (net 46 "unconnected-(J2-Pad14)")
  (net 47 "unconnected-(J2-Pad15)")
  (net 48 "unconnected-(J2-Pad16)")
  (net 49 "unconnected-(J2-Pad17)")
  (net 50 "unconnected-(J2-Pad18)")
  (net 51 "unconnected-(J2-Pad19)")
  (net 52 "unconnected-(J2-SHIELD-PadS1)")
  (net 53 "unconnected-(J2-SHIELD__1-PadS2)")
  (net 54 "unconnected-(J2-SHIELD__2-PadS3)")
  (net 55 "unconnected-(J2-SHIELD__3-PadS4)")
  (net 56 "unconnected-(J3-P1-Pad1)")
  (net 57 "unconnected-(J3-P2-Pad2)")
  (net 58 "unconnected-(J3-P3-Pad3)")
  (net 59 "unconnected-(J3-P4-Pad4)")
  (net 60 "unconnected-(J3-P5-Pad5)")
  (net 61 "unconnected-(J3-P6-Pad6)")
  (net 62 "unconnected-(J3-P7-Pad7)")
  (net 63 "unconnected-(J3-P8-Pad8)")
  (net 64 "unconnected-(J3-Pad9)")
  (net 65 "unconnected-(J3-Pad10)")
  (net 66 "unconnected-(J3-Pad11)")
  (net 67 "unconnected-(J3-Pad12)")
  (net 68 "unconnected-(J3-SHIELD-PadS1)")
  (net 69 "unconnected-(J3-SHIELD__1-PadS2)")
  (net 70 "unconnected-(J4-GND-PadA1)")
  (net 71 "unconnected-(J4-VBUS-PadA4)")
  (net 72 "unconnected-(J4-CC1-PadA5)")
  (net 73 "unconnected-(J4-DP1-PadA6)")
  (net 74 "unconnected-(J4-DN1-PadA7)")
  (net 75 "unconnected-(J4-SBU1-PadA8)")
  (net 76 "unconnected-(J4-VBUS__1-PadA9)")
  (net 77 "unconnected-(J4-GND__1-PadA12)")
  (net 78 "unconnected-(J4-GND__2-PadB1)")
  (net 79 "unconnected-(J4-VBUS__2-PadB4)")
  (net 80 "unconnected-(J4-CC2-PadB5)")
  (net 81 "unconnected-(J4-DP2-PadB6)")
  (net 82 "unconnected-(J4-DN2-PadB7)")
  (net 83 "unconnected-(J4-SBU2-PadB8)")
  (net 84 "unconnected-(J4-VBUS__3-PadB9)")
  (net 85 "unconnected-(J4-GND__3-PadB12)")
  (net 86 "unconnected-(J4-SHELL-PadS1)")
  (net 87 "unconnected-(J4-SHELL__1-PadS2)")
  (net 88 "unconnected-(J4-SHELL__2-PadS3)")
  (net 89 "unconnected-(J4-SHELL__3-PadS4)")
  (net 90 "unconnected-(J5-VBUS1-Pad1)")
  (net 91 "unconnected-(J5-D1--Pad2)")
  (net 92 "unconnected-(J5-D1+-Pad3)")
  (net 93 "unconnected-(J5-GND1-Pad4)")
  (net 94 "unconnected-(J5-VBUS2-Pad5)")
  (net 95 "unconnected-(J5-D2--Pad6)")
  (net 96 "unconnected-(J5-D2+-Pad7)")
  (net 97 "unconnected-(J5-GND2-Pad8)")
  (net 98 "unconnected-(J5-Shield-Pad9)")
  (net 99 "unconnected-(J6-VBUS1-Pad1)")
  (net 100 "unconnected-(J6-D1--Pad2)")
  (net 101 "unconnected-(J6-D1+-Pad3)")
  (net 102 "unconnected-(J6-GND1-Pad4)")
  (net 103 "unconnected-(J6-VBUS2-Pad5)")
  (net 104 "unconnected-(J6-D2--Pad6)")
  (net 105 "unconnected-(J6-D2+-Pad7)")
  (net 106 "unconnected-(J6-GND2-Pad8)")
  (net 107 "unconnected-(J6-Shield-Pad9)")
  (net 108 "unconnected-(SW1-Pad1)")
  (net 109 "unconnected-(SW1-Pad2)")
  (net 110 "unconnected-(SW1-Pad3)")
  (net 111 "unconnected-(SW1-Pad4)")
  (net 112 "unconnected-(SW1-Pad5)")
  (net 113 "unconnected-(SW1-Pad6)")
  (net 114 "unconnected-(SW1-Pad7)")
  (net 115 "unconnected-(SW1-Pad8)")
  (net 116 "unconnected-(SW1-Pad9)")
  (net 117 "unconnected-(SW1-Pad10)")
  (net 118 "unconnected-(SW1-Pad11)")
  (net 119 "unconnected-(SW1-Pad12)")
  (net 120 "unconnected-(SW1-Pad13)")
  (net 121 "unconnected-(SW1-Pad14)")
  (net 122 "unconnected-(SW1-Pad15)")
  (net 123 "unconnected-(SW1-Pad16)")
  (net 124 "unconnected-(SW2-Pad1)")
  (net 125 "unconnected-(SW2-Pad2)")
  (net 126 "unconnected-(SW3-Pad1)")
  (net 127 "unconnected-(SW3-Pad2)")
  (net 128 "unconnected-(U1A-GND-PadA1)")
  (net 129 "unconnected-(U1H-GPIOT_RXN13-PadA2)")
  (net 130 "unconnected-(U1H-GPIOT_RXP13-PadA3)")
  (net 131 "unconnected-(U1G-GPIOT_RXN05-PadA4)")
  (net 132 "unconnected-(U1G-GPIOT_RXP05-PadA5)")
  (net 133 "unconnected-(U1G-GPIOT_RXN06-PadA6)")
  (net 134 "unconnected-(U1G-GPIOT_RXP06-PadA7)")
  (net 135 "unconnected-(U1G-GPIOT_RXP03-PadA8)")
  (net 136 "unconnected-(U1G-GPIOT_RXP02-PadA9)")
  (net 137 "unconnected-(U1G-GPIOT_RXN02-PadA10)")
  (net 138 "unconnected-(U1F-GPIOL_108_CBSEL0-PadA11)")
  (net 139 "unconnected-(U1F-GPIOL_109_CBSEL1-PadA12)")
  (net 140 "unconnected-(U1F-GPIOL_106-PadA13)")
  (net 141 "unconnected-(U1F-GPIOL_107-PadA14)")
  (net 142 "unconnected-(U1F-GPIOL_105-PadA15)")
  (net 143 "unconnected-(U1F-GPIOL_97-PadA16)")
  (net 144 "unconnected-(U1E-GPIOL_90-PadA17)")
  (net 145 "unconnected-(U1E-GPIOL_88-PadA18)")
  (net 146 "unconnected-(U1E-GPIOL_86-PadA19)")
  (net 147 "unconnected-(U1A-GND-PadA20)")
  (net 148 "unconnected-(U1H-GPIOT_RXN16_EXTFB1-PadB1)")
  (net 149 "unconnected-(U1H-GPIOT_RXP16_EXTFB1-PadB2)")
  (net 150 "unconnected-(U1H-GPIOT_RXN15-PadB3)")
  (net 151 "unconnected-(U1A-GND-PadB4)")
  (net 152 "unconnected-(U1G-GPIOT_RXN08_CLKN0-PadB5)")
  (net 153 "unconnected-(U1G-GPIOT_RXP08_CLKP0-PadB6)")
  (net 154 "unconnected-(U1G-VCCIO2A-PadB7)")
  (net 155 "unconnected-(U1G-GPIOT_RXN03-PadB8)")
  (net 156 "unconnected-(U1G-GPIOT_RXP04-PadB9)")
  (net 157 "unconnected-(U1G-VCCIO2A-PadB10)")
  (net 158 "unconnected-(U1G-GPIOT_RXP00-PadB11)")
  (net 159 "unconnected-(U1F-VCCIO1E-PadB12)")
  (net 160 "unconnected-(U1F-GPIOL_112-PadB13)")
  (net 161 "unconnected-(U1F-VCCIO1E-PadB14)")
  (net 162 "unconnected-(U1F-GPIOL_96-PadB15)")
  (net 163 "unconnected-(U1E-GPIOL_87-PadB16)")
  (net 164 "unconnected-(U1E-VCCIO1D-PadB17)")
  (net 165 "unconnected-(U1E-GPIOL_73_CLK7-PadB18)")
  (net 166 "unconnected-(U1E-GPIOL_77_CTRL7-PadB19)")
  (net 167 "unconnected-(U1E-GPIOL_71_CLK5-PadB20)")
  (net 168 "unconnected-(U1I-GPIOT_RXN18-PadC1)")
  (net 169 "unconnected-(U1H-VCCIO2B-PadC2)")
  (net 170 "unconnected-(U1H-GPIOT_RXP15-PadC3)")
  (net 171 "unconnected-(U1H-GPIOT_RXP14-PadC4)")
  (net 172 "unconnected-(U1H-GPIOT_RXN14-PadC5)")
  (net 173 "unconnected-(U1H-GPIOT_RXP10-PadC6)")
  (net 174 "unconnected-(U1H-GPIOT_RXN10-PadC7)")
  (net 175 "unconnected-(U1H-VCCIO2B-PadC8)")
  (net 176 "unconnected-(U1G-GPIOT_RXN04-PadC9)")
  (net 177 "unconnected-(U1G-GPIOT_RXP01-PadC10)")
  (net 178 "unconnected-(U1G-GPIOT_RXN00-PadC11)")
  (net 179 "unconnected-(U1F-GPIOL_111-PadC12)")
  (net 180 "unconnected-(U1F-GPIOL_110-PadC13)")
  (net 181 "unconnected-(U1F-GPIOL_102_NSTATUS-PadC14)")
  (net 182 "unconnected-(U1F-GPIOL_94-PadC15)")
  (net 183 "unconnected-(U1E-GPIOL_93-PadC16)")
  (net 184 "unconnected-(U1E-GPIOL_84-PadC17)")
  (net 185 "unconnected-(U1E-GPIOL_76_CTRL6-PadC18)")
  (net 186 "unconnected-(U1E-VCCIO1D-PadC19)")
  (net 187 "unconnected-(U1E-GPIOL_74_CTRL4-PadC20)")
  (net 188 "unconnected-(U1I-GPIOT_RXP18-PadD1)")
  (net 189 "unconnected-(U1I-GPIOT_RXN21-PadD2)")
  (net 190 "unconnected-(U1H-GPIOT_RXN17_CLKN1-PadD3)")
  (net 191 "unconnected-(U1H-GPIOT_RXP17_CLKP1-PadD4)")
  (net 192 "unconnected-(U1H-GPIOT_RXN11-PadD5)")
  (net 193 "unconnected-(U1H-GPIOT_RXP11-PadD6)")
  (net 194 "unconnected-(U1H-GPIOT_RX09-PadD7)")
  (net 195 "unconnected-(U1H-GPIOT_RXP09-PadD8)")
  (net 196 "unconnected-(U1H-GPIOT_RXP12-PadD9)")
  (net 197 "unconnected-(U1G-GPIOT_RXN01-PadD10)")
  (net 198 "unconnected-(U1A-GND-PadD11)")
  (net 199 "unconnected-(U1F-GPIOL_113-PadD12)")
  (net 200 "unconnected-(U1F-GPIOL_114-PadD13)")
  (net 201 "unconnected-(U1F-GPIOL_100-PadD14)")
  (net 202 "unconnected-(U1F-GPIOL_95-PadD15)")
  (net 203 "unconnected-(U1E-GPIOL_92-PadD16)")
  (net 204 "unconnected-(U1E-GPIOL_79-PadD17)")
  (net 205 "unconnected-(U1E-GPIOL_72_CLK6-PadD18)")
  (net 206 "unconnected-(U1D-GPIOL_63_CTRL1-PadD19)")
  (net 207 "unconnected-(U1D-GPIOL_66_CLK0-PadD20)")
  (net 208 "unconnected-(U1I-GPIOT_RXP23-PadE1)")
  (net 209 "unconnected-(U1I-GPIOT_RXP21-PadE2)")
  (net 210 "unconnected-(U1I-GPIOT_RXN20-PadE3)")
  (net 211 "unconnected-(U1I-GPIOT_RXP20-PadE4)")
  (net 212 "unconnected-(U1I-VCCIO2C-PadE5)")
  (net 213 "unconnected-(U1I-GPIOT_RXP19-PadE6)")
  (net 214 "unconnected-(U1I-GPIOT_RXN19-PadE7)")
  (net 215 "unconnected-(U1A-GND-PadE8)")
  (net 216 "unconnected-(U1H-GPIOT_RXN12-PadE9)")
  (net 217 "unconnected-(U1G-GPIOT_RXP07_EXTFB0-PadE10)")
  (net 218 "unconnected-(U1G-GPIOT_RXN07_EXTFB0-PadE11)")
  (net 219 "unconnected-(U1F-GPIOL_116-PadE12)")
  (net 220 "unconnected-(U1F-VCCIO1E-PadE13)")
  (net 221 "unconnected-(U1F-GPIOL_104-PadE14)")
  (net 222 "unconnected-(U1F-GPIOL_99-PadE15)")
  (net 223 "unconnected-(U1E-VCCIO1D-PadE16)")
  (net 224 "unconnected-(U1E-GPIOL_75_CTRL5-PadE17)")
  (net 225 "unconnected-(U1D-GPIOL_68_CLK2-PadE18)")
  (net 226 "unconnected-(U1D-VCCIO1C-PadE19)")
  (net 227 "unconnected-(U1D-GPIOL_67_CLK1-PadE20)")
  (net 228 "unconnected-(U1I-GPIOT_RXN23-PadF1)")
  (net 229 "unconnected-(U1I-VCCIO2C-PadF2)")
  (net 230 "unconnected-(U1I-GPIOT_RXN22-PadF3)")
  (net 231 "unconnected-(U1I-GPIOT_RXP24_EXTFB2-PadF4)")
  (net 232 "unconnected-(U1I-GPIOT_RXN24_EXTFB2-PadF5)")
  (net 233 "unconnected-(U1J-GPIOR_121_MREFCLK-PadF6)")
  (net 234 "unconnected-(U1J-GPIOR_118_PLLIN0-PadF7)")
  (net 235 "unconnected-(U1P-VCCA_TR-PadF8)")
  (net 236 "unconnected-(U1I-VCCIO2C-PadF9)")
  (net 237 "unconnected-(U1H-VCCIO2B-PadF10)")
  (net 238 "unconnected-(U1G-VCCIO2A-PadF11)")
  (net 239 "unconnected-(U1F-GPIOL_115-PadF12)")
  (net 240 "unconnected-(U1F-GPIOL_117-PadF13)")
  (net 241 "unconnected-(U1F-GPIOL_103_TEST_N-PadF14)")
  (net 242 "unconnected-(U1F-GPIOL_98-PadF15)")
  (net 243 "unconnected-(U1E-GPIOL_85-PadF16)")
  (net 244 "unconnected-(U1E-GPIOL_82-PadF17)")
  (net 245 "unconnected-(U1D-GPIOL_69_CLK3-PadF18)")
  (net 246 "unconnected-(U1D-GPIOL_64_CTRL2-PadF19)")
  (net 247 "unconnected-(U1D-GPIOL_58-PadF20)")
  (net 248 "unconnected-(U1I-GPIOT_RXN25_CLKIN2-PadG1)")
  (net 249 "unconnected-(U1I-GPIOT_RXP25_CLKP2-PadG2)")
  (net 250 "unconnected-(U1I-GPIOT_RXP22-PadG3)")
  (net 251 "unconnected-(U1J-GPIOR_127_CLK14-PadG4)")
  (net 252 "unconnected-(U1J-GPIOR_123_CTRL14-PadG5)")
  (net 253 "unconnected-(U1J-GPIOR_119_PLLIN1-PadG6)")
  (net 254 "unconnected-(U1J-GPIOR_120_PLLIN2-PadG7)")
  (net 255 "unconnected-(U1A-GND-PadG8)")
  (net 256 "unconnected-(U1A-GND-PadG9)")
  (net 257 "unconnected-(U1A-GND-PadG10)")
  (net 258 "unconnected-(U1A-GND-PadG11)")
  (net 259 "unconnected-(U1A-GND-PadG12)")
  (net 260 "unconnected-(U1A-GND-PadG13)")
  (net 261 "unconnected-(U1F-GPIOL_101-PadG14)")
  (net 262 "unconnected-(U1E-GPIOL_91-PadG15)")
  (net 263 "unconnected-(U1E-GPIOL_89-PadG16)")
  (net 264 "unconnected-(U1E-GPIOL_70_CLK4-PadG17)")
  (net 265 "unconnected-(U1D-GPIOL_65_CTRL3-PadG18)")
  (net 266 "unconnected-(U1A-GND-PadG19)")
  (net 267 "unconnected-(U1D-GPIOL_56-PadG20)")
  (net 268 "unconnected-(U1J-GPIOR_130_CLK11-PadH1)")
  (net 269 "unconnected-(U1J-GPIOR_131_CLK10-PadH2)")
  (net 270 "unconnected-(U1J-GPIOR_124_CTRL13-PadH3)")
  (net 271 "unconnected-(U1J-GPIOR_125_CTRL12-PadH4)")
  (net 272 "unconnected-(U1J-VCCIO3C_TR-PadH5)")
  (net 273 "unconnected-(U1J-GPIOR_122_CTRL15-PadH6)")
  (net 274 "unconnected-(U1J-GPIOR_126_CLK15-PadH7)")
  (net 275 "unconnected-(U1O-VCC-PadH8)")
  (net 276 "unconnected-(U1O-VCC-PadH9)")
  (net 277 "unconnected-(U1O-VCC-PadH10)")
  (net 278 "unconnected-(U1O-VCC-PadH11)")
  (net 279 "unconnected-(U1O-VCC-PadH12)")
  (net 280 "unconnected-(U1O-VCC-PadH13)")
  (net 281 "unconnected-(U1E-GPIOL_83-PadH14)")
  (net 282 "unconnected-(U1E-GPIOL_81-PadH15)")
  (net 283 "unconnected-(U1D-VCCIO1C-PadH16)")
  (net 284 "unconnected-(U1D-GPIOL_60-PadH17)")
  (net 285 "unconnected-(U1D-GPIOL_62_CTRL0-PadH18)")
  (net 286 "unconnected-(U1D-GPIOL_54-PadH19)")
  (net 287 "unconnected-(U1D-GPIOL_53-PadH20)")
  (net 288 "unconnected-(U1J-GPIOR_134_CTRL11-PadJ1)")
  (net 289 "unconnected-(U1A-GND-PadJ2)")
  (net 290 "unconnected-(U1J-GPIOR_135_CTRL10-PadJ3)")
  (net 291 "unconnected-(U1J-GPIOR_132_CLK9-PadJ4)")
  (net 292 "unconnected-(U1J-GPIOR_133_CLK8-PadJ5)")
  (net 293 "unconnected-(U1J-GPIOR_129_CLK12-PadJ6)")
  (net 294 "unconnected-(U1J-VCCIO3C_TR-PadJ7)")
  (net 295 "unconnected-(U1A-GND-PadJ8)")
  (net 296 "unconnected-(U1A-GND-PadJ9)")
  (net 297 "unconnected-(U1A-GND-PadJ10)")
  (net 298 "unconnected-(U1A-GND-PadJ11)")
  (net 299 "unconnected-(U1A-GND-PadJ12)")
  (net 300 "unconnected-(U1A-GND-PadJ13)")
  (net 301 "unconnected-(U1D-GPIOL_59-PadJ14)")
  (net 302 "unconnected-(U1D-GPIOL_57-PadJ15)")
  (net 303 "unconnected-(U1D-GPIOL_51-PadJ16)")
  (net 304 "unconnected-(U1D-GPIOL_52-PadJ17)")
  (net 305 "unconnected-(U1D-GPIOL_47-PadJ18)")
  (net 306 "unconnected-(U1D-VCCIO1C-PadJ19)")
  (net 307 "unconnected-(U1D-GPIOL_50-PadJ20)")
  (net 308 "unconnected-(U1K-DDR_BA2-PadK1)")
  (net 309 "unconnected-(U1K-DDR_BA2-PadK2)")
  (net 310 "unconnected-(U1K-DDR_BA0-PadK3)")
  (net 311 "unconnected-(U1K-DDR_WE_N-PadK4)")
  (net 312 "unconnected-(U1J-GPIOR_128_CLK13-PadK5)")
  (net 313 "unconnected-(U1J-GPIOR_136_CTRL9-PadK6)")
  (net 314 "unconnected-(U1J-GPIOR_137_CTRL8-PadK7)")
  (net 315 "unconnected-(U1O-VCC-PadK8)")
  (net 316 "unconnected-(U1O-VCC-PadK9)")
  (net 317 "unconnected-(U1O-VCC-PadK10)")
  (net 318 "unconnected-(U1O-VCC-PadK11)")
  (net 319 "unconnected-(U1O-VCC-PadK12)")
  (net 320 "unconnected-(U1O-VCC-PadK13)")
  (net 321 "unconnected-(U1D-GPIOL_49-PadK14)")
  (net 322 "unconnected-(U1C-GPIOL_45-PadK15)")
  (net 323 "unconnected-(U1C-GPIOL_44-PadK16)")
  (net 324 "unconnected-(U1C-GPIOL_43-PadK17)")
  (net 325 "unconnected-(U1C-GPIOL_42-PadK18)")
  (net 326 "unconnected-(U1D-GPIOL_46-PadK19)")
  (net 327 "unconnected-(U1D-GPIOL_48-PadK20)")
  (net 328 "unconnected-(U1K-DDR_DQ14-PadL1)")
  (net 329 "unconnected-(U1K-DDR_DQ13-PadL2)")
  (net 330 "unconnected-(U1K-DDR_DQ12-PadL3)")
  (net 331 "unconnected-(U1K-DDR_RST_N-PadL4)")
  (net 332 "unconnected-(U1A-GND-PadL5)")
  (net 333 "unconnected-(U1K-DDR_ODT-PadL6)")
  (net 334 "unconnected-(U1K-VCCIO_DDR-PadL7)")
  (net 335 "unconnected-(U1A-GND-PadL8)")
  (net 336 "unconnected-(U1A-GND-PadL9)")
  (net 337 "unconnected-(U1A-GND-PadL10)")
  (net 338 "unconnected-(U1A-GND-PadL11)")
  (net 339 "unconnected-(U1A-GND-PadL12)")
  (net 340 "unconnected-(U1A-GND-PadL13)")
  (net 341 "unconnected-(U1C-GPIOL_41-PadL14)")
  (net 342 "unconnected-(U1C-GPIOL_37-PadL15)")
  (net 343 "unconnected-(U1C-VCCIO1B-PadL16)")
  (net 344 "unconnected-(U1C-GPIOL_36-PadL17)")
  (net 345 "unconnected-(U1C-GPIOL_40-PadL18)")
  (net 346 "unconnected-(U1C-VCCIO1B-PadL19)")
  (net 347 "unconnected-(U1C-GPIOL_39-PadL20)")
  (net 348 "unconnected-(U1K-DDR_DQ15-PadM1)")
  (net 349 "unconnected-(U1A-GND-PadM2)")
  (net 350 "unconnected-(U1K-DDR_DQS_N1-PadM3)")
  (net 351 "unconnected-(U1K-DDR_RAS_N-PadM4)")
  (net 352 "unconnected-(U1K-DDR_A15-PadM5)")
  (net 353 "unconnected-(U1K-DDR_A13-PadM6)")
  (net 354 "unconnected-(U1A-GND-PadM7)")
  (net 355 "unconnected-(U1O-VCC-PadM8)")
  (net 356 "unconnected-(U1O-VCC-PadM9)")
  (net 357 "unconnected-(U1O-VCC-PadM10)")
  (net 358 "unconnected-(U1O-VCC-PadM11)")
  (net 359 "unconnected-(U1O-VCC-PadM12)")
  (net 360 "unconnected-(U1O-VCC-PadM13)")
  (net 361 "unconnected-(U1C-GPIOL_21-PadM14)")
  (net 362 "unconnected-(U1C-GPIOL_31-PadM15)")
  (net 363 "unconnected-(U1C-GPIOL_34-PadM16)")
  (net 364 "unconnected-(U1C-GPIOL_32-PadM17)")
  (net 365 "unconnected-(U1C-GPIOL_33-PadM18)")
  (net 366 "unconnected-(U1C-GPIOL_38-PadM19)")
  (net 367 "unconnected-(U1C-GPIOL_35-PadM20)")
  (net 368 "unconnected-(U1K-DDR_DM1-PadN1)")
  (net 369 "unconnected-(U1K-DDR_DQ11-PadN2)")
  (net 370 "unconnected-(U1K-DDR_DQS1-PadN3)")
  (net 371 "unconnected-(U1K-DDR_A14-PadN4)")
  (net 372 "unconnected-(U1K-DDR_A11-PadN5)")
  (net 373 "unconnected-(U1K-DDR_CKE-PadN6)")
  (net 374 "unconnected-(U1K-VCCIO_DDR-PadN7)")
  (net 375 "unconnected-(U1A-GND-PadN8)")
  (net 376 "unconnected-(U1A-GND-PadN9)")
  (net 377 "unconnected-(U1A-GND-PadN10)")
  (net 378 "unconnected-(U1A-GND-PadN11)")
  (net 379 "unconnected-(U1A-GND-PadN12)")
  (net 380 "unconnected-(U1A-GND-PadN13)")
  (net 381 "unconnected-(U1C-GPIOL_17_EXTFB0-PadN14)")
  (net 382 "unconnected-(U1C-GPIOL_20_CDI5-PadN15)")
  (net 383 "unconnected-(U1C-GPIOL_27-PadN16)")
  (net 384 "unconnected-(U1C-GPIOL_30-PadN17)")
  (net 385 "unconnected-(U1C-GPIOL_28-PadN18)")
  (net 386 "unconnected-(U1C-VCCIO1B-PadN19)")
  (net 387 "unconnected-(U1C-GPIOL_29-PadN20)")
  (net 388 "unconnected-(U1K-DDR_DQ8-PadP1)")
  (net 389 "unconnected-(U1K-DDR_DQ9-PadP2)")
  (net 390 "unconnected-(U1K-DDR_D10-PadP3)")
  (net 391 "unconnected-(U1K-DDR_A12-PadP4)")
  (net 392 "unconnected-(U1K-VCCIO_DDR-PadP5)")
  (net 393 "unconnected-(U1K-DDR_CAS_N-PadP6)")
  (net 394 "unconnected-(U1A-GND-PadP7)")
  (net 395 "unconnected-(U1O-VCC-PadP8)")
  (net 396 "unconnected-(U1O-VCC-PadP9)")
  (net 397 "unconnected-(U1O-VCC-PadP10)")
  (net 398 "unconnected-(U1O-VCC-PadP11)")
  (net 399 "unconnected-(U1O-VCC-PadP12)")
  (net 400 "unconnected-(U1O-VCC-PadP13)")
  (net 401 "unconnected-(U1B-GPIOL_10-PadP14)")
  (net 402 "unconnected-(U1C-GPIOL_14_CDI2-PadP15)")
  (net 403 "unconnected-(U1C-GPIOL_19_PLLIN1-PadP16)")
  (net 404 "unconnected-(U1A-GND-PadP17)")
  (net 405 "unconnected-(U1C-GPIOL_22_CDI6-PadP18)")
  (net 406 "unconnected-(U1C-GPIOL_26-PadP19)")
  (net 407 "unconnected-(U1C-GPIOL_25-PadP20)")
  (net 408 "unconnected-(U1K-DDR_A8-PadR1)")
  (net 409 "unconnected-(U1K-VCCIO_DDR-PadR2)")
  (net 410 "unconnected-(U1K-DDR_CK-PadR3)")
  (net 411 "unconnected-(U1K-DDR_CK_N-PadR4)")
  (net 412 "unconnected-(U1K-DDR_A10-PadR5)")
  (net 413 "unconnected-(U1K-DDR_CS_N-PadR6)")
  (net 414 "unconnected-(U1K-VCCIO_DDR-PadR7)")
  (net 415 "unconnected-(U1P-VCCA_BR-PadR8)")
  (net 416 "unconnected-(U1N-VCCIO_BR-PadR9)")
  (net 417 "unconnected-(U1L-REF_RES_4A-PadR10)")
  (net 418 "unconnected-(U1A-GND-PadR11)")
  (net 419 "unconnected-(U1M-REF_RES_4B-PadR12)")
  (net 420 "unconnected-(U1P-VCCA_BL-PadR13)")
  (net 421 "unconnected-(U1B-GPIOL_03-PadR14)")
  (net 422 "unconnected-(U1B-VCCIO1A-PadR15)")
  (net 423 "unconnected-(U1C-GPIOL_15_PLLIN0-PadR16)")
  (net 424 "unconnected-(U1C-GPIOL_16_CDI3-PadR17)")
  (net 425 "unconnected-(U1C-GPIOL_18_CDI4-PadR18)")
  (net 426 "unconnected-(U1A-GND-PadR19)")
  (net 427 "unconnected-(U1C-GPIOL_23-PadR20)")
  (net 428 "unconnected-(U1K-DDR_A7-PadT1)")
  (net 429 "unconnected-(U1K-DDR_A9-PadT2)")
  (net 430 "unconnected-(U1K-DDR_A4-PadT3)")
  (net 431 "unconnected-(U1K-DDR_A6-PadT4)")
  (net 432 "unconnected-(U1K-DDR_A5-PadT5)")
  (net 433 "unconnected-(U1K-DDR_A3-PadT6)")
  (net 434 "unconnected-(U1N-GPIOR_141-PadT7)")
  (net 435 "unconnected-(U1N-GPIOR_138_PLLIN0-PadT8)")
  (net 436 "unconnected-(U1N-GPIOR_139_PLLIN1-PadT9)")
  (net 437 "unconnected-(U1L-GPIOB_TXN10-PadT10)")
  (net 438 "unconnected-(U1L-GPIOB_TXP10-PadT11)")
  (net 439 "unconnected-(U1M-GPIOB_TXN05_CDI26-PadT12)")
  (net 440 "unconnected-(U1M-GPIOB_TXP05_CDI27-PadT13)")
  (net 441 "unconnected-(U1M-VCCIO4B-PadT14)")
  (net 442 "unconnected-(U1B-GPIOL_02-PadT15)")
  (net 443 "unconnected-(U1B-GPIOL_04_CSI-PadT16)")
  (net 444 "unconnected-(U1B-GPIOL_05_CSO-PadT17)")
  (net 445 "unconnected-(U1B-GPIOL_12_CBUS1-PadT18)")
  (net 446 "unconnected-(U1B-CDONE-PadT19)")
  (net 447 "unconnected-(U1C-GPIOL_24_CDI7-PadT20)")
  (net 448 "unconnected-(U1K-DDR_DQS_N0-PadU1)")
  (net 449 "unconnected-(U1K-DDR_DQ3-PadU2)")
  (net 450 "unconnected-(U1K-DDR_DQ0-PadU3)")
  (net 451 "unconnected-(U1K-DDR_A0-PadU4)")
  (net 452 "unconnected-(U1A-GND-PadU5)")
  (net 453 "unconnected-(U1L-GPIOB_TXN17_CDI10-PadU6)")
  (net 454 "unconnected-(U1L-GPIOB_TXP17_CDI11-PadU7)")
  (net 455 "unconnected-(U1A-GND-PadU8)")
  (net 456 "unconnected-(U1N-GPIOR_139_PLLIN2-PadU9)")
  (net 457 "unconnected-(U1L-GPIOB_TXN15_CDI14-PadU10)")
  (net 458 "unconnected-(U1L-VCCIO4A-PadU11)")
  (net 459 "unconnected-(U1M-GPIOB_TXN06_CDI24-PadU12)")
  (net 460 "unconnected-(U1M-GPIOB_TXP07_CDI23-PadU13)")
  (net 461 "unconnected-(U1M-GPIOB_TXP02-PadU14)")
  (net 462 "unconnected-(U1M-GPIOB_TXN00-PadU15)")
  (net 463 "unconnected-(U1A-GND-PadU16)")
  (net 464 "unconnected-(U1B-GPIOL_06-PadU17)")
  (net 465 "unconnected-(U1B-GPIOL_11_CBUS0-PadU18)")
  (net 466 "unconnected-(U1B-~{CRESET_N}-PadU19)")
  (net 467 "unconnected-(U1B-TMS-PadU20)")
  (net 468 "unconnected-(U1K-DDR_DQS0-PadV1)")
  (net 469 "unconnected-(U1A-GND-PadV2)")
  (net 470 "unconnected-(U1K-DDR_DQ2-PadV3)")
  (net 471 "unconnected-(U1K-DDR_VREF-PadV4)")
  (net 472 "unconnected-(U1K-DDR_A2-PadV5)")
  (net 473 "unconnected-(U1L-GPIOB_TXP18_EXTFB_CDI9-PadV6)")
  (net 474 "unconnected-(U1L-GPIOB_TXN18_CDI8-PadV7)")
  (net 475 "unconnected-(U1L-GPIOB_TXN19-PadV8)")
  (net 476 "unconnected-(U1L-GPIOB_TXP19_CLK2-PadV9)")
  (net 477 "unconnected-(U1L-GPIOB_TXP15_CLK1_CDI15-PadV10)")
  (net 478 "unconnected-(U1L-GPIOB_TXN11-PadV11)")
  (net 479 "unconnected-(U1M-GPIOB_TXP06_CDI25-PadV12)")
  (net 480 "unconnected-(U1M-GPIOB_TXN07_CDI22-PadV13)")
  (net 481 "unconnected-(U1M-GPIOB_TXN02-PadV14)")
  (net 482 "unconnected-(U1M-GPIOB_TXP00-PadV15)")
  (net 483 "unconnected-(U1M-GPIOB_TXN03_CDI30-PadV16)")
  (net 484 "unconnected-(U1B-GPIOL_07-PadV17)")
  (net 485 "unconnected-(U1B-GPIOL_13_CBUS2-PadV18)")
  (net 486 "unconnected-(U1B-VCCIO1A-PadV19)")
  (net 487 "unconnected-(U1B-TDO-PadV20)")
  (net 488 "unconnected-(U1K-DDR_DM0-PadW1)")
  (net 489 "unconnected-(U1K-DDR_DQ4-PadW2)")
  (net 490 "unconnected-(U1K-DDR_DQ1-PadW3)")
  (net 491 "unconnected-(U1K-VCCIO_DDR-PadW4)")
  (net 492 "unconnected-(U1K-DDR_A1-PadW5)")
  (net 493 "unconnected-(U1L-GPIOB_TXN14_CDI16-PadW6)")
  (net 494 "unconnected-(U1L-VCCIO4A-PadW7)")
  (net 495 "unconnected-(U1L-GPIOB_TXN16_CDI12-PadW8)")
  (net 496 "unconnected-(U1L-GPIOB_TXP16_CDI13-PadW9)")
  (net 497 "unconnected-(U1L-VCCIO4A-PadW10)")
  (net 498 "unconnected-(U1L-GPIOB_TXP11-PadW11)")
  (net 499 "unconnected-(U1M-VCCIO4B-PadW12)")
  (net 500 "unconnected-(U1M-GPIOB_TXN08_CDI20-PadW13)")
  (net 501 "unconnected-(U1M-GPIOB_TXN04_CDI28-PadW14)")
  (net 502 "unconnected-(U1M-VCCIO4B-PadW15)")
  (net 503 "unconnected-(U1M-GPIOB_TXP03_CDI31-PadW16)")
  (net 504 "unconnected-(U1A-VND-PadW17)")
  (net 505 "unconnected-(U1B-GPIOL_00_SS_N-PadW18)")
  (net 506 "unconnected-(U1B-GPIOL_01_CCK-PadW19)")
  (net 507 "unconnected-(U1B-TCK-PadW20)")
  (net 508 "unconnected-(U1A-GND-PadY1)")
  (net 509 "unconnected-(U1K-DDR_DQ7-PadY2)")
  (net 510 "unconnected-(U1K-DDR_DQ5-PadY3)")
  (net 511 "unconnected-(U1K-DDR_DQ6-PadY4)")
  (net 512 "unconnected-(U1K-DDR_ZQ-PadY5)")
  (net 513 "unconnected-(U1L-GPIOB_TXP14_EXTFB1_CDI17-PadY6)")
  (net 514 "unconnected-(U1L-GPIOB_TXP13_CDI19-PadY7)")
  (net 515 "unconnected-(U1L-GPIOB_TXN13_CDI18-PadY8)")
  (net 516 "unconnected-(U1L-GPIOB_TXN12-PadY9)")
  (net 517 "unconnected-(U1L-GPIOB_TXP12-PadY10)")
  (net 518 "unconnected-(U1M-GPIOB_TXP09_CLK0-PadY11)")
  (net 519 "unconnected-(U1M-GPIOB_TXN09-PadY12)")
  (net 520 "unconnected-(U1M-GPIOB_TXP08_EXTFB0_CDI21-PadY13)")
  (net 521 "unconnected-(U1M-GPIOB_TXP04_CDI29-PadY14)")
  (net 522 "unconnected-(U1M-GPIOB_TXN01-PadY15)")
  (net 523 "unconnected-(U1M-GPIOB_TXP01-PadY16)")
  (net 524 "unconnected-(U1B-GPIOL_08_CDI0-PadY17)")
  (net 525 "unconnected-(U1B-GPIOL_09_CDI1-PadY18)")
  (net 526 "unconnected-(U1B-TDI-PadY19)")
  (net 527 "unconnected-(U1A-GND-PadY20)")
  (net 528 "unconnected-(U2-SW-Pad1)")
  (net 529 "unconnected-(U2-PGND-Pad2)")
  (net 530 "unconnected-(U2-VINA-Pad3)")
  (net 531 "unconnected-(U2-EN-Pad4)")
  (net 532 "unconnected-(U2-FB-Pad5)")
  (net 533 "unconnected-(U2-AGND-Pad6)")
  (net 534 "unconnected-(U2-GND-Pad7)")
  (net 535 "unconnected-(U2-VINSW-Pad8)")
  (net 536 "unconnected-(U3-SW-Pad1)")
  (net 537 "unconnected-(U3-PGND-Pad2)")
  (net 538 "unconnected-(U3-VINA-Pad3)")
  (net 539 "unconnected-(U3-EN-Pad4)")
  (net 540 "unconnected-(U3-FB-Pad5)")
  (net 541 "unconnected-(U3-AGND-Pad6)")
  (net 542 "unconnected-(U3-GND-Pad7)")
  (net 543 "unconnected-(U3-VINSW-Pad8)")
  (net 544 "unconnected-(U4-SW-Pad1)")
  (net 545 "unconnected-(U4-PGND-Pad2)")
  (net 546 "unconnected-(U4-VINA-Pad3)")
  (net 547 "unconnected-(U4-EN-Pad4)")
  (net 548 "unconnected-(U4-FB-Pad5)")
  (net 549 "unconnected-(U4-AGND-Pad6)")
  (net 550 "unconnected-(U4-GND-Pad7)")
  (net 551 "unconnected-(U4-VINSW-Pad8)")
  (net 552 "unconnected-(U5-SW-Pad1)")
  (net 553 "unconnected-(U5-PGND-Pad2)")
  (net 554 "unconnected-(U5-VINA-Pad3)")
  (net 555 "unconnected-(U5-EN-Pad4)")
  (net 556 "unconnected-(U5-FB-Pad5)")
  (net 557 "unconnected-(U5-AGND-Pad6)")
  (net 558 "unconnected-(U5-GND-Pad7)")
  (net 559 "unconnected-(U5-VINSW-Pad8)")
  (net 560 "unconnected-(U6-VIN-Pad1)")
  (net 561 "unconnected-(U6-GND-Pad2)")
  (net 562 "unconnected-(U6-EN-Pad3)")
  (net 563 "unconnected-(U6-ADJ-Pad4)")
  (net 564 "unconnected-(U6-VOUT-Pad5)")
  (net 565 "/cpu/~{CPU_VPB}")
  (net 566 "/cpu/CPU_RDY")
  (net 567 "unconnected-(U7-PHI1O-Pad3)")
  (net 568 "/cpu/~{CPU_IRQB}")
  (net 569 "/cpu/~{CPU_MLB}")
  (net 570 "/cpu/~{CPU_NMIB}")
  (net 571 "/cpu/CPU_SYNC")
  (net 572 "+3V3")
  (net 573 "/cpu/CPU_ADDR0")
  (net 574 "/cpu/CPU_ADDR1")
  (net 575 "/cpu/CPU_ADDR2")
  (net 576 "/cpu/CPU_ADDR3")
  (net 577 "/cpu/CPU_ADDR4")
  (net 578 "/cpu/CPU_ADDR5")
  (net 579 "/cpu/CPU_ADDR6")
  (net 580 "/cpu/CPU_ADDR7")
  (net 581 "/cpu/CPU_ADDR8")
  (net 582 "/cpu/CPU_ADDR9")
  (net 583 "/cpu/CPU_ADDR10")
  (net 584 "/cpu/CPU_ADDR11")
  (net 585 "GND")
  (net 586 "/cpu/CPU_ADDR12")
  (net 587 "/cpu/CPU_ADDR13")
  (net 588 "/cpu/CPU_ADDR14")
  (net 589 "/cpu/CPU_ADDR15")
  (net 590 "/cpu/CPU_DATA7")
  (net 591 "/cpu/CPU_DATA6")
  (net 592 "/cpu/CPU_DATA5")
  (net 593 "/cpu/CPU_DATA4")
  (net 594 "/cpu/CPU_DATA3")
  (net 595 "/cpu/CPU_DATA2")
  (net 596 "/cpu/CPU_DATA1")
  (net 597 "/cpu/CPU_DATA0")
  (net 598 "/cpu/~{CPU_RWB}")
  (net 599 "unconnected-(U7-NC-Pad35)")
  (net 600 "/cpu/CPU_BE")
  (net 601 "/cpu/CPU_PHI2")
  (net 602 "Net-(U7-~{SOB})")
  (net 603 "unconnected-(U7-PHI2O-Pad39)")
  (net 604 "/cpu/~{CPU_RESB}")
  (net 605 "unconnected-(U8A-VSS-PadA1)")
  (net 606 "unconnected-(U8A-VDD-PadA2)")
  (net 607 "unconnected-(U8B-NC-PadA3)")
  (net 608 "unconnected-(U8B-NF{slash}TDQS#-PadA7)")
  (net 609 "unconnected-(U8A-VSS-PadA8)")
  (net 610 "unconnected-(U8A-VDD-PadA9)")
  (net 611 "unconnected-(U8A-VSS-PadB1)")
  (net 612 "unconnected-(U8A-VSSQ-PadB2)")
  (net 613 "unconnected-(U8B-DQ0-PadB3)")
  (net 614 "unconnected-(U8B-DM{slash}TDQS-PadB7)")
  (net 615 "unconnected-(U8A-VSSQ-PadB8)")
  (net 616 "unconnected-(U8A-VDDQ-PadB9)")
  (net 617 "unconnected-(U8A-VDDQ-PadC1)")
  (net 618 "unconnected-(U8B-DQ2-PadC2)")
  (net 619 "unconnected-(U8B-DQS-PadC3)")
  (net 620 "unconnected-(U8B-DQ1-PadC7)")
  (net 621 "unconnected-(U8B-DQ3-PadC8)")
  (net 622 "unconnected-(U8A-VSSQ-PadC9)")
  (net 623 "unconnected-(U8A-VSSQ-PadD1)")
  (net 624 "unconnected-(U8B-DQ6-PadD2)")
  (net 625 "unconnected-(U8B-DQS#-PadD3)")
  (net 626 "unconnected-(U8A-VDD-PadD7)")
  (net 627 "unconnected-(U8A-VSS-PadD8)")
  (net 628 "unconnected-(U8A-VSSQ-PadD9)")
  (net 629 "unconnected-(U8A-VREFDQ-PadE1)")
  (net 630 "unconnected-(U8A-VDDQ-PadE2)")
  (net 631 "unconnected-(U8B-DQ4-PadE3)")
  (net 632 "unconnected-(U8B-DQ7-PadE7)")
  (net 633 "unconnected-(U8B-DQ5-PadE8)")
  (net 634 "unconnected-(U8A-VDDQ-PadE9)")
  (net 635 "unconnected-(U8B-NC-PadF1)")
  (net 636 "unconnected-(U8A-VSS-PadF2)")
  (net 637 "unconnected-(U8B-RAS#-PadF3)")
  (net 638 "unconnected-(U8B-CK-PadF7)")
  (net 639 "unconnected-(U8A-VSS-PadF8)")
  (net 640 "unconnected-(U8B-NC-PadF9)")
  (net 641 "unconnected-(U8B-ODT-PadG1)")
  (net 642 "unconnected-(U8A-VDD-PadG2)")
  (net 643 "unconnected-(U8B-CAS#-PadG3)")
  (net 644 "unconnected-(U8B-CK#-PadG7)")
  (net 645 "unconnected-(U8A-VDD-PadG8)")
  (net 646 "unconnected-(U8B-CKE-PadG9)")
  (net 647 "unconnected-(U8B-NC-PadH1)")
  (net 648 "unconnected-(U8B-CS#-PadH2)")
  (net 649 "unconnected-(U8B-WE#-PadH3)")
  (net 650 "unconnected-(U8B-A10{slash}AP-PadH7)")
  (net 651 "unconnected-(U8B-ZQ-PadH8)")
  (net 652 "unconnected-(U8B-NC-PadH9)")
  (net 653 "unconnected-(U8A-VSS-PadJ1)")
  (net 654 "unconnected-(U8B-BA0-PadJ2)")
  (net 655 "unconnected-(U8B-BA2-PadJ3)")
  (net 656 "unconnected-(U8B-NC-PadJ7)")
  (net 657 "unconnected-(U8A-VREFCA-PadJ8)")
  (net 658 "unconnected-(U8A-VSS-PadJ9)")
  (net 659 "unconnected-(U8A-VDD-PadK1)")
  (net 660 "unconnected-(U8B-A3-PadK2)")
  (net 661 "unconnected-(U8B-A0-PadK3)")
  (net 662 "unconnected-(U8B-A12{slash}BC#-PadK7)")
  (net 663 "unconnected-(U8B-BA1-PadK8)")
  (net 664 "unconnected-(U8A-VDD-PadK9)")
  (net 665 "unconnected-(U8A-VSS-PadL1)")
  (net 666 "unconnected-(U8B-A5-PadL2)")
  (net 667 "unconnected-(U8B-A2-PadL3)")
  (net 668 "unconnected-(U8B-A1-PadL7)")
  (net 669 "unconnected-(U8B-A4-PadL8)")
  (net 670 "unconnected-(U8A-VSS-PadL9)")
  (net 671 "unconnected-(U8A-VDD-PadM1)")
  (net 672 "unconnected-(U8B-A7-PadM2)")
  (net 673 "unconnected-(U8B-A9-PadM3)")
  (net 674 "unconnected-(U8B-A11-PadM7)")
  (net 675 "unconnected-(U8B-A6-PadM8)")
  (net 676 "unconnected-(U8A-VDD-PadM9)")
  (net 677 "unconnected-(U8A-VSS-PadN1)")
  (net 678 "unconnected-(U8B-RESET#-PadN2)")
  (net 679 "unconnected-(U8B-A13-PadN3)")
  (net 680 "unconnected-(U8B-A14-PadN7)")
  (net 681 "unconnected-(U8B-A8-PadN8)")
  (net 682 "unconnected-(U8A-VSS-PadN9)")
  (net 683 "unconnected-(U9-GND-Pad1)")
  (net 684 "unconnected-(U9-GND-Pad2)")
  (net 685 "unconnected-(U9-GND-Pad3)")
  (net 686 "unconnected-(U9-VDD_1P2-Pad4)")
  (net 687 "unconnected-(U9-NC-Pad5)")
  (net 688 "unconnected-(U9-NC-Pad6)")
  (net 689 "unconnected-(U9-VDDA_3P3-Pad7)")
  (net 690 "unconnected-(U9-NC-Pad8)")
  (net 691 "unconnected-(U9-RXM-Pad9)")
  (net 692 "unconnected-(U9-RXP-Pad10)")
  (net 693 "unconnected-(U9-TXM-Pad11)")
  (net 694 "unconnected-(U9-TXP-Pad12)")
  (net 695 "unconnected-(U9-GND-Pad13)")
  (net 696 "unconnected-(U9-XO-Pad14)")
  (net 697 "unconnected-(U9-XI-Pad15)")
  (net 698 "unconnected-(U9-REXT-Pad16)")
  (net 699 "unconnected-(U9-GND-Pad17)")
  (net 700 "unconnected-(U9-MDIO-Pad18)")
  (net 701 "unconnected-(U9-MDC-Pad19)")
  (net 702 "unconnected-(U9-RXD3_PHYAD0-Pad20)")
  (net 703 "unconnected-(U9-RXD2_PHYAD1-Pad21)")
  (net 704 "unconnected-(U9-RXD1_PHYAD2-Pad22)")
  (net 705 "unconnected-(U9-RXD0_DUPLEX-Pad23)")
  (net 706 "unconnected-(U9-GND-Pad24)")
  (net 707 "unconnected-(U9-VDDIO-Pad25)")
  (net 708 "unconnected-(U9-NC-Pad26)")
  (net 709 "unconnected-(U9-RXDV_CONFIG2-Pad27)")
  (net 710 "unconnected-(U9-RXC_B-CAST-OFF-Pad28)")
  (net 711 "unconnected-(U9-RXER_ISO-Pad29)")
  (net 712 "unconnected-(U9-GND-Pad30)")
  (net 713 "unconnected-(U9-VDD_1P2-Pad31)")
  (net 714 "unconnected-(U9-INTRP_NAND-TREE-Pad32)")
  (net 715 "unconnected-(U9-TXC-Pad33)")
  (net 716 "unconnected-(U9-TXEN-Pad34)")
  (net 717 "unconnected-(U9-TXD0-Pad35)")
  (net 718 "unconnected-(U9-TXD1-Pad36)")
  (net 719 "unconnected-(U9-GND-Pad37)")
  (net 720 "unconnected-(U9-TXD2-Pad38)")
  (net 721 "unconnected-(U9-TXD3-Pad39)")
  (net 722 "unconnected-(U9-COL_CONFIG0-Pad40)")
  (net 723 "unconnected-(U9-CRS_CONFIG1-Pad41)")
  (net 724 "unconnected-(U9-LED0_NWAYEN-Pad42)")
  (net 725 "unconnected-(U9-LED1_SPEED-Pad43)")
  (net 726 "unconnected-(U9-TEST_NC-Pad44)")
  (net 727 "unconnected-(U9-NC-Pad45)")
  (net 728 "unconnected-(U9-NC-Pad46)")
  (net 729 "unconnected-(U9-RST#-Pad47)")
  (net 730 "unconnected-(U9-NC-Pad48)")
  (net 731 "unconnected-(U10-CA-Pad1)")
  (net 732 "unconnected-(U10-F-Pad2)")
  (net 733 "unconnected-(U10-G-Pad3)")
  (net 734 "unconnected-(U10-E-Pad4)")
  (net 735 "unconnected-(U10-D-Pad5)")
  (net 736 "unconnected-(U10-CA-Pad6)")
  (net 737 "unconnected-(U10-DP-Pad7)")
  (net 738 "unconnected-(U10-C-Pad8)")
  (net 739 "unconnected-(U10-B-Pad9)")
  (net 740 "unconnected-(U10-A-Pad10)")
  (net 741 "unconnected-(U11-CA-Pad1)")
  (net 742 "unconnected-(U11-F-Pad2)")
  (net 743 "unconnected-(U11-G-Pad3)")
  (net 744 "unconnected-(U11-E-Pad4)")
  (net 745 "unconnected-(U11-D-Pad5)")
  (net 746 "unconnected-(U11-CA-Pad6)")
  (net 747 "unconnected-(U11-DP-Pad7)")
  (net 748 "unconnected-(U11-C-Pad8)")
  (net 749 "unconnected-(U11-B-Pad9)")
  (net 750 "unconnected-(U11-A-Pad10)")
  (net 751 "unconnected-(U12-CA-Pad1)")
  (net 752 "unconnected-(U12-F-Pad2)")
  (net 753 "unconnected-(U12-G-Pad3)")
  (net 754 "unconnected-(U12-E-Pad4)")
  (net 755 "unconnected-(U12-D-Pad5)")
  (net 756 "unconnected-(U12-CA-Pad6)")
  (net 757 "unconnected-(U12-DP-Pad7)")
  (net 758 "unconnected-(U12-C-Pad8)")
  (net 759 "unconnected-(U12-B-Pad9)")
  (net 760 "unconnected-(U12-A-Pad10)")
  (net 761 "unconnected-(U13-CA-Pad1)")
  (net 762 "unconnected-(U13-F-Pad2)")
  (net 763 "unconnected-(U13-G-Pad3)")
  (net 764 "unconnected-(U13-E-Pad4)")
  (net 765 "unconnected-(U13-D-Pad5)")
  (net 766 "unconnected-(U13-CA-Pad6)")
  (net 767 "unconnected-(U13-DP-Pad7)")
  (net 768 "unconnected-(U13-C-Pad8)")
  (net 769 "unconnected-(U13-B-Pad9)")
  (net 770 "unconnected-(U13-A-Pad10)")
  (net 771 "unconnected-(U14-CA-Pad1)")
  (net 772 "unconnected-(U14-F-Pad2)")
  (net 773 "unconnected-(U14-G-Pad3)")
  (net 774 "unconnected-(U14-E-Pad4)")
  (net 775 "unconnected-(U14-D-Pad5)")
  (net 776 "unconnected-(U14-CA-Pad6)")
  (net 777 "unconnected-(U14-DP-Pad7)")
  (net 778 "unconnected-(U14-C-Pad8)")
  (net 779 "unconnected-(U14-B-Pad9)")
  (net 780 "unconnected-(U14-A-Pad10)")
  (net 781 "unconnected-(U15-CA-Pad1)")
  (net 782 "unconnected-(U15-F-Pad2)")
  (net 783 "unconnected-(U15-G-Pad3)")
  (net 784 "unconnected-(U15-E-Pad4)")
  (net 785 "unconnected-(U15-D-Pad5)")
  (net 786 "unconnected-(U15-CA-Pad6)")
  (net 787 "unconnected-(U15-DP-Pad7)")
  (net 788 "unconnected-(U15-C-Pad8)")
  (net 789 "unconnected-(U15-B-Pad9)")
  (net 790 "unconnected-(U15-A-Pad10)")
  (net 791 "unconnected-(U17-CS#-Pad1)")
  (net 792 "unconnected-(U17-S0{slash}SI01-Pad2)")
  (net 793 "unconnected-(U17-WP#{slash}SIO2-Pad3)")
  (net 794 "unconnected-(U17-GND-Pad4)")
  (net 795 "unconnected-(U17-SI{slash}SIO0-Pad5)")
  (net 796 "unconnected-(U17-SCLK-Pad6)")
  (net 797 "unconnected-(U17-HOLD#{slash}SIO3-Pad7)")
  (net 798 "unconnected-(U17-VCC-Pad8)")
  (net 799 "unconnected-(U18-GPIN7-Pad1)")
  (net 800 "unconnected-(U18-VL-Pad2)")
  (net 801 "unconnected-(U18-GND-Pad3)")
  (net 802 "unconnected-(U18-GPOUT0-Pad4)")
  (net 803 "unconnected-(U18-GPOUT1-Pad5)")
  (net 804 "unconnected-(U18-GPOUT2-Pad6)")
  (net 805 "unconnected-(U18-GPOUT3-Pad7)")
  (net 806 "unconnected-(U18-GPOUT4-Pad8)")
  (net 807 "unconnected-(U18-GPOUT5-Pad9)")
  (net 808 "unconnected-(U18-GPOUT6-Pad10)")
  (net 809 "unconnected-(U18-GPOUT7-Pad11)")
  (net 810 "unconnected-(U18-~{RES}-Pad12)")
  (net 811 "unconnected-(U18-SCLK-Pad13)")
  (net 812 "unconnected-(U18-~{SS}-Pad14)")
  (net 813 "unconnected-(U18-MISO-Pad15)")
  (net 814 "unconnected-(U18-MOSI-Pad16)")
  (net 815 "unconnected-(U18-GPX-Pad17)")
  (net 816 "unconnected-(U18-INT-Pad18)")
  (net 817 "unconnected-(U18-GND-Pad19)")
  (net 818 "unconnected-(U18-D--Pad20)")
  (net 819 "unconnected-(U18-D+-Pad21)")
  (net 820 "unconnected-(U18-VBCOMP-Pad22)")
  (net 821 "unconnected-(U18-VCC-Pad23)")
  (net 822 "unconnected-(U18-XI-Pad24)")
  (net 823 "unconnected-(U18-XO-Pad25)")
  (net 824 "unconnected-(U18-GPIN0-Pad26)")
  (net 825 "unconnected-(U18-GPIN1-Pad27)")
  (net 826 "unconnected-(U18-GPIN2-Pad28)")
  (net 827 "unconnected-(U18-GPIN3-Pad29)")
  (net 828 "unconnected-(U18-GPIN4-Pad30)")
  (net 829 "unconnected-(U18-GPIN5-Pad31)")
  (net 830 "unconnected-(U18-GPIN6-Pad32)")
  (net 831 "unconnected-(U19-DP0-Pad1)")
  (net 832 "unconnected-(U19-DM0-Pad2)")
  (net 833 "unconnected-(U19-VCC-Pad3)")
  (net 834 "unconnected-(U19-~{RESET}-Pad4)")
  (net 835 "unconnected-(U19-EECLK-Pad5)")
  (net 836 "unconnected-(U19-EEDATA{slash}GANGED-Pad6)")
  (net 837 "unconnected-(U19-GND-Pad7)")
  (net 838 "unconnected-(U19-BUSPWR-Pad8)")
  (net 839 "unconnected-(U19-~{PWRON1}-Pad9)")
  (net 840 "unconnected-(U19-~{OVRCUR1}-Pad10)")
  (net 841 "unconnected-(U19-DM1-Pad11)")
  (net 842 "unconnected-(U19-DP1-Pad12)")
  (net 843 "unconnected-(U19-~{PWRON2}-Pad13)")
  (net 844 "unconnected-(U19-~{OVRCUR2}-Pad14)")
  (net 845 "unconnected-(U19-DM2-Pad15)")
  (net 846 "unconnected-(U19-DP2-Pad16)")
  (net 847 "unconnected-(U19-~{PWRON3}-Pad17)")
  (net 848 "unconnected-(U19-~{OVRCUR3}-Pad18)")
  (net 849 "unconnected-(U19-DM3-Pad19)")
  (net 850 "unconnected-(U19-DP3-Pad20)")
  (net 851 "unconnected-(U19-~{PWRON4}-Pad21)")
  (net 852 "unconnected-(U19-~{OVRCUR4}-Pad22)")
  (net 853 "unconnected-(U19-DM4-Pad23)")
  (net 854 "unconnected-(U19-DP4-Pad24)")
  (net 855 "unconnected-(U19-VCC__1-Pad25)")
  (net 856 "unconnected-(U19-~{EXTMEM}-Pad26)")
  (net 857 "unconnected-(U19-TSTPLL{slash}48MCLK-Pad27)")
  (net 858 "unconnected-(U19-GND__1-Pad28)")
  (net 859 "unconnected-(U19-XTAL2-Pad29)")
  (net 860 "unconnected-(U19-XTAL1-Pad30)")
  (net 861 "unconnected-(U19-TSTMODE-Pad31)")
  (net 862 "unconnected-(U19-SUSPND-Pad32)")
  (net 863 "unconnected-(U20-GND-Pad1)")
  (net 864 "unconnected-(U20-OSCI-Pad2)")
  (net 865 "unconnected-(U20-OSCO-Pad3)")
  (net 866 "unconnected-(U20-VPHY-Pad4)")
  (net 867 "unconnected-(U20-GND-Pad5)")
  (net 868 "unconnected-(U20-REF-Pad6)")
  (net 869 "unconnected-(U20-DM-Pad7)")
  (net 870 "unconnected-(U20-DP-Pad8)")
  (net 871 "unconnected-(U20-VPLL-Pad9)")
  (net 872 "unconnected-(U20-AGND-Pad10)")
  (net 873 "unconnected-(U20-GND-Pad11)")
  (net 874 "unconnected-(U20-VCORE-Pad12)")
  (net 875 "unconnected-(U20-TEST-Pad13)")
  (net 876 "unconnected-(U20-~{RESET}-Pad14)")
  (net 877 "unconnected-(U20-GND-Pad15)")
  (net 878 "unconnected-(U20-ADBUS0-Pad16)")
  (net 879 "unconnected-(U20-ADBUS1-Pad17)")
  (net 880 "unconnected-(U20-ADBUS2-Pad18)")
  (net 881 "unconnected-(U20-ADBUS3-Pad19)")
  (net 882 "unconnected-(U20-VCCIO-Pad20)")
  (net 883 "unconnected-(U20-ADBUS4-Pad21)")
  (net 884 "unconnected-(U20-ADBUS5-Pad22)")
  (net 885 "unconnected-(U20-ADBUS6-Pad23)")
  (net 886 "unconnected-(U20-ADBUS7-Pad24)")
  (net 887 "unconnected-(U20-GND-Pad25)")
  (net 888 "unconnected-(U20-BDBUS0-Pad26)")
  (net 889 "unconnected-(U20-BDBUS1-Pad27)")
  (net 890 "unconnected-(U20-BDBUS2-Pad28)")
  (net 891 "unconnected-(U20-BDBUS3-Pad29)")
  (net 892 "unconnected-(U20-BDBUS4-Pad30)")
  (net 893 "unconnected-(U20-VCCIO-Pad31)")
  (net 894 "unconnected-(U20-BDBUS5-Pad32)")
  (net 895 "unconnected-(U20-BDBUS6-Pad33)")
  (net 896 "unconnected-(U20-BDBUS7-Pad34)")
  (net 897 "unconnected-(U20-GND-Pad35)")
  (net 898 "unconnected-(U20-~{SUSPEND}-Pad36)")
  (net 899 "unconnected-(U20-VCORE-Pad37)")
  (net 900 "unconnected-(U20-CDBUS0-Pad38)")
  (net 901 "unconnected-(U20-CDBUS1-Pad39)")
  (net 902 "unconnected-(U20-CDBUS2-Pad40)")
  (net 903 "unconnected-(U20-CDBUS3-Pad41)")
  (net 904 "unconnected-(U20-VCCIO-Pad42)")
  (net 905 "unconnected-(U20-CDBUS4-Pad43)")
  (net 906 "unconnected-(U20-CDBUS5-Pad44)")
  (net 907 "unconnected-(U20-CDBUS6-Pad45)")
  (net 908 "unconnected-(U20-CDBUS7-Pad46)")
  (net 909 "unconnected-(U20-GND-Pad47)")
  (net 910 "unconnected-(U20-DDBUS0-Pad48)")
  (net 911 "unconnected-(U20-VREGOUT-Pad49)")
  (net 912 "unconnected-(U20-VREGIN-Pad50)")
  (net 913 "unconnected-(U20-GND-Pad51)")
  (net 914 "unconnected-(U20-DDBUS1-Pad52)")
  (net 915 "unconnected-(U20-DDBUS2-Pad53)")
  (net 916 "unconnected-(U20-DDBUS3-Pad54)")
  (net 917 "unconnected-(U20-DDBUS4-Pad55)")
  (net 918 "unconnected-(U20-VCCIO-Pad56)")
  (net 919 "unconnected-(U20-DDBUS5-Pad57)")
  (net 920 "unconnected-(U20-DDBUS6-Pad58)")
  (net 921 "unconnected-(U20-DDBUS7-Pad59)")
  (net 922 "unconnected-(U20-~{PWREN}-Pad60)")
  (net 923 "unconnected-(U20-EEDATA-Pad61)")
  (net 924 "unconnected-(U20-EECLK-Pad62)")
  (net 925 "unconnected-(U20-EECS-Pad63)")
  (net 926 "unconnected-(U20-VCORE-Pad64)")

  (footprint "Connector_USB:0672984091" (layer "F.Cu")
    (tstamp 023893f6-366c-41c4-b569-02ade8c3d895)
    (at 120.9525 93.885)
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "usb")
    (property "ki_description" "USB Type A connector, stacked")
    (property "ki_keywords" "connector USB")
    (path "/608a5705-96be-4a71-b2b6-c4625a5aee39/83371247-4120-4e7b-86a2-d6d289cc6222")
    (attr through_hole)
    (fp_text reference "J5" (at 3.7975 -7.885 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 40141441-656c-4c44-aea0-06661fae10a1)
    )
    (fp_text value "USB_A_Stacked" (at 3.5 3 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 71b77a27-8be3-4932-b520-fecef2b5edc0)
    )
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7672d04b-03fe-45b7-9d3d-5578e84bcb1e)
    )
    (fp_rect (start -6 -6.5) (end 13 15)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 847f002b-4233-43f1-ad47-ad9fe0a2abff))
    (fp_rect (start -5.5 -6) (end 12.5 14.5)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.Fab") (tstamp 8dbd3970-0a15-4806-8d7a-eae4f383a8b7))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 90 "unconnected-(J5-VBUS1-Pad1)") (pinfunction "VBUS1") (pintype "power_in") (tstamp 247e34b8-f042-4612-aff2-eb5afc116aa8))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 91 "unconnected-(J5-D1--Pad2)") (pinfunction "D1-") (pintype "bidirectional") (tstamp 9788f46e-1ce5-46bf-a299-cfafe705e8bf))
    (pad "3" thru_hole circle (at 4.5 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 92 "unconnected-(J5-D1+-Pad3)") (pinfunction "D1+") (pintype "bidirectional") (tstamp 44c683c9-9e32-4014-b051-5ed07376900c))
    (pad "4" thru_hole circle (at 7 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 93 "unconnected-(J5-GND1-Pad4)") (pinfunction "GND1") (pintype "power_in") (tstamp 752336a6-c7cd-493d-9045-d7cfec1cd590))
    (pad "5" thru_hole circle (at 0 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 94 "unconnected-(J5-VBUS2-Pad5)") (pinfunction "VBUS2") (pintype "power_in") (tstamp c8df0eef-499b-4289-9b01-2165c2d35381))
    (pad "6" thru_hole circle (at 2.5 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 95 "unconnected-(J5-D2--Pad6)") (pinfunction "D2-") (pintype "bidirectional") (tstamp b4452c2a-4142-4271-92b8-bd598294eecc))
    (pad "7" thru_hole circle (at 4.5 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 96 "unconnected-(J5-D2+-Pad7)") (pinfunction "D2+") (pintype "bidirectional") (tstamp 8b329f4b-0946-4f02-8f4a-152398001595))
    (pad "8" thru_hole circle (at 7 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 97 "unconnected-(J5-GND2-Pad8)") (pinfunction "GND2") (pintype "power_in") (tstamp a1e89d08-b978-4ff7-a838-cbc25f784dab))
    (pad "9" thru_hole circle (at -3.07 -2.97) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(J5-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp 731cf0e1-d58e-40d7-83e8-2e87640886a5))
    (pad "9" thru_hole circle (at -3.07 2.71) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(J5-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp 0aad8fb7-a5dd-44c3-825d-841890b1894d))
    (pad "9" thru_hole circle (at 10.07 -2.97) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(J5-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp c10e71cb-2913-4a17-bbcf-92398ef27b27))
    (pad "9" thru_hole circle (at 10.07 2.71) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(J5-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp 062c0d95-91b5-4548-895c-06f4931a6745))
    (model ":KICAD7_3DMODEL_DIR:Connector_USB.3dshapes/672984091.stp"
      (offset (xyz 3.5 -12.5 7.8))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 0617dbb8-55fb-4b31-afb7-cf1a4c2d2764)
    (at 82.91 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/243667fb-9878-4eaa-a3d8-45e388be62d3")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 05e1ba94-e2c0-456b-bd89-ef3ac699ae7c)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 64f86585-4da3-469e-a848-9df0fd72112d)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 59408b91-1354-455f-9722-46b46845d253)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca6f0ec0-b7c2-4626-8ac4-aa2f9c9f0682))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 79de0b14-d108-4739-83ab-f31d756006d3))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c8c653b-574c-4e46-80ad-1e3d105d61de))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 12e3f9ea-4069-4c8a-86c5-c6524490b410))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9928a868-f146-459a-b043-e8e32d8ec602))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 80e561d6-9d1f-486c-8ea2-a5554b5cfaaf))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a9303a90-0f95-47ce-87f6-598cbd0438e4))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 699df35d-b45b-4dda-a9a2-29e72a810f7a))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 29079e0c-00d9-4bd9-a9ee-2c8e629fba29))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca59e18f-5a0c-4215-be08-d388a1ec592e))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 29a84ce5-2d51-43da-9bdd-1f424c029a84))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77ca74b4-8b56-492c-9c3c-b8cf09703f72))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "unconnected-(D7-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 2ab0a51c-c468-48a3-bdca-652bbd004559))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "unconnected-(D7-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp e388183d-1840-4557-9ba1-5c4f8f2adb87))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 0bea8a68-3572-4a69-b746-d46f6946f267)
    (at 58.5 36.6625 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/090da324-3735-4668-aeba-899323b7ab4c")
    (attr smd)
    (fp_text reference "R6" (at 0 1.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a4463a12-d2af-425c-9aaa-b4fd005af0f6)
    )
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 561d3e8e-5ee3-404a-b8ae-d45e45ca6914)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 96820169-f226-45fb-804f-9b3c94793a72)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9fe8ea8c-ea7d-4064-b726-82a6403af8c9))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 839cbc48-475b-4fad-9ddc-ff5cfb0a429b))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2a212c3a-cea4-4346-aeb2-f1774b09c0e6))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a90cedf9-b9e2-4fa6-a010-50600e37910c))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1eb784bb-39c4-41dd-bea7-c6db7ec3c300))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 789d403f-62fc-46c1-87ee-30213f1f8122))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3322611f-69ba-430c-885d-46147720a049))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4896c782-7f0c-4112-ba1e-dab624187433))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d4071c6-5119-4fe5-a31a-fac9713d026e))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ba9c3de3-0cb2-4b1a-89a0-66709ad817cf))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 572 "+3V3") (pintype "passive") (tstamp a1faae1b-5982-41e6-9a29-2ef48c7ed13a))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 600 "/cpu/CPU_BE") (pintype "passive") (tstamp 7de147fa-dc86-49da-9608-f68a2917f833))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 1fb94356-8a45-4f67-80cc-e73b0f2b70a3)
    (at 34 37.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/6cf6abb0-8653-4309-a78b-ade9f5190558")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bcf08dc0-1764-4655-9a02-8e9b44f0c0ee)
    )
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f801f37-459f-4456-942d-9a564638e9c9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 891e8da6-02e3-4d81-93cb-402d972af985)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 711b4ab7-3a94-4fd7-acc1-ed8096e1420b))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e7c1128c-ba73-447c-a4e5-0eb6ed3673a4))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp deb51027-c449-4a6b-86d7-30d34fc7a010))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e73d34f-6db0-4b86-9eb1-620765c5bfc1))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d51bbd90-6033-4489-a965-8828694ce44d))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1da27a55-9921-446f-a4e7-b1a138f473c2))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bbb27426-9f9d-480c-9c07-d517e67dd5a3))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 628dd248-c2a5-4894-997c-42acd87ea7ea))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9952fe33-98ff-4690-a52d-2f334b5acdd8))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp efc2b75d-a67e-4ff5-a3a4-c4308ef5e7cb))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 572 "+3V3") (pintype "passive") (tstamp 4307975e-3154-4492-b256-3131c8955e97))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 570 "/cpu/~{CPU_NMIB}") (pintype "passive") (tstamp 3c93f0db-ecb1-4eb8-8624-2021079b49a8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Display_7Segment:LTS-4802B" (layer "F.Cu")
    (tstamp 246f88ee-56f7-4d83-8746-16533a0f8a42)
    (at 40.75 90.34)
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/87ddf1e7-2662-46dd-b789-79c2788da4da")
    (attr through_hole)
    (fp_text reference "U10" (at 0 -2.54 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c325107-ac23-4997-b471-03c88e9ed946)
    )
    (fp_text value "~" (at 3.58 13.1 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 86c52dcd-7063-4657-8430-4465cac49b58)
    )
    (fp_text user "${REFERENCE}" (at 3.58 4.01 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 929a509f-79bd-45a6-a628-42b01bef81d9)
    )
    (fp_rect (start -1.04 -1.07) (end 8.66 11.83)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 56722a4b-dc26-4d6f-b04a-519b4d8d61d8))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 731 "unconnected-(U10-CA-Pad1)") (pinfunction "CA") (pintype "passive") (tstamp c8e7b82f-c1b7-422f-8d60-a14c60c935ce))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 732 "unconnected-(U10-F-Pad2)") (pinfunction "F") (pintype "passive") (tstamp 99f11b4f-f0a5-4d7c-b623-bde9b809a024))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 733 "unconnected-(U10-G-Pad3)") (pinfunction "G") (pintype "passive") (tstamp 7531abb2-60e8-4c9a-9c3f-91af3d5c8ff8))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 734 "unconnected-(U10-E-Pad4)") (pinfunction "E") (pintype "passive") (tstamp 972c5ad4-6556-47a4-a6dd-63e9b780451e))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 735 "unconnected-(U10-D-Pad5)") (pinfunction "D") (pintype "passive") (tstamp 5c317310-2b09-41b2-bdeb-491a8d10b4f6))
    (pad "6" thru_hole circle (at 7.62 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 736 "unconnected-(U10-CA-Pad6)") (pinfunction "CA") (pintype "passive") (tstamp df2164c0-8407-4423-9679-20f5b97b220a))
    (pad "7" thru_hole circle (at 7.62 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 737 "unconnected-(U10-DP-Pad7)") (pinfunction "DP") (pintype "passive") (tstamp 64d87b83-7620-45c8-b1d0-f67f481fbeb3))
    (pad "8" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 738 "unconnected-(U10-C-Pad8)") (pinfunction "C") (pintype "passive") (tstamp abf09931-a0af-4dd1-875c-c15d00b6732d))
    (pad "9" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 739 "unconnected-(U10-B-Pad9)") (pinfunction "B") (pintype "passive") (tstamp 20ad22c5-ef52-46a1-988c-43ba579c27d2))
    (pad "10" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 740 "unconnected-(U10-A-Pad10)") (pinfunction "A") (pintype "passive") (tstamp e5e57b69-024f-4bd4-bdac-486a4b8926d7))
    (model ":KICAD7_3DMODEL_DIR:Display_7Segment.3dshapes/LTS-4802BJR-H1_LTO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_HDMI:AMPHENOL_10029449-111RLF" (layer "F.Cu")
    (tstamp 36796735-ddee-4282-9dab-727166b2ee1f)
    (at 118.21925 25.5975 180)
    (property "MANUFACTURER" "Amphenol")
    (property "MAXIMUM_PACKAGE_HEIGHT" "6.18mm")
    (property "PARTREV" "Y")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hdmi.kicad_sch")
    (property "Sheetname" "hdmi")
    (path "/d1b08bf9-d018-4d88-92a5-af0d22dce754/f46d421e-9294-4334-b9b3-b35bf5739855")
    (attr smd)
    (fp_text reference "J2" (at -5.925 -9.635) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84a86457-7ab8-4f98-807e-d942ed09f091)
    )
    (fp_text value "10029449-111RLF" (at 6.14 -8.135) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9892807-6ed6-4a74-94b9-25b167048b93)
    )
    (fp_text user "PCB EDGE" (at 9.5 2.25) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.15)))
      (tstamp 11896f5c-8a43-468c-9074-458bd6f20560)
    )
    (fp_line (start -7.5 -1.35) (end -7.5 -3.6)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 863f4517-ab47-4944-9179-6eea1f24c5e1))
    (fp_line (start -7.5 1.35) (end -7.5 2.55)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp d1103b5b-abdc-4618-9b44-ae43ef494e00))
    (fp_line (start -7.5 2.55) (end 7.5 2.55)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 05d793b3-4cf5-4dc5-a5b8-d2aa76da8958))
    (fp_line (start -5.9 -5.98) (end -4.75 -5.98)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp c05b1d6c-c107-4b2f-b1fe-ec6b86777f92))
    (fp_line (start 5.9 -5.98) (end 5.25 -5.98)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 191d620c-cb8c-4d0e-ab4e-57e9a421847d))
    (fp_line (start 7.5 -3.6) (end 7.5 -1.35)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 5e67a708-26c2-4ee5-bb92-1bb073efd09b))
    (fp_line (start 7.5 2.55) (end 7.5 1.35)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 8eebb0ef-d754-41a5-b5ad-3ab963b14a5d))
    (fp_circle (center 4.75 -7.4) (end 4.85 -7.4)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.SilkS") (tstamp 88dc39cb-9c08-4a77-87b0-117e59b9ba8e))
    (fp_poly
      (pts
        (xy -4.45 -6.85)
        (xy -4.05 -6.85)
        (xy -4.05 -4.85)
        (xy -4.45 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 9752229d-1da0-468a-b68c-165be5c0e864))
    (fp_poly
      (pts
        (xy -3.95 -6.85)
        (xy -3.55 -6.85)
        (xy -3.55 -4.85)
        (xy -3.95 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 549f2f0c-32a5-43a3-954f-da9680ec00cc))
    (fp_poly
      (pts
        (xy -3.45 -6.85)
        (xy -3.05 -6.85)
        (xy -3.05 -4.85)
        (xy -3.45 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp b814d7c8-330a-4306-b90c-943eb83e73b1))
    (fp_poly
      (pts
        (xy -2.95 -6.85)
        (xy -2.55 -6.85)
        (xy -2.55 -4.85)
        (xy -2.95 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp dc55fe1d-3a9c-43ea-b623-588dfab7d4d8))
    (fp_poly
      (pts
        (xy -2.45 -6.85)
        (xy -2.05 -6.85)
        (xy -2.05 -4.85)
        (xy -2.45 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp bba1ab3c-96de-482f-960f-e25b918aea28))
    (fp_poly
      (pts
        (xy -1.95 -6.85)
        (xy -1.55 -6.85)
        (xy -1.55 -4.85)
        (xy -1.95 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 3b2e27eb-ae61-4317-8918-15a2854fdeed))
    (fp_poly
      (pts
        (xy -1.45 -6.85)
        (xy -1.05 -6.85)
        (xy -1.05 -4.85)
        (xy -1.45 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp d1e7cddd-94a9-4a87-87a5-9fc03f423514))
    (fp_poly
      (pts
        (xy -0.95 -6.85)
        (xy -0.55 -6.85)
        (xy -0.55 -4.85)
        (xy -0.95 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp edbd9156-5bdf-4a2c-b63f-1f74cbdc33c4))
    (fp_poly
      (pts
        (xy -0.45 -6.85)
        (xy -0.05 -6.85)
        (xy -0.05 -4.85)
        (xy -0.45 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 38910251-b07d-47ca-9d2b-b7593fb6b145))
    (fp_poly
      (pts
        (xy 0.05 -6.85)
        (xy 0.45 -6.85)
        (xy 0.45 -4.85)
        (xy 0.05 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 6523d2b8-efb7-4ba8-a04a-ab7bed1929b7))
    (fp_poly
      (pts
        (xy 0.55 -6.85)
        (xy 0.95 -6.85)
        (xy 0.95 -4.85)
        (xy 0.55 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 765ea60d-2734-429c-834d-7ad5914df55f))
    (fp_poly
      (pts
        (xy 1.05 -6.85)
        (xy 1.45 -6.85)
        (xy 1.45 -4.85)
        (xy 1.05 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 20a1e082-1a51-4578-816a-3e1b5febef8c))
    (fp_poly
      (pts
        (xy 1.55 -6.85)
        (xy 1.95 -6.85)
        (xy 1.95 -4.85)
        (xy 1.55 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 3eaf7d51-bd90-4bbf-9fff-c680dbbfac77))
    (fp_poly
      (pts
        (xy 2.05 -6.85)
        (xy 2.45 -6.85)
        (xy 2.45 -4.85)
        (xy 2.05 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 17602dff-bf16-4b75-adf9-c8ee165c2f28))
    (fp_poly
      (pts
        (xy 2.55 -6.85)
        (xy 2.95 -6.85)
        (xy 2.95 -4.85)
        (xy 2.55 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 51e3d62f-6f2e-4597-9df9-b7991dbbb56a))
    (fp_poly
      (pts
        (xy 3.05 -6.85)
        (xy 3.45 -6.85)
        (xy 3.45 -4.85)
        (xy 3.05 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp d0b19d1a-f998-4202-8211-fa41d534e66d))
    (fp_poly
      (pts
        (xy 3.55 -6.85)
        (xy 3.95 -6.85)
        (xy 3.95 -4.85)
        (xy 3.55 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 4e3d874b-a14e-4ed5-b522-50758d7692a8))
    (fp_poly
      (pts
        (xy 4.05 -6.85)
        (xy 4.45 -6.85)
        (xy 4.45 -4.85)
        (xy 4.05 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 342f0325-0b80-437e-b33b-65d6470ddf7b))
    (fp_poly
      (pts
        (xy 4.55 -6.85)
        (xy 4.95 -6.85)
        (xy 4.95 -4.85)
        (xy 4.55 -4.85)
      )

      (stroke (width 0.01) (type solid)) (fill solid) (layer "F.Mask") (tstamp 21b52ac3-e60e-49c8-b58e-f8226e4a6b55))
    (fp_line (start -9.1 -7.05) (end -9.1 3.77)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9a437e68-a257-4fee-98b1-51357fe511d8))
    (fp_line (start -9.1 3.77) (end 9.1 3.77)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f8ad97e8-4684-4417-8146-24fe0d05e9bb))
    (fp_line (start 9.1 -7.05) (end -9.1 -7.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c5d0966-77ee-4225-8d78-2161f89c980c))
    (fp_line (start 9.1 3.77) (end 9.1 -7.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3cc91df7-bb00-40b6-96d4-07ed8f27b801))
    (fp_line (start -7.5 -5.98) (end -7.5 2.55)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 6a656190-de2e-4724-9456-0cdf9308e24e))
    (fp_line (start -7.5 2.55) (end -7.5 3.52)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 27865efc-6ea9-4869-8ce8-021b857ee3a0))
    (fp_line (start -7.5 2.55) (end 10 2.55)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 0d009617-1ce6-40a9-861a-f41a7ed11439))
    (fp_line (start -7.5 3.52) (end 7.5 3.52)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp ce7d5dcf-b554-489e-8232-37ad064cf6fd))
    (fp_line (start 7.5 -5.98) (end -7.5 -5.98)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp de74d359-2028-4eb1-9f79-eda1c51ce4f3))
    (fp_line (start 7.5 3.52) (end 7.5 -5.98)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp c9be68fe-abab-491c-ab7a-4ee4cbfd4f29))
    (fp_circle (center 4.75 -7.4) (end 4.85 -7.4)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.Fab") (tstamp ed9d1a2e-e992-47ac-8837-42b4446f19e9))
    (pad "1" smd rect (at 4.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 33 "unconnected-(J2-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 0cd9e3a8-42a8-409f-83f8-742725c16a85))
    (pad "2" smd rect (at 4.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 34 "unconnected-(J2-Pad2)") (pinfunction "2") (pintype "passive") (tstamp d11b7aae-b0ec-44ad-b8cf-1d2f95087468))
    (pad "3" smd rect (at 3.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 35 "unconnected-(J2-Pad3)") (pinfunction "3") (pintype "passive") (tstamp f1d75753-d0e1-495f-a5d1-3f70044a8bb9))
    (pad "4" smd rect (at 3.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 36 "unconnected-(J2-Pad4)") (pinfunction "4") (pintype "passive") (tstamp 6384d889-3dd2-4980-abf6-a9e79ee58970))
    (pad "5" smd rect (at 2.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 37 "unconnected-(J2-Pad5)") (pinfunction "5") (pintype "passive") (tstamp 7584852a-70b0-487b-b13c-8fdfbe6479bd))
    (pad "6" smd rect (at 2.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 38 "unconnected-(J2-Pad6)") (pinfunction "6") (pintype "passive") (tstamp 7ed72efa-6b8d-4041-b955-c0d95b0316c2))
    (pad "7" smd rect (at 1.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 39 "unconnected-(J2-Pad7)") (pinfunction "7") (pintype "passive") (tstamp 74387793-3610-4fcb-b7e2-6fe64f4e8468))
    (pad "8" smd rect (at 1.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 40 "unconnected-(J2-Pad8)") (pinfunction "8") (pintype "passive") (tstamp f35faa26-c4d9-4ed3-bcad-86238e4dd843))
    (pad "9" smd rect (at 0.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 41 "unconnected-(J2-Pad9)") (pinfunction "9") (pintype "passive") (tstamp 0e7296a2-bee2-4f06-85dd-0241afa22315))
    (pad "10" smd rect (at 0.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 42 "unconnected-(J2-Pad10)") (pinfunction "10") (pintype "passive") (tstamp c5220ba2-035a-4efb-bb1b-9314c348c467))
    (pad "11" smd rect (at -0.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 43 "unconnected-(J2-Pad11)") (pinfunction "11") (pintype "passive") (tstamp 6c003a01-cfe5-43e8-a07e-2aa00ea3fbc2))
    (pad "12" smd rect (at -0.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 44 "unconnected-(J2-Pad12)") (pinfunction "12") (pintype "passive") (tstamp 49c82893-6264-4adb-8ae7-c0f6e9a43463))
    (pad "13" smd rect (at -1.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 45 "unconnected-(J2-Pad13)") (pinfunction "13") (pintype "passive") (tstamp 526e6310-744d-4f4f-935e-22e10b57d9f8))
    (pad "14" smd rect (at -1.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 46 "unconnected-(J2-Pad14)") (pinfunction "14") (pintype "passive") (tstamp 654ec278-e798-4aee-89d1-063e9eab8495))
    (pad "15" smd rect (at -2.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 47 "unconnected-(J2-Pad15)") (pinfunction "15") (pintype "passive") (tstamp 525a32be-a02c-47bc-a5b3-584248db5542))
    (pad "16" smd rect (at -2.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 48 "unconnected-(J2-Pad16)") (pinfunction "16") (pintype "passive") (tstamp 91ecfdf4-8543-4adb-88af-d85c04547cb7))
    (pad "17" smd rect (at -3.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 49 "unconnected-(J2-Pad17)") (pinfunction "17") (pintype "passive") (tstamp 583194f4-4eb9-4992-b83a-169dcfcb8158))
    (pad "18" smd rect (at -3.75 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 50 "unconnected-(J2-Pad18)") (pinfunction "18") (pintype "passive") (tstamp f5c76634-b9a8-45b4-9791-70dfea630c81))
    (pad "19" smd rect (at -4.25 -5.85 180) (size 0.3 1.9) (layers "F.Cu" "F.Paste")
      (net 51 "unconnected-(J2-Pad19)") (pinfunction "19") (pintype "passive") (tstamp 933cca81-7d87-4463-ac96-a2ac5805bf09))
    (pad "S1" thru_hole circle (at -7.25 -4.95 180) (size 1.995 1.995) (drill 1.33) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(J2-SHIELD-PadS1)") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102) (tstamp 1e3b2059-d2d0-42ad-89eb-d861463ecba1))
    (pad "S2" thru_hole circle (at 7.25 -4.95 180) (size 1.995 1.995) (drill 1.33) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(J2-SHIELD__1-PadS2)") (pinfunction "SHIELD__1") (pintype "passive") (solder_mask_margin 0.102) (tstamp f6a8113a-1060-4abd-a1bf-b9ef8a6a66d2))
    (pad "S3" thru_hole circle (at -7.85 0 180) (size 1.995 1.995) (drill 1.33) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(J2-SHIELD__2-PadS3)") (pinfunction "SHIELD__2") (pintype "passive") (solder_mask_margin 0.102) (tstamp 2147b680-adf6-4188-9272-edf0c1fe358b))
    (pad "S4" thru_hole circle (at 7.85 0 180) (size 1.995 1.995) (drill 1.33) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(J2-SHIELD__3-PadS4)") (pinfunction "SHIELD__3") (pintype "passive") (solder_mask_margin 0.102) (tstamp 8c79e352-4aa4-4437-a28a-2b9be7ec875c))
    (model ":KICAD7_3DMODEL_DIR:Connector_HDMI.3dshapes/10029449-111RLF.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "Package_QFP:LQFP-32_5x5mm_P0.5mm" (layer "F.Cu")
    (tstamp 36b2769b-5bbd-425b-93ef-239e2bdfac68)
    (at 135.85 62.825)
    (descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT401-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "usb")
    (path "/608a5705-96be-4a71-b2b6-c4625a5aee39/7e62afdf-c71a-4a81-b44e-4270c1f04016")
    (attr smd)
    (fp_text reference "U18" (at 0 -4.88) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d8994f12-9a93-446d-81ec-091a8a11afd6)
    )
    (fp_text value "MAX3421E" (at 0 4.88) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 22b9f49d-83f3-4e1d-b762-6097a7e3c54e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 46fe51ae-8970-451e-b8bb-451ed67dc07a)
    )
    (fp_line (start -2.61 -2.61) (end -2.61 -2.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5b9fbfbe-1cfd-48b0-b8eb-c9d8150fec1b))
    (fp_line (start -2.61 -2.16) (end -3.925 -2.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 10be4276-a8b2-4f35-b0ee-f70df1f77ec7))
    (fp_line (start -2.61 2.61) (end -2.61 2.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 15624234-00ae-46bf-a66f-515ac8f7f159))
    (fp_line (start -2.16 -2.61) (end -2.61 -2.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 721af5f6-0b10-4095-a285-5bee84b37119))
    (fp_line (start -2.16 2.61) (end -2.61 2.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5ce5cb7-2298-4b51-b85f-bb0a8debef92))
    (fp_line (start 2.16 -2.61) (end 2.61 -2.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f4448cf-f146-4977-aa66-b2d4a7c6723a))
    (fp_line (start 2.16 2.61) (end 2.61 2.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d6c251e3-15c3-404f-8759-c64acdeecf51))
    (fp_line (start 2.61 -2.61) (end 2.61 -2.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c188910f-231c-42b0-bf2b-42205881b6bf))
    (fp_line (start 2.61 2.61) (end 2.61 2.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c9f4450-b0cb-4147-9db1-2f126c23ebeb))
    (fp_line (start -4.18 -2.15) (end -4.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 41f953d5-5490-45a1-963a-ab1e57c07192))
    (fp_line (start -4.18 2.15) (end -4.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 477f6b16-cc0e-44c4-b3c6-90403f3717c3))
    (fp_line (start -2.75 -2.75) (end -2.75 -2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1826a036-af26-48ae-9b49-2ea2c3c98dee))
    (fp_line (start -2.75 -2.15) (end -4.18 -2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 53926d19-316b-4345-a7f8-6649882e052d))
    (fp_line (start -2.75 2.15) (end -4.18 2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dd350a89-20ce-4d7e-832b-5377937f21e7))
    (fp_line (start -2.75 2.75) (end -2.75 2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1b9d4e54-2630-4601-922d-849505a6e2cb))
    (fp_line (start -2.15 -4.18) (end -2.15 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fb812840-b24c-4eb8-986c-7fef8f00dc37))
    (fp_line (start -2.15 -2.75) (end -2.75 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e6b5e723-6285-48eb-9073-fd1d7c658e68))
    (fp_line (start -2.15 2.75) (end -2.75 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a4be40d0-d8f4-4d94-aff5-a67c203fa51e))
    (fp_line (start -2.15 4.18) (end -2.15 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1ef33c4-ed5d-4e57-b3f3-195b8928475d))
    (fp_line (start 0 -4.18) (end -2.15 -4.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a1431809-763d-4a2d-8d7f-3b49da344a53))
    (fp_line (start 0 -4.18) (end 2.15 -4.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c87fbf3-0655-4676-80df-61a2df9e209c))
    (fp_line (start 0 4.18) (end -2.15 4.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6502a0e1-c713-4fb7-9aa8-47e5c2b2cc27))
    (fp_line (start 0 4.18) (end 2.15 4.18)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 33293c64-4dd7-4771-9355-46ebc8959be9))
    (fp_line (start 2.15 -4.18) (end 2.15 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 68dafae3-1ec3-44ec-8cc2-f266da55c100))
    (fp_line (start 2.15 -2.75) (end 2.75 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b25ea3d2-9369-4326-acc1-4a92d95c3a5c))
    (fp_line (start 2.15 2.75) (end 2.75 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c9de022a-8f0a-41f1-b6b3-857c96a33193))
    (fp_line (start 2.15 4.18) (end 2.15 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ffccb640-f4c1-49a2-a102-a6f6303e12ae))
    (fp_line (start 2.75 -2.75) (end 2.75 -2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 878c5826-a16c-4f7c-a267-2ea6e366fc16))
    (fp_line (start 2.75 -2.15) (end 4.18 -2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bbce3b43-e028-4767-ab6c-61596f112ca1))
    (fp_line (start 2.75 2.15) (end 4.18 2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6e4872c6-abc6-4d3c-8fd4-1e01df3a7ffd))
    (fp_line (start 2.75 2.75) (end 2.75 2.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 955a9fcf-d2bd-476e-95f5-1a6517f54434))
    (fp_line (start 4.18 -2.15) (end 4.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 294f908f-f6cc-46ad-bbda-872ded02de8c))
    (fp_line (start 4.18 2.15) (end 4.18 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a6ec7d8d-9423-4b30-977e-fba567b9e835))
    (fp_line (start -2.5 -1.5) (end -1.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc8db90a-62fb-49b3-8206-61315f4cdb51))
    (fp_line (start -2.5 2.5) (end -2.5 -1.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2333a94-4c56-405f-9c0a-6cec1ab31889))
    (fp_line (start -1.5 -2.5) (end 2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp de5783ca-791a-4b44-af0f-38dc32f04213))
    (fp_line (start 2.5 -2.5) (end 2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 101f6f36-bb33-413d-acb9-50e36284e9d0))
    (fp_line (start 2.5 2.5) (end -2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b67cedca-d81c-427b-8e5e-f828daa37775))
    (pad "1" smd roundrect (at -3.175 -1.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 799 "unconnected-(U18-GPIN7-Pad1)") (pinfunction "GPIN7") (pintype "input") (tstamp 74d70b63-3e14-4957-b199-31664e9c6a5f))
    (pad "2" smd roundrect (at -3.175 -1.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 800 "unconnected-(U18-VL-Pad2)") (pinfunction "VL") (pintype "input") (tstamp 9ddc193c-d5d3-462e-ac3d-856d9b309e99))
    (pad "3" smd roundrect (at -3.175 -0.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 801 "unconnected-(U18-GND-Pad3)") (pinfunction "GND") (pintype "input") (tstamp 5be6bc57-5d7e-475c-b8e0-7f2e8f88d6f8))
    (pad "4" smd roundrect (at -3.175 -0.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 802 "unconnected-(U18-GPOUT0-Pad4)") (pinfunction "GPOUT0") (pintype "output") (tstamp 68dbdf13-4468-4eb5-85b2-4fc3d18fe6b2))
    (pad "5" smd roundrect (at -3.175 0.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 803 "unconnected-(U18-GPOUT1-Pad5)") (pinfunction "GPOUT1") (pintype "output") (tstamp 6196668d-532e-45b0-a17e-d00464722ad2))
    (pad "6" smd roundrect (at -3.175 0.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 804 "unconnected-(U18-GPOUT2-Pad6)") (pinfunction "GPOUT2") (pintype "output") (tstamp 256d4439-4112-4948-98ea-421585be7c6e))
    (pad "7" smd roundrect (at -3.175 1.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 805 "unconnected-(U18-GPOUT3-Pad7)") (pinfunction "GPOUT3") (pintype "output") (tstamp a8fc6b32-d1d6-497b-a2cf-4c23cce591cb))
    (pad "8" smd roundrect (at -3.175 1.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 806 "unconnected-(U18-GPOUT4-Pad8)") (pinfunction "GPOUT4") (pintype "output") (tstamp f7f171ad-0e0e-4fa7-a5cd-6f5cf8f8d199))
    (pad "9" smd roundrect (at -1.75 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 807 "unconnected-(U18-GPOUT5-Pad9)") (pinfunction "GPOUT5") (pintype "output") (tstamp 98d723d5-99e8-4d3a-bb46-aa2834fbad47))
    (pad "10" smd roundrect (at -1.25 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 808 "unconnected-(U18-GPOUT6-Pad10)") (pinfunction "GPOUT6") (pintype "output") (tstamp 9dff4e93-9016-4298-a64c-c143b654698e))
    (pad "11" smd roundrect (at -0.75 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 809 "unconnected-(U18-GPOUT7-Pad11)") (pinfunction "GPOUT7") (pintype "output") (tstamp b3474cbc-8426-4c7e-9aad-82a86c0cd98b))
    (pad "12" smd roundrect (at -0.25 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 810 "unconnected-(U18-~{RES}-Pad12)") (pinfunction "~{RES}") (pintype "input") (tstamp 46784ffb-25fb-49f7-be6a-6ad6f8cc5367))
    (pad "13" smd roundrect (at 0.25 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 811 "unconnected-(U18-SCLK-Pad13)") (pinfunction "SCLK") (pintype "input") (tstamp c743a3c9-9772-40e4-ba5c-94e393fecfb0))
    (pad "14" smd roundrect (at 0.75 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 812 "unconnected-(U18-~{SS}-Pad14)") (pinfunction "~{SS}") (pintype "input") (tstamp 62f992b0-752b-408f-b482-91c7cd74adea))
    (pad "15" smd roundrect (at 1.25 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 813 "unconnected-(U18-MISO-Pad15)") (pinfunction "MISO") (pintype "output") (tstamp 4450f3c0-d227-48f1-8e38-aa9b57e89532))
    (pad "16" smd roundrect (at 1.75 3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 814 "unconnected-(U18-MOSI-Pad16)") (pinfunction "MOSI") (pintype "input") (tstamp a109f7c3-5329-4440-a326-3a3df43c1f55))
    (pad "17" smd roundrect (at 3.175 1.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 815 "unconnected-(U18-GPX-Pad17)") (pinfunction "GPX") (pintype "output") (tstamp e5cf0164-6515-43d7-82d9-4d6e6a01e252))
    (pad "18" smd roundrect (at 3.175 1.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 816 "unconnected-(U18-INT-Pad18)") (pinfunction "INT") (pintype "output") (tstamp c4c9ae78-bc92-4885-9f97-3838321298ba))
    (pad "19" smd roundrect (at 3.175 0.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 817 "unconnected-(U18-GND-Pad19)") (pinfunction "GND") (pintype "input") (tstamp bf3458c7-af24-444c-b895-a7a6eb87e75a))
    (pad "20" smd roundrect (at 3.175 0.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 818 "unconnected-(U18-D--Pad20)") (pinfunction "D-") (pintype "bidirectional") (tstamp c993870d-9a36-4545-af01-b6c8bacf2b24))
    (pad "21" smd roundrect (at 3.175 -0.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 819 "unconnected-(U18-D+-Pad21)") (pinfunction "D+") (pintype "bidirectional") (tstamp b3059c44-ea09-4c9d-a9e0-355e321ce2c7))
    (pad "22" smd roundrect (at 3.175 -0.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 820 "unconnected-(U18-VBCOMP-Pad22)") (pinfunction "VBCOMP") (pintype "input") (tstamp 9454192e-cca0-411d-abf6-3be35abc7821))
    (pad "23" smd roundrect (at 3.175 -1.25) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 821 "unconnected-(U18-VCC-Pad23)") (pinfunction "VCC") (pintype "power_in") (tstamp b3411389-2315-4292-b81d-adc770212273))
    (pad "24" smd roundrect (at 3.175 -1.75) (size 1.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 822 "unconnected-(U18-XI-Pad24)") (pinfunction "XI") (pintype "input") (tstamp 9fbb44a6-2e38-4bf9-8ad8-f3b20cb31256))
    (pad "25" smd roundrect (at 1.75 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 823 "unconnected-(U18-XO-Pad25)") (pinfunction "XO") (pintype "output") (tstamp 803b65d1-18d5-48a9-91c1-2fab743b1e76))
    (pad "26" smd roundrect (at 1.25 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 824 "unconnected-(U18-GPIN0-Pad26)") (pinfunction "GPIN0") (pintype "input") (tstamp 67a72489-3eb6-48cc-aaf3-37d5a934a813))
    (pad "27" smd roundrect (at 0.75 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 825 "unconnected-(U18-GPIN1-Pad27)") (pinfunction "GPIN1") (pintype "input") (tstamp b0c9c73f-9587-4126-9fbf-e268c42b5f02))
    (pad "28" smd roundrect (at 0.25 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 826 "unconnected-(U18-GPIN2-Pad28)") (pinfunction "GPIN2") (pintype "input") (tstamp fd9018a8-d0ca-46dc-8512-eeb890a685d1))
    (pad "29" smd roundrect (at -0.25 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 827 "unconnected-(U18-GPIN3-Pad29)") (pinfunction "GPIN3") (pintype "input") (tstamp 493f9968-12e4-4a31-9acf-f43205faeb64))
    (pad "30" smd roundrect (at -0.75 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 828 "unconnected-(U18-GPIN4-Pad30)") (pinfunction "GPIN4") (pintype "input") (tstamp def29de2-5aa1-489c-a8f8-8a6bccb6ab3e))
    (pad "31" smd roundrect (at -1.25 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 829 "unconnected-(U18-GPIN5-Pad31)") (pinfunction "GPIN5") (pintype "input") (tstamp ef6b3756-72db-45f8-bd73-fe465b4f17e1))
    (pad "32" smd roundrect (at -1.75 -3.175) (size 0.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 830 "unconnected-(U18-GPIN6-Pad32)") (pinfunction "GPIN6") (pintype "input") (tstamp 63417c55-a0e0-4524-b837-96b7de568b21))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-32_5x5mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 3c32113d-1049-46e0-8cd1-38ae03b6547f)
    (at 85.5 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/9c5f308a-fbc1-4d42-81c6-42f9a5ec35ec")
    (attr smd)
    (fp_text reference "D8" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 482f9996-1432-46a0-883d-c77bdb0e61f8)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6954623a-13b3-4d53-8ca6-dd50ac976611)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 225b801b-6f69-4bd0-96cb-a653ca80900e)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8e55fb72-e29b-4992-ada9-8b5d2146a666))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 16475ea4-b2b4-46f4-abf1-ca4bd09bfcaa))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2b41fd76-1050-47c0-977f-591a7102ef42))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 851b8651-f9b3-4c27-8c7d-33bc8b87d264))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp df523955-5491-4c9a-b476-5d621ac2f53a))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 83ab2ed4-4e3d-402b-acfc-f7d8cb10ef53))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bfeabeb1-2624-4924-89a9-ebd5539943a7))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79e40ea4-0698-44a2-b8d1-08378f17040e))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6edb0a0d-a7cf-46d5-8180-c404d4480d0d))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8d50f31-1535-48b5-8352-745f9442ddeb))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c0ea06b2-3587-42c4-89c9-807c1ca818fa))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 386ea9b0-6431-4811-9d62-a9265b4a49cf))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(D8-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 78ebd298-db79-4290-a6cd-2d5b2ff95bb8))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "unconnected-(D8-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 98a6d48c-a95a-4a08-a9d0-d3569588962c))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 3ea4c796-69dd-47a8-9810-3f92a4070465)
    (at 58.5 24.75 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/67a343bc-66f0-487f-a63b-2e74c4d36413")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 87232900-c5b4-4a90-8a92-cc7603fc725b)
    )
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d4f703d2-c171-4266-a13b-5298d5762786)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 8fd9d104-268b-4a01-81bd-7c784c240d16)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ad78ebb6-82c0-4e27-b248-725284024688))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40577d13-69db-4c16-baa6-080cb955c432))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 040d710b-2172-4ad3-ade4-76b33c368fde))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c66277d1-cce6-4e14-9d26-931a503870ac))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bdafddcb-c28b-4d0e-a93a-3e0e84cc793c))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c5062128-c5be-4a71-8d24-92b3811aab84))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 68d77953-8d57-4670-a405-0d36df6e601a))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d70641f-01c0-4f1e-b7dd-cac6e92daeb3))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fcdf0f66-31a2-4465-a15f-22fa39a448ae))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7954e503-7a1d-4fa2-9f30-933273a60c99))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 572 "+3V3") (pintype "passive") (tstamp 9bee41d6-daf1-40dd-9be0-9c94f2db2f31))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 604 "/cpu/~{CPU_RESB}") (pintype "passive") (tstamp 91983241-4ebc-4390-b043-2c078321db28))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 4728b204-db4a-431c-8619-72eecf06e975)
    (at 77.73 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/79317d0b-dc8d-4a2d-ad5c-a7badfbfeaab")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0146a74-b478-4edd-99d7-e6749da44d40)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da3460c2-1632-413c-8a43-4d7bbe406155)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 79dbe1bd-4787-4710-b0c9-cec00c8f01b0)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f23b6168-845d-41ec-b1f7-914c57d4f627))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a367a4f4-d415-420b-b7b3-6d74c6c178d7))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c01bbe4-b045-4a44-b46c-f80d9c84c5d2))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e10fe46-c851-48f2-a9f0-aa3c35cfcf69))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 71e2bc4b-abe6-4a03-bb86-99386fa15581))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b0b6ef92-5322-453b-9fd3-bfd9ff935b4c))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e41f47e4-f5fe-42ba-873c-f5509c272c36))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15d5b087-9a83-4c8e-a60c-d0bd00198caf))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8de53c91-a38f-4dd7-89b5-adf5cc315828))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19f9b9b7-c9bf-4ae6-a664-01b173c302a4))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 67dfddae-950b-4eeb-b0ca-a67d49266bd7))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6cd3228e-a2cd-4a2b-90a4-c12ebed774f2))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "unconnected-(D5-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 6f1bd4e4-1fc9-4822-be02-70b22dd82399))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "unconnected-(D5-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp d4d15494-a9c8-41cc-8e13-444d9f576e7f))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_QFP:LQFP-64_10x10mm_P0.5mm" (layer "F.Cu")
    (tstamp 4e523172-5cd4-4891-9552-a08aa76383b7)
    (at 157.25 62.425)
    (descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Sheetfile" "ftdi.kicad_sch")
    (property "Sheetname" "ftdi")
    (property "ki_description" "Hi Speed Quad Channel USB UART/FIFO, LQFP/QFN-64")
    (property "ki_keywords" "FTDI USB Quad UART FIFO")
    (path "/95d69960-5749-4bf0-ba13-8cc427d1e8e9/7d8f97cc-69be-4689-8157-fafee1c14082")
    (attr smd)
    (fp_text reference "U20" (at 0 -7.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4dcb915e-762c-42a7-a5bb-e6eec03f8a3a)
    )
    (fp_text value "FT4232H" (at 0 7.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d903042-9c57-49e2-84e6-037ea7cd3ca9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f76f9127-7827-4f78-8cda-250831aa04a6)
    )
    (fp_line (start -5.11 -5.11) (end -5.11 -4.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1aa935d5-03ea-4acd-9e34-b1fa7b24e4c2))
    (fp_line (start -5.11 -4.16) (end -6.45 -4.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 87dce046-34a0-4451-b3a4-b59770d829ff))
    (fp_line (start -5.11 5.11) (end -5.11 4.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9905713e-742f-45db-98ab-c525761feb64))
    (fp_line (start -4.16 -5.11) (end -5.11 -5.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 02ea717c-c493-478a-9abb-952f4496aa64))
    (fp_line (start -4.16 5.11) (end -5.11 5.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eecfbee2-9b3e-48bb-b876-3d1756a81dc3))
    (fp_line (start 4.16 -5.11) (end 5.11 -5.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7b10a819-9ff4-4e5c-bfb7-0b6963912de3))
    (fp_line (start 4.16 5.11) (end 5.11 5.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 804959be-18d8-4914-a961-edf205fea529))
    (fp_line (start 5.11 -5.11) (end 5.11 -4.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 506a366a-8bce-40da-96c7-d0a05ed451e6))
    (fp_line (start 5.11 5.11) (end 5.11 4.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7ab2cd8-c620-43a3-ab92-926d52c60276))
    (fp_line (start -6.7 -4.15) (end -6.7 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 622abb49-ad45-47d4-ac1b-5ac51717231a))
    (fp_line (start -6.7 4.15) (end -6.7 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e438a01-c734-447e-8de0-511bf6594332))
    (fp_line (start -5.25 -5.25) (end -5.25 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f961de57-0061-4f39-ba7d-8c482998c95f))
    (fp_line (start -5.25 -4.15) (end -6.7 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8422c896-2828-451c-8048-8af6c82f167a))
    (fp_line (start -5.25 4.15) (end -6.7 4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 943959b7-9d8f-4f5f-a74b-f0e4822a7e47))
    (fp_line (start -5.25 5.25) (end -5.25 4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 847dae3d-eddd-49a6-bf9c-7e5f0b7799f4))
    (fp_line (start -4.15 -6.7) (end -4.15 -5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b5c1fb3-021c-47a1-8dfd-c3d148369535))
    (fp_line (start -4.15 -5.25) (end -5.25 -5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3469dfdb-8868-438d-ab75-6d2fabddabe4))
    (fp_line (start -4.15 5.25) (end -5.25 5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 609352ad-2291-4436-bd82-fa3991d74df4))
    (fp_line (start -4.15 6.7) (end -4.15 5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 570034d0-1911-4751-b669-3ea522987e6a))
    (fp_line (start 0 -6.7) (end -4.15 -6.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9afc17a-4d1b-4f86-a272-95b6ced76c00))
    (fp_line (start 0 -6.7) (end 4.15 -6.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa42fb5f-fa0a-46e8-b7d4-718d03b2cbdd))
    (fp_line (start 0 6.7) (end -4.15 6.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9b6de7f2-4bf9-4100-9068-0ddea37288eb))
    (fp_line (start 0 6.7) (end 4.15 6.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 68f5a2f9-2564-44bb-8b50-02ecb094e6bd))
    (fp_line (start 4.15 -6.7) (end 4.15 -5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76daa3c8-9833-43c7-b0f5-46c381a5b455))
    (fp_line (start 4.15 -5.25) (end 5.25 -5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp db964ecd-4f93-4dc9-9013-039a249763af))
    (fp_line (start 4.15 5.25) (end 5.25 5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7a4ec4c0-a77f-4e0c-9dae-98a47364ff00))
    (fp_line (start 4.15 6.7) (end 4.15 5.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f1affc1d-7445-460b-a661-5034a8cc54bd))
    (fp_line (start 5.25 -5.25) (end 5.25 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 994eac18-e64e-4b13-96de-5a64e6283372))
    (fp_line (start 5.25 -4.15) (end 6.7 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9b34f62c-7295-407b-870a-99f2c3733001))
    (fp_line (start 5.25 4.15) (end 6.7 4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f5375d00-aa19-4152-a25f-dd5bdac4a632))
    (fp_line (start 5.25 5.25) (end 5.25 4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 52c84716-ee86-4f51-ae60-37bc8864cbb0))
    (fp_line (start 6.7 -4.15) (end 6.7 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 537ea2c2-1dbd-4978-be6a-752d44f51344))
    (fp_line (start 6.7 4.15) (end 6.7 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1a2e69a7-a166-4e06-a604-96690f4ae320))
    (fp_line (start -5 -4) (end -4 -5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b864ad1-5e6b-4f36-913d-5c7e3c992dbf))
    (fp_line (start -5 5) (end -5 -4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ab25b268-89df-4ff5-a213-2bf8663436f3))
    (fp_line (start -4 -5) (end 5 -5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6ca41aef-c82d-45c3-a4df-1327cf69d7a6))
    (fp_line (start 5 -5) (end 5 5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 83a4241c-9b9d-45e8-8a08-3534a81042a7))
    (fp_line (start 5 5) (end -5 5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4737ca2c-0990-4191-8963-40701c420c77))
    (pad "1" smd roundrect (at -5.675 -3.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 863 "unconnected-(U20-GND-Pad1)") (pinfunction "GND") (pintype "power_in") (tstamp 4f3a9b4f-dcaa-413f-b773-87768aa47602))
    (pad "2" smd roundrect (at -5.675 -3.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 864 "unconnected-(U20-OSCI-Pad2)") (pinfunction "OSCI") (pintype "input") (tstamp 1834512a-b0ff-440f-8ee4-9a75201e08d5))
    (pad "3" smd roundrect (at -5.675 -2.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 865 "unconnected-(U20-OSCO-Pad3)") (pinfunction "OSCO") (pintype "output") (tstamp 402fbf01-b442-4385-b5da-d90e77c10558))
    (pad "4" smd roundrect (at -5.675 -2.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 866 "unconnected-(U20-VPHY-Pad4)") (pinfunction "VPHY") (pintype "power_in") (tstamp 6ad2b925-8128-434b-800a-e29f0e0f7a2b))
    (pad "5" smd roundrect (at -5.675 -1.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 867 "unconnected-(U20-GND-Pad5)") (pinfunction "GND") (pintype "power_in") (tstamp 58cb17e6-9e39-49f8-ab6a-37e001836040))
    (pad "6" smd roundrect (at -5.675 -1.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 868 "unconnected-(U20-REF-Pad6)") (pinfunction "REF") (pintype "input") (tstamp 26d1ce72-52d9-4f2a-96b0-419365b3d657))
    (pad "7" smd roundrect (at -5.675 -0.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 869 "unconnected-(U20-DM-Pad7)") (pinfunction "DM") (pintype "bidirectional") (tstamp b1860aa3-8b6b-4e62-98a4-e968df5ac8f1))
    (pad "8" smd roundrect (at -5.675 -0.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 870 "unconnected-(U20-DP-Pad8)") (pinfunction "DP") (pintype "bidirectional") (tstamp 1b55aae4-6a71-47ff-a775-e64d127892a0))
    (pad "9" smd roundrect (at -5.675 0.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 871 "unconnected-(U20-VPLL-Pad9)") (pinfunction "VPLL") (pintype "power_in") (tstamp a0190dcf-831e-4129-8ca2-3853498e0132))
    (pad "10" smd roundrect (at -5.675 0.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 872 "unconnected-(U20-AGND-Pad10)") (pinfunction "AGND") (pintype "power_in") (tstamp da1f11d4-b458-4845-9977-7d5b06ad4a53))
    (pad "11" smd roundrect (at -5.675 1.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 873 "unconnected-(U20-GND-Pad11)") (pinfunction "GND") (pintype "power_in") (tstamp aefdc2e8-121a-4c8b-8dda-2340114bf5bd))
    (pad "12" smd roundrect (at -5.675 1.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 874 "unconnected-(U20-VCORE-Pad12)") (pinfunction "VCORE") (pintype "power_in") (tstamp 9e9a9176-db88-4b5b-a0d2-f672ad778732))
    (pad "13" smd roundrect (at -5.675 2.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 875 "unconnected-(U20-TEST-Pad13)") (pinfunction "TEST") (pintype "input") (tstamp c76c8287-6953-435a-8761-37e999c9129a))
    (pad "14" smd roundrect (at -5.675 2.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 876 "unconnected-(U20-~{RESET}-Pad14)") (pinfunction "~{RESET}") (pintype "input") (tstamp ae0bc7bb-8a34-4bda-b173-43b2edc7879f))
    (pad "15" smd roundrect (at -5.675 3.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 877 "unconnected-(U20-GND-Pad15)") (pinfunction "GND") (pintype "power_in") (tstamp b4b9d447-9809-4693-b44f-fdc811bde746))
    (pad "16" smd roundrect (at -5.675 3.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 878 "unconnected-(U20-ADBUS0-Pad16)") (pinfunction "ADBUS0") (pintype "bidirectional") (tstamp 66204e1d-2ddf-4190-b520-200aa8fa2347))
    (pad "17" smd roundrect (at -3.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 879 "unconnected-(U20-ADBUS1-Pad17)") (pinfunction "ADBUS1") (pintype "bidirectional") (tstamp d6331a1e-019e-42d6-9bae-97a9d77920bc))
    (pad "18" smd roundrect (at -3.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 880 "unconnected-(U20-ADBUS2-Pad18)") (pinfunction "ADBUS2") (pintype "bidirectional") (tstamp e064fb38-ab45-4490-953e-8811591eef37))
    (pad "19" smd roundrect (at -2.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 881 "unconnected-(U20-ADBUS3-Pad19)") (pinfunction "ADBUS3") (pintype "bidirectional") (tstamp 9f81a83b-f639-4f01-8001-582e830c7d85))
    (pad "20" smd roundrect (at -2.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 882 "unconnected-(U20-VCCIO-Pad20)") (pinfunction "VCCIO") (pintype "power_in") (tstamp b552d1ae-838c-4a2a-bc9a-b8ba44e89dd2))
    (pad "21" smd roundrect (at -1.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 883 "unconnected-(U20-ADBUS4-Pad21)") (pinfunction "ADBUS4") (pintype "bidirectional") (tstamp b0943fff-6193-4a8c-97b7-1573ae5f7866))
    (pad "22" smd roundrect (at -1.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 884 "unconnected-(U20-ADBUS5-Pad22)") (pinfunction "ADBUS5") (pintype "bidirectional") (tstamp c4b2ce53-1945-4211-858f-4c0054dd9be3))
    (pad "23" smd roundrect (at -0.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 885 "unconnected-(U20-ADBUS6-Pad23)") (pinfunction "ADBUS6") (pintype "bidirectional") (tstamp bd0bfdcc-190b-4478-a9b2-5bfef6d2aee4))
    (pad "24" smd roundrect (at -0.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 886 "unconnected-(U20-ADBUS7-Pad24)") (pinfunction "ADBUS7") (pintype "bidirectional") (tstamp 5ea4f23e-ef75-4c11-9432-03e80663060c))
    (pad "25" smd roundrect (at 0.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 887 "unconnected-(U20-GND-Pad25)") (pinfunction "GND") (pintype "power_in") (tstamp 72fb66dd-9669-46c0-8364-2125e0d3a8f7))
    (pad "26" smd roundrect (at 0.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 888 "unconnected-(U20-BDBUS0-Pad26)") (pinfunction "BDBUS0") (pintype "bidirectional") (tstamp 91b6b4b6-c4f3-481b-83d4-8d5508de85fe))
    (pad "27" smd roundrect (at 1.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 889 "unconnected-(U20-BDBUS1-Pad27)") (pinfunction "BDBUS1") (pintype "bidirectional") (tstamp 4bf87581-f070-4d44-9cdb-6072cda8a43b))
    (pad "28" smd roundrect (at 1.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 890 "unconnected-(U20-BDBUS2-Pad28)") (pinfunction "BDBUS2") (pintype "bidirectional") (tstamp 99f50f64-4c39-4deb-8819-0e24daf7cdd9))
    (pad "29" smd roundrect (at 2.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 891 "unconnected-(U20-BDBUS3-Pad29)") (pinfunction "BDBUS3") (pintype "bidirectional") (tstamp f229a004-1cae-435f-b25f-9543ce68a368))
    (pad "30" smd roundrect (at 2.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 892 "unconnected-(U20-BDBUS4-Pad30)") (pinfunction "BDBUS4") (pintype "bidirectional") (tstamp 0df15dba-01f7-4223-8dea-c26414cccebd))
    (pad "31" smd roundrect (at 3.25 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 893 "unconnected-(U20-VCCIO-Pad31)") (pinfunction "VCCIO") (pintype "power_in") (tstamp 6e8b810d-04b9-4095-80a6-d9f7dff3af37))
    (pad "32" smd roundrect (at 3.75 5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 894 "unconnected-(U20-BDBUS5-Pad32)") (pinfunction "BDBUS5") (pintype "bidirectional") (tstamp fa96d064-125f-4a62-8315-3f05fd8203e3))
    (pad "33" smd roundrect (at 5.675 3.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 895 "unconnected-(U20-BDBUS6-Pad33)") (pinfunction "BDBUS6") (pintype "bidirectional") (tstamp 6d67c2b5-ced9-4bf8-a914-121222a8be7b))
    (pad "34" smd roundrect (at 5.675 3.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 896 "unconnected-(U20-BDBUS7-Pad34)") (pinfunction "BDBUS7") (pintype "bidirectional") (tstamp 57f893ff-a73c-4d58-bd93-c968a1399fb3))
    (pad "35" smd roundrect (at 5.675 2.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 897 "unconnected-(U20-GND-Pad35)") (pinfunction "GND") (pintype "power_in") (tstamp 68f813d9-d703-48d6-bda8-6b3ce0bdd1ab))
    (pad "36" smd roundrect (at 5.675 2.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 898 "unconnected-(U20-~{SUSPEND}-Pad36)") (pinfunction "~{SUSPEND}") (pintype "output") (tstamp fec721c0-a621-4111-9bd3-5b0308565f2b))
    (pad "37" smd roundrect (at 5.675 1.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 899 "unconnected-(U20-VCORE-Pad37)") (pinfunction "VCORE") (pintype "power_in") (tstamp 682d54f0-43c0-47a1-a3e8-888b9045df5e))
    (pad "38" smd roundrect (at 5.675 1.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 900 "unconnected-(U20-CDBUS0-Pad38)") (pinfunction "CDBUS0") (pintype "bidirectional") (tstamp 74d5cd50-27b2-4917-a496-e520fcffec43))
    (pad "39" smd roundrect (at 5.675 0.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 901 "unconnected-(U20-CDBUS1-Pad39)") (pinfunction "CDBUS1") (pintype "bidirectional") (tstamp f6743176-12f0-4f5a-80c2-bebd7d6c6d00))
    (pad "40" smd roundrect (at 5.675 0.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 902 "unconnected-(U20-CDBUS2-Pad40)") (pinfunction "CDBUS2") (pintype "bidirectional") (tstamp c96bac07-a726-4eb4-8bad-1b90718851be))
    (pad "41" smd roundrect (at 5.675 -0.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 903 "unconnected-(U20-CDBUS3-Pad41)") (pinfunction "CDBUS3") (pintype "bidirectional") (tstamp 0c8ff341-b777-497e-af3a-baffb2fec18e))
    (pad "42" smd roundrect (at 5.675 -0.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 904 "unconnected-(U20-VCCIO-Pad42)") (pinfunction "VCCIO") (pintype "power_in") (tstamp 634fe773-9192-4c6c-a29a-536e46a6a643))
    (pad "43" smd roundrect (at 5.675 -1.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 905 "unconnected-(U20-CDBUS4-Pad43)") (pinfunction "CDBUS4") (pintype "bidirectional") (tstamp 9d9e77e1-2498-4f04-8952-9c12dc2b523c))
    (pad "44" smd roundrect (at 5.675 -1.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 906 "unconnected-(U20-CDBUS5-Pad44)") (pinfunction "CDBUS5") (pintype "bidirectional") (tstamp b04965d9-985f-483b-a1d0-28b975739d1f))
    (pad "45" smd roundrect (at 5.675 -2.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 907 "unconnected-(U20-CDBUS6-Pad45)") (pinfunction "CDBUS6") (pintype "bidirectional") (tstamp f6789806-59df-46cc-b9da-8c96c7f82fc7))
    (pad "46" smd roundrect (at 5.675 -2.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 908 "unconnected-(U20-CDBUS7-Pad46)") (pinfunction "CDBUS7") (pintype "bidirectional") (tstamp 91012a9a-0b57-466e-9caa-101ffc54cc03))
    (pad "47" smd roundrect (at 5.675 -3.25) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 909 "unconnected-(U20-GND-Pad47)") (pinfunction "GND") (pintype "power_in") (tstamp f594400f-f489-486a-bc7a-cef28a289e16))
    (pad "48" smd roundrect (at 5.675 -3.75) (size 1.55 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 910 "unconnected-(U20-DDBUS0-Pad48)") (pinfunction "DDBUS0") (pintype "bidirectional") (tstamp b2f335a4-0315-455c-b8b0-de3554d5c597))
    (pad "49" smd roundrect (at 3.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 911 "unconnected-(U20-VREGOUT-Pad49)") (pinfunction "VREGOUT") (pintype "power_out") (tstamp f7ee8dff-5833-4259-9d43-c5e7c2654a18))
    (pad "50" smd roundrect (at 3.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 912 "unconnected-(U20-VREGIN-Pad50)") (pinfunction "VREGIN") (pintype "power_in") (tstamp d6304101-b0a9-4714-9e5f-385104250753))
    (pad "51" smd roundrect (at 2.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 913 "unconnected-(U20-GND-Pad51)") (pinfunction "GND") (pintype "power_in") (tstamp 17e32050-1cfe-446a-b32c-2220e9f6fcb5))
    (pad "52" smd roundrect (at 2.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 914 "unconnected-(U20-DDBUS1-Pad52)") (pinfunction "DDBUS1") (pintype "bidirectional") (tstamp 8728acd6-9765-43c3-b78a-2842a6b47b90))
    (pad "53" smd roundrect (at 1.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 915 "unconnected-(U20-DDBUS2-Pad53)") (pinfunction "DDBUS2") (pintype "bidirectional") (tstamp c1bc9df4-0f31-4751-99f2-94a67a99dee9))
    (pad "54" smd roundrect (at 1.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 916 "unconnected-(U20-DDBUS3-Pad54)") (pinfunction "DDBUS3") (pintype "bidirectional") (tstamp 0e2c5bda-df8d-42a7-8b98-9e6dc6071e7b))
    (pad "55" smd roundrect (at 0.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 917 "unconnected-(U20-DDBUS4-Pad55)") (pinfunction "DDBUS4") (pintype "bidirectional") (tstamp e7d9c219-f7ce-44b2-a9e2-83c91eb7db1b))
    (pad "56" smd roundrect (at 0.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 918 "unconnected-(U20-VCCIO-Pad56)") (pinfunction "VCCIO") (pintype "power_in") (tstamp e3d3885f-28c7-4f55-b9a9-a4a2fa606b6d))
    (pad "57" smd roundrect (at -0.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 919 "unconnected-(U20-DDBUS5-Pad57)") (pinfunction "DDBUS5") (pintype "bidirectional") (tstamp 7de91f0b-6163-4ba4-9f0f-902760311075))
    (pad "58" smd roundrect (at -0.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 920 "unconnected-(U20-DDBUS6-Pad58)") (pinfunction "DDBUS6") (pintype "bidirectional") (tstamp ad42bf5f-4360-4b9a-9529-6f10d88b47bd))
    (pad "59" smd roundrect (at -1.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 921 "unconnected-(U20-DDBUS7-Pad59)") (pinfunction "DDBUS7") (pintype "bidirectional") (tstamp 291b8f87-c21e-4cde-a43c-451365ecec74))
    (pad "60" smd roundrect (at -1.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 922 "unconnected-(U20-~{PWREN}-Pad60)") (pinfunction "~{PWREN}") (pintype "output") (tstamp b32fed4a-b347-4820-a611-ba65d8ab0cd7))
    (pad "61" smd roundrect (at -2.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 923 "unconnected-(U20-EEDATA-Pad61)") (pinfunction "EEDATA") (pintype "bidirectional") (tstamp 1bae07fa-19a7-48d6-95aa-290cce558bc4))
    (pad "62" smd roundrect (at -2.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 924 "unconnected-(U20-EECLK-Pad62)") (pinfunction "EECLK") (pintype "output") (tstamp c1564905-c574-4933-b0f2-5ede5f15e7a3))
    (pad "63" smd roundrect (at -3.25 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 925 "unconnected-(U20-EECS-Pad63)") (pinfunction "EECS") (pintype "output") (tstamp fbf6fb6f-19ed-45d4-92c1-278d51395c51))
    (pad "64" smd roundrect (at -3.75 -5.675) (size 0.3 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 926 "unconnected-(U20-VCORE-Pad64)") (pinfunction "VCORE") (pintype "power_in") (tstamp 822ff076-7185-4c26-ac9c-9019a6853c26))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_RJ:BEL_SI-50170-F" (layer "F.Cu")
    (tstamp 5b04a9fb-5630-4241-9344-512a9a79563d)
    (at 166.5 102.75)
    (property "MANUFACTURER" "Bel Fuse")
    (property "MAXIMUM_PACKAGE_HEIGHT" "13.97mm")
    (property "PARTREV" "07")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "ethernet.kicad_sch")
    (property "Sheetname" "ethernet")
    (path "/0e586220-674f-4460-8339-5e3e7edc244c/7a9f0dee-a13e-4b44-af95-8ed3667b5089")
    (attr through_hole)
    (fp_text reference "J3" (at -4.445 -15.875) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c48b539-f9e0-458d-80ab-43eadc86f1dc)
    )
    (fp_text value "SI-50170-F" (at 1.27 12.065) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dfbeabbe-15d9-46cd-a0af-62ce45a5e815)
    )
    (fp_line (start -8.065 -14.61) (end -6.5 -14.61)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 258bcd00-94c8-4d08-ab44-d05af649c926))
    (fp_line (start -8.065 -4.8) (end -8.065 -14.61)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp c082d68e-8ce4-473b-83d4-3f25db7756e5))
    (fp_line (start -8.065 10.79) (end -8.065 -1.23)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp a9760c70-b4df-4d2b-b638-d6e1704fd03c))
    (fp_line (start -1.85 -14.61) (end 1.9 -14.61)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 2708d431-65b3-4d7f-b12f-0872b7935b91))
    (fp_line (start 6.6 -14.61) (end 8.065 -14.61)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 1fc1fc7c-1937-4e35-aa0c-965a105ae54e))
    (fp_line (start 8.065 -14.61) (end 8.065 -4.8)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 035e4ab5-a3e9-40eb-8e0d-379b13bea0b1))
    (fp_line (start 8.065 -1.23) (end 8.065 10.79)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 2b1a82bb-de92-4ad7-b1f3-77498c7033aa))
    (fp_line (start 8.065 10.79) (end -8.065 10.79)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp a21d35b4-7c4e-4c16-8281-d065d11b1804))
    (fp_circle (center 8.88 -8.84) (end 8.98 -8.84)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.SilkS") (tstamp 6b5f6c06-ffeb-49b4-8eea-68539b62f9f2))
    (fp_line (start -9.24 -4.535) (end -8.315 -4.535)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 436792a0-e08d-4e88-aab1-3982e1787d11))
    (fp_line (start -9.24 -1.56) (end -9.24 -4.535)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0889238e-5a3d-4922-b9eb-163d0d551f6e))
    (fp_line (start -8.315 -14.86) (end 8.315 -14.86)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 334c7521-cad2-4fb8-9789-eebed08f80ae))
    (fp_line (start -8.315 -4.535) (end -8.315 -14.86)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 578e68b0-83fc-4ab9-bc8a-d7a345e81632))
    (fp_line (start -8.315 -1.56) (end -9.24 -1.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 088f4a3e-ab08-47a4-acf4-52d28ca52a50))
    (fp_line (start -8.315 11.04) (end -8.315 -1.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ff74e0b0-2781-4b3c-bb04-bd513b7d07e7))
    (fp_line (start 8.315 -14.86) (end 8.315 -4.535)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 745e070c-fbc4-4d0e-af5e-343b1f207703))
    (fp_line (start 8.315 -4.535) (end 9.24 -4.535)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4da568cf-06b2-4e82-a783-6dec966409d7))
    (fp_line (start 8.315 -1.56) (end 8.315 11.04)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4d0360c2-10ab-414e-a6a9-2bcf368ce402))
    (fp_line (start 8.315 11.04) (end -8.315 11.04)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 753b6705-db63-441a-b28c-424bd872aa56))
    (fp_line (start 9.24 -4.535) (end 9.24 -1.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cdf1895d-5139-4e32-8b8c-d775efba380f))
    (fp_line (start 9.24 -1.56) (end 8.315 -1.56)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6577e23e-fd2f-4084-ae23-4c9ef2aca8eb))
    (fp_line (start -8.065 -14.61) (end 8.065 -14.61)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp c9871e32-1974-41c0-842a-60fe126d1928))
    (fp_line (start -8.065 10.79) (end -8.065 -14.61)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp d4f9c798-8fad-4a7f-a2e9-502b147bf2d9))
    (fp_line (start 8.065 -14.61) (end 8.065 10.79)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp bd691e50-b86d-47ae-a71a-d97ffb9f17bc))
    (fp_line (start 8.065 10.79) (end -8.065 10.79)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 4c2bc86c-3dd0-4919-8929-2d8c3f229702))
    (fp_circle (center 8.88 -8.84) (end 8.98 -8.84)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.Fab") (tstamp f352b1c3-e511-417c-83f2-a044c3d34a10))
    (pad "" np_thru_hole circle (at -5.715 0) (size 3.25 3.25) (drill 3.25) (layers "*.Cu" "*.Mask") (tstamp 669de933-6152-4458-b047-fc3b588c69ce))
    (pad "" np_thru_hole circle (at 5.715 0) (size 3.25 3.25) (drill 3.25) (layers "*.Cu" "*.Mask") (tstamp 0e402326-72fe-4ff8-b225-346b856751cf))
    (pad "1" thru_hole rect (at 4.445 -8.89) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(J3-P1-Pad1)") (pinfunction "P1") (pintype "passive") (solder_mask_margin 0.102) (tstamp 9aa6b706-0747-4326-8ed4-03f8f00d4398))
    (pad "2" thru_hole circle (at 3.175 -6.35) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(J3-P2-Pad2)") (pinfunction "P2") (pintype "passive") (solder_mask_margin 0.102) (tstamp 90aeffb6-ec72-425b-a868-05665fc865b2))
    (pad "3" thru_hole circle (at 1.905 -8.89) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(J3-P3-Pad3)") (pinfunction "P3") (pintype "passive") (solder_mask_margin 0.102) (tstamp 31d23418-4291-463d-a048-ed132ddd88f5))
    (pad "4" thru_hole circle (at 0.635 -6.35) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(J3-P4-Pad4)") (pinfunction "P4") (pintype "passive") (solder_mask_margin 0.102) (tstamp f5b0eceb-b7d5-4fce-a4ac-ff5c419c85f1))
    (pad "5" thru_hole circle (at -0.635 -8.89) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(J3-P5-Pad5)") (pinfunction "P5") (pintype "passive") (solder_mask_margin 0.102) (tstamp d1ab4664-b83e-4039-a44f-fc347942137a))
    (pad "6" thru_hole circle (at -1.905 -6.35) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(J3-P6-Pad6)") (pinfunction "P6") (pintype "passive") (solder_mask_margin 0.102) (tstamp cfed899c-dbd3-4325-9f55-889173d2c531))
    (pad "7" thru_hole circle (at -3.175 -8.89) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(J3-P7-Pad7)") (pinfunction "P7") (pintype "passive") (solder_mask_margin 0.102) (tstamp ab38d569-5a7d-4051-9021-410747af9a4d))
    (pad "8" thru_hole circle (at -4.445 -6.35) (size 1.478 1.478) (drill 0.97) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(J3-P8-Pad8)") (pinfunction "P8") (pintype "passive") (solder_mask_margin 0.102) (tstamp 7b92eac8-0f6d-4adc-80c5-11b019adefef))
    (pad "9" thru_hole circle (at -5.465 -13.72) (size 1.65 1.65) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(J3-Pad9)") (pintype "passive") (solder_mask_margin 0.102) (tstamp 7f16abad-d587-48b7-8b6b-80448454dc00))
    (pad "10" thru_hole circle (at -2.925 -13.72) (size 1.65 1.65) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(J3-Pad10)") (pintype "passive") (solder_mask_margin 0.102) (tstamp 8c027800-f0ca-459a-a9de-a1ef259d2378))
    (pad "11" thru_hole circle (at 2.925 -13.72) (size 1.65 1.65) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(J3-Pad11)") (pintype "passive") (solder_mask_margin 0.102) (tstamp b88602f1-6050-4856-aaed-776292182655))
    (pad "12" thru_hole circle (at 5.465 -13.72) (size 1.65 1.65) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(J3-Pad12)") (pintype "passive") (solder_mask_margin 0.102) (tstamp fd2f4a2b-5842-4068-b252-8bc88413bacb))
    (pad "S1" thru_hole circle (at -7.745 -3.05) (size 2.475 2.475) (drill 1.65) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(J3-SHIELD-PadS1)") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102) (tstamp 49f2b018-0daa-461c-a8e0-0f140ccaa2b9))
    (pad "S2" thru_hole circle (at 7.745 -3.05) (size 2.475 2.475) (drill 1.65) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(J3-SHIELD__1-PadS2)") (pinfunction "SHIELD__1") (pintype "passive") (solder_mask_margin 0.102) (tstamp 48b8c0ca-6eba-4b14-a088-3ac4a86f4653))
    (model ":KICAD7_3DMODEL_DIR:Connector_RJ.3dshapes/SI-50170-F.step"
      (offset (xyz 0 -10.75 6.75))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 5bf551de-9d05-4463-a09e-56537b4719ae)
    (at 34 27 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/dd43808a-f185-4ccc-ab39-b8c665e14aa3")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 77a12f71-8ca0-4f84-a669-50383afa7168)
    )
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5afab4d-d73a-4912-a2e5-b706f0e13fba)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 5dd7726b-176e-4fd5-9e8d-797d60a4087d)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce33215f-ca03-42c0-8bbc-374feeee88b3))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0e6790ac-4635-4e7d-94d0-0a950db7b280))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 78943e8e-8d53-4b65-a7bd-7aa68e4eee59))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d8097650-6083-44ca-88f3-54dadeb6b9ab))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fed6d22a-394f-40c0-a252-d476f7555974))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bec6f241-1541-45b1-944d-97eec26a000d))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eab23981-ee00-41df-8968-e979f85d0471))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b5e68cd-0d6d-402d-a031-8fa6fc0ea8e7))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 628d59f2-8276-40a2-a4cc-d7eb201b50ac))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e2c7edeb-c257-4da5-bbb7-fdbb314bceb4))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 572 "+3V3") (pintype "passive") (tstamp 1259875c-f544-4da1-a2b4-0ff37591255e))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 566 "/cpu/CPU_RDY") (pintype "passive") (tstamp 9c792919-3931-4bf0-b0ca-bc5cea149f71))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tstamp 5e3fb623-eb8b-4fa9-9460-3dff7e0c324b)
    (at 24 34)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/00a755e8-bac1-4912-a7b4-c06ef049a870")
    (attr through_hole)
    (fp_text reference "SW4" (at 3.25 -2) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33566109-7425-48c3-90c6-70d54e86f4fa)
    )
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d3f230d1-16d5-477f-b632-13782a7c3fa0)
    )
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1a0e632-3eae-4d22-8d7a-4d6846b0ed7d)
    )
    (fp_line (start -0.25 1.5) (end -0.25 3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7662ca47-2dd1-4aed-8d42-5c8fb6f71f06))
    (fp_line (start 1 5.5) (end 5.5 5.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4dba94d5-0b7a-45a6-bb3b-d759110cdf53))
    (fp_line (start 5.5 -1) (end 1 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3f1e2428-6cbd-481e-974d-fcc94e718dd8))
    (fp_line (start 6.75 3) (end 6.75 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e055fa7-4d9d-4706-a957-02b66c8cd6a4))
    (fp_line (start -1.5 -1.5) (end -1.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 530ae410-dcbc-46da-bfad-9ed670c56bc7))
    (fp_line (start -1.5 -1.25) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 053c4526-2d98-41ce-b9b3-46729cabf65e))
    (fp_line (start -1.5 5.75) (end -1.5 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 123916a0-cc24-4d54-be25-163b4cdbb651))
    (fp_line (start -1.5 5.75) (end -1.5 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a310230e-530b-41ad-a497-a4e76a21ff53))
    (fp_line (start -1.5 6) (end -1.25 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 654be500-ff03-489a-98c6-9eb9ccf9a27c))
    (fp_line (start -1.25 -1.5) (end 7.75 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 16292fe0-26ad-4ffa-ae35-83590220d735))
    (fp_line (start 7.75 -1.5) (end 8 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 67446a63-efc3-4037-92de-92e0cccaa634))
    (fp_line (start 7.75 6) (end -1.25 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c03c873e-a140-4c86-92e1-58170fda5285))
    (fp_line (start 7.75 6) (end 8 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad7a70f7-8e5c-45a4-a9c7-3ddf8566d8ff))
    (fp_line (start 8 -1.5) (end 8 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 47475b69-f9c7-495f-bb79-a193fedde7cd))
    (fp_line (start 8 -1.25) (end 8 5.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a03674fd-2e8b-467a-be9a-a1518ef417cc))
    (fp_line (start 8 6) (end 8 5.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5deba721-3c64-44fe-8975-0bc63e66aaf7))
    (fp_line (start 0.25 -0.75) (end 3.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bde32961-06c9-4883-9892-a98f62f19cd9))
    (fp_line (start 0.25 5.25) (end 0.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd08e915-f16d-4e52-aa87-96edb98b28e3))
    (fp_line (start 3.25 -0.75) (end 6.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b3833ee-f2cd-45dc-b5b7-c5986d0df3a1))
    (fp_line (start 6.25 -0.75) (end 6.25 5.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 81580ea0-2b89-4a67-a898-36bca8cdf221))
    (fp_line (start 6.25 5.25) (end 0.25 5.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2a6aaba1-b621-41bb-af39-0fec0f6b787e))
    (fp_circle (center 3.25 2.25) (end 1.25 2.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp dc057944-a27c-43f3-86df-51e790286c69))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 585 "GND") (pinfunction "1") (pintype "passive") (tstamp 8c109e5e-7790-41ac-b2bd-7522a7847ea4))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 585 "GND") (pinfunction "1") (pintype "passive") (tstamp 1d1efc82-a54f-4c8f-9138-ac7d2e12e5a5))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 570 "/cpu/~{CPU_NMIB}") (pinfunction "2") (pintype "passive") (tstamp c3813b4c-25ed-41dc-ac57-2305b837fc5f))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 570 "/cpu/~{CPU_NMIB}") (pinfunction "2") (pintype "passive") (tstamp ec2c20c4-78b6-4ac6-9d1d-fe8596eb1c83))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 6736c518-6124-40f2-b75a-924ab37a7f1a)
    (at 69.96 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/4fe8e3e2-20ff-434d-9204-17289a42ea52")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aad3d3b8-0b46-46a0-ac14-826f2dd45962)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2338bc34-0055-4481-ba0d-e880376792b0)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 98ab7a8f-1422-49b9-88dd-c00e72b8397f)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9453e55b-69c6-45e0-b1a9-04e0ebbd73ba))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b44d688f-0332-41cd-aa38-43c6670cb8bf))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cff4b5af-96c1-4340-9e16-43cc3f742a81))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9629a44a-3d94-4fba-9721-222439dac813))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32702432-33a9-4fbc-9ae0-d0f838ffbaa1))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 36cd7d7f-7926-4df6-b1d4-9f7618815d76))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c75a4b23-1e60-4ea4-92b1-f42122453e9b))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 57bb2fcd-15c0-41ab-bdae-5706f4609959))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1da716f-f371-4731-8880-9d914259638e))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66bcd529-ccde-4e17-b734-bc37f309a0bf))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a073cf4c-34f1-4e8a-bad4-f59b3cd63388))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 63abcab1-7348-4897-b203-65ca38fa6136))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "unconnected-(D2-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 3c110998-6e6c-4f59-b1d7-59a502049816))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "unconnected-(D2-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2bfc665f-2506-4949-b741-653fbb26b5e4))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 686765ec-178b-4326-8d5b-b4e0b02518b4)
    (at 72.55 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/5e5c290b-200b-4e49-8985-c67f2c5b3450")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f80f7854-e89a-4898-9d9b-4ea87d937a0a)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1540a521-baa6-4e47-a5f5-b0a66df01d1a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7b945f36-aef8-4fa7-9cc6-f321512c682d)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e70d7f02-ab71-4531-8af0-0252110cfdae))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f7be1eeb-3f95-4681-b73d-9cb1decb495e))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a1019215-abb1-41ab-81dd-27623271700e))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d8b67504-4f41-470b-a5a7-54de2e8acd36))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f8926654-89cc-4173-a712-45fd4cfe98a4))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bcdab39d-1b3e-4b08-a88b-0bf65c159c58))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6fac4237-7a4b-41a7-90c6-8b9b5b8b0d49))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5ac12ae-e930-467d-b37d-6c39c7595969))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 10b10e09-85b3-42ae-bbea-e10d8bcb54b6))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5a0aced8-ad4e-4aa0-afca-e08af773b5dc))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d31c749f-e84d-48c2-be43-89a13163c08a))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5616a544-fe47-4bc3-b45a-fb69c2cdc8c3))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "unconnected-(D3-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 8c9df304-a105-4d71-92ee-9cf70a46edb7))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "unconnected-(D3-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2145d34e-92c7-45b1-be9f-8ca58bd434f9))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Display_7Segment:LTS-4802B" (layer "F.Cu")
    (tstamp 6a50cfa1-7c75-4ec7-ab81-a04dcdceb880)
    (at 62.25 90.34)
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/d5138fe2-6cd8-4f18-9d2f-24f6fa6c5e83")
    (attr through_hole)
    (fp_text reference "U12" (at 0 -2.54 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cebf8871-e95d-43cd-8111-ec8e62f0b622)
    )
    (fp_text value "~" (at 3.58 13.1 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 607dd898-ad13-4dc5-ac69-029f10842f29)
    )
    (fp_text user "${REFERENCE}" (at 3.58 4.01 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 83fc08e1-4fef-48bf-b7b8-12f1418656eb)
    )
    (fp_rect (start -1.04 -1.07) (end 8.66 11.83)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp dbd23d72-e255-4520-a6dc-59ef2d4caa6c))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 751 "unconnected-(U12-CA-Pad1)") (pinfunction "CA") (pintype "passive") (tstamp b01ca673-1882-4d21-8981-3366aa0afc92))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 752 "unconnected-(U12-F-Pad2)") (pinfunction "F") (pintype "passive") (tstamp ade45f96-d453-4993-8278-64491ccba112))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 753 "unconnected-(U12-G-Pad3)") (pinfunction "G") (pintype "passive") (tstamp 6b40dd87-36b4-451d-b36d-b53e05803a16))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 754 "unconnected-(U12-E-Pad4)") (pinfunction "E") (pintype "passive") (tstamp 2a75c35f-2f98-46f7-9a5d-2c57db826297))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 755 "unconnected-(U12-D-Pad5)") (pinfunction "D") (pintype "passive") (tstamp 9d306309-c382-404a-9491-47ad4ec39b66))
    (pad "6" thru_hole circle (at 7.62 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 756 "unconnected-(U12-CA-Pad6)") (pinfunction "CA") (pintype "passive") (tstamp 9c9fb878-20d7-41d8-91c5-13bb9d541c5b))
    (pad "7" thru_hole circle (at 7.62 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 757 "unconnected-(U12-DP-Pad7)") (pinfunction "DP") (pintype "passive") (tstamp 866aeb1d-959e-4f7f-869f-49c7cdd73264))
    (pad "8" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 758 "unconnected-(U12-C-Pad8)") (pinfunction "C") (pintype "passive") (tstamp 035109b2-e5f5-44cf-a11a-802bd6fc93d7))
    (pad "9" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 759 "unconnected-(U12-B-Pad9)") (pinfunction "B") (pintype "passive") (tstamp 604c63e8-b077-4400-a972-8e10a9f174f5))
    (pad "10" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 760 "unconnected-(U12-A-Pad10)") (pinfunction "A") (pintype "passive") (tstamp b94f7894-a23f-4480-8245-9a4106bd0dd1))
    (model ":KICAD7_3DMODEL_DIR:Display_7Segment.3dshapes/LTS-4802BJR-H1_LTO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_QFP:LQFP-48_7x7mm_P0.5mm" (layer "F.Cu")
    (tstamp 6c4dd829-6b59-4ca2-8e7b-66ef7d8171f3)
    (at 166 78.75)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Sheetfile" "ethernet.kicad_sch")
    (property "Sheetname" "ethernet")
    (path "/0e586220-674f-4460-8339-5e3e7edc244c/74a2128d-f631-455c-bd88-8b2aa42595a6")
    (attr smd)
    (fp_text reference "U9" (at 0 -5.85) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c9ced88-f88a-4ef6-96c5-f024ceced7d6)
    )
    (fp_text value "~" (at 0 5.85) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7adeb551-5c0e-4929-8238-09c5faac5d5a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1649b6a3-9b17-4db0-b404-b129b0c04292)
    )
    (fp_line (start -3.61 -3.61) (end -3.61 -3.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb46e3c3-207b-4aa7-a776-7b79bf36699b))
    (fp_line (start -3.61 -3.16) (end -4.9 -3.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc7adb85-a3c0-4d7c-a17b-87f5bb477475))
    (fp_line (start -3.61 3.61) (end -3.61 3.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23f0a2c0-5d14-4789-8ba0-5281dde0eec0))
    (fp_line (start -3.16 -3.61) (end -3.61 -3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f3403b41-d6c4-4229-a1af-222ca88e8909))
    (fp_line (start -3.16 3.61) (end -3.61 3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0af82415-7e16-4872-a4dc-ce25ff3dc69b))
    (fp_line (start 3.16 -3.61) (end 3.61 -3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9300ecd2-547d-4e96-8f86-191ca7284494))
    (fp_line (start 3.16 3.61) (end 3.61 3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a15b91a0-5ed7-4ecb-a3ea-6a2305dcc3a8))
    (fp_line (start 3.61 -3.61) (end 3.61 -3.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd374e43-f884-4f39-a0ce-2bebf4074373))
    (fp_line (start 3.61 3.61) (end 3.61 3.16)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4346e705-48a2-4b2e-892f-9352ca8fea9c))
    (fp_line (start -5.15 -3.15) (end -5.15 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9e84c8e9-c4bd-4d2d-88f3-9ead41210e62))
    (fp_line (start -5.15 3.15) (end -5.15 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 421d354e-0119-493f-8824-8c39406794b4))
    (fp_line (start -3.75 -3.75) (end -3.75 -3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b80aae48-c7ff-459a-9ae4-9ea53fc9ffef))
    (fp_line (start -3.75 -3.15) (end -5.15 -3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f6a3402-3839-4aff-ad54-88ccd4e51b84))
    (fp_line (start -3.75 3.15) (end -5.15 3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ea1724b7-19ad-4cae-85cb-9946e0592fff))
    (fp_line (start -3.75 3.75) (end -3.75 3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 84ac9901-038c-4d98-b919-daa585bebecd))
    (fp_line (start -3.15 -5.15) (end -3.15 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dbf66739-7819-4c4e-8845-06e40d6d4e1e))
    (fp_line (start -3.15 -3.75) (end -3.75 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 171f6268-d607-40e2-8982-c2e81348bf0d))
    (fp_line (start -3.15 3.75) (end -3.75 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e8998fd9-77ab-41f8-999d-630c7f55661d))
    (fp_line (start -3.15 5.15) (end -3.15 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp afe6c830-c039-40c1-8241-7e96ff1e21c5))
    (fp_line (start 0 -5.15) (end -3.15 -5.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 43a335ce-669d-4610-a3f9-53d0b651bd5b))
    (fp_line (start 0 -5.15) (end 3.15 -5.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2ec4dbc6-3169-463e-a83d-129a4bd797c9))
    (fp_line (start 0 5.15) (end -3.15 5.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 48568ea4-b7e2-4eed-9aec-7c2e514b65df))
    (fp_line (start 0 5.15) (end 3.15 5.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 50354fff-2e29-4ba9-bcae-4a7104f021ad))
    (fp_line (start 3.15 -5.15) (end 3.15 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 62fb5ada-34ae-43cb-8863-a73abfc7a02a))
    (fp_line (start 3.15 -3.75) (end 3.75 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3861c721-6406-4769-af2c-b15b327d01ba))
    (fp_line (start 3.15 3.75) (end 3.75 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3fd238da-ec64-4179-b63b-b2043a22fb55))
    (fp_line (start 3.15 5.15) (end 3.15 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 31972d22-3f54-4799-9f70-39d04996159b))
    (fp_line (start 3.75 -3.75) (end 3.75 -3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6174ab9c-54c4-4daa-a256-86c1c1a86271))
    (fp_line (start 3.75 -3.15) (end 5.15 -3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f8a98294-e565-45b0-831a-a59d4b3bf8d9))
    (fp_line (start 3.75 3.15) (end 5.15 3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 71cf3fa5-f985-4765-ade9-ab07dd521397))
    (fp_line (start 3.75 3.75) (end 3.75 3.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp efc6456c-120d-4785-b6d7-625bbc5caa9c))
    (fp_line (start 5.15 -3.15) (end 5.15 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 10887c77-5ad8-4544-a8dc-9345dd980cde))
    (fp_line (start 5.15 3.15) (end 5.15 0)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b3e44e35-96a4-4b4d-99b2-7a8f6c73e140))
    (fp_line (start -3.5 -2.5) (end -2.5 -3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1ecbcb3b-93db-4fdb-94ea-43a1e11ba189))
    (fp_line (start -3.5 3.5) (end -3.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2e1b3bb-0f9d-40b7-a59f-bb73d65bbf2f))
    (fp_line (start -2.5 -3.5) (end 3.5 -3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90e95d74-878c-456f-85d5-cd75c67c6a0b))
    (fp_line (start 3.5 -3.5) (end 3.5 3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 256ea8c2-2fbb-4acd-9725-b95e02825859))
    (fp_line (start 3.5 3.5) (end -3.5 3.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d016e838-ffeb-4002-aad8-b4844f8dfada))
    (pad "1" smd roundrect (at -4.1625 -2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 683 "unconnected-(U9-GND-Pad1)") (pinfunction "GND") (pintype "passive") (tstamp 4bd259a1-161e-4c12-84b6-183912c9fc0f))
    (pad "2" smd roundrect (at -4.1625 -2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 684 "unconnected-(U9-GND-Pad2)") (pinfunction "GND") (pintype "passive") (tstamp cfd40040-1b4f-4eb7-8b79-5a14f77afef8))
    (pad "3" smd roundrect (at -4.1625 -1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 685 "unconnected-(U9-GND-Pad3)") (pinfunction "GND") (pintype "passive") (tstamp 6a4a9123-80e2-429b-925b-b8234c30d61d))
    (pad "4" smd roundrect (at -4.1625 -1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 686 "unconnected-(U9-VDD_1P2-Pad4)") (pinfunction "VDD_1P2") (pintype "power_out") (tstamp 1d810f82-2c76-408f-b971-7c4f552224bb))
    (pad "5" smd roundrect (at -4.1625 -0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 687 "unconnected-(U9-NC-Pad5)") (pinfunction "NC") (pintype "no_connect") (tstamp 0dd94193-b6d0-48a8-8c2c-81e152a5bfc6))
    (pad "6" smd roundrect (at -4.1625 -0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 688 "unconnected-(U9-NC-Pad6)") (pinfunction "NC") (pintype "no_connect") (tstamp ee41cd5a-a030-4548-bf51-2f638e9f9532))
    (pad "7" smd roundrect (at -4.1625 0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 689 "unconnected-(U9-VDDA_3P3-Pad7)") (pinfunction "VDDA_3P3") (pintype "power_out") (tstamp df2d7237-0a13-4599-91b0-df5a0123e8b1))
    (pad "8" smd roundrect (at -4.1625 0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 690 "unconnected-(U9-NC-Pad8)") (pinfunction "NC") (pintype "no_connect") (tstamp d245b865-f630-432d-b413-79d4ca57a8ef))
    (pad "9" smd roundrect (at -4.1625 1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 691 "unconnected-(U9-RXM-Pad9)") (pinfunction "RXM") (pintype "bidirectional") (tstamp 3f6e521f-936b-475c-840b-d004fdc00053))
    (pad "10" smd roundrect (at -4.1625 1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 692 "unconnected-(U9-RXP-Pad10)") (pinfunction "RXP") (pintype "bidirectional") (tstamp 7c4a6977-2016-4954-ad90-4ee38e4762ba))
    (pad "11" smd roundrect (at -4.1625 2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 693 "unconnected-(U9-TXM-Pad11)") (pinfunction "TXM") (pintype "bidirectional") (tstamp 5c7cf6f5-3535-406a-b8bb-4eb6fadf2e6b))
    (pad "12" smd roundrect (at -4.1625 2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 694 "unconnected-(U9-TXP-Pad12)") (pinfunction "TXP") (pintype "bidirectional") (tstamp 6c7425ad-5708-4477-aed5-c572b87214dc))
    (pad "13" smd roundrect (at -2.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 695 "unconnected-(U9-GND-Pad13)") (pinfunction "GND") (pintype "passive") (tstamp 3ccc8d9d-8701-4fd7-a523-705415296114))
    (pad "14" smd roundrect (at -2.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 696 "unconnected-(U9-XO-Pad14)") (pinfunction "XO") (pintype "output") (tstamp 8e348915-5ff1-4b6a-a4fe-baa32b57853f))
    (pad "15" smd roundrect (at -1.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 697 "unconnected-(U9-XI-Pad15)") (pinfunction "XI") (pintype "input") (tstamp 6fca0f58-e907-4da9-9d00-3c11068231e8))
    (pad "16" smd roundrect (at -1.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 698 "unconnected-(U9-REXT-Pad16)") (pinfunction "REXT") (pintype "input") (tstamp b3970704-873d-48f0-93a3-fa0b65e66e4a))
    (pad "17" smd roundrect (at -0.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 699 "unconnected-(U9-GND-Pad17)") (pinfunction "GND") (pintype "passive") (tstamp 2d1b2341-bcc6-4630-90e7-524004ed22c5))
    (pad "18" smd roundrect (at -0.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 700 "unconnected-(U9-MDIO-Pad18)") (pinfunction "MDIO") (pintype "bidirectional") (tstamp 5a9387ba-2fa9-4d1c-9007-4527baa21c3a))
    (pad "19" smd roundrect (at 0.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 701 "unconnected-(U9-MDC-Pad19)") (pinfunction "MDC") (pintype "input") (tstamp 12bbe4bb-c86d-4199-a3b3-9c22635fbec5))
    (pad "20" smd roundrect (at 0.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 702 "unconnected-(U9-RXD3_PHYAD0-Pad20)") (pinfunction "RXD3_PHYAD0") (pintype "bidirectional") (tstamp 08e47df1-15f1-45f0-bd58-be5f15a2853f))
    (pad "21" smd roundrect (at 1.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 703 "unconnected-(U9-RXD2_PHYAD1-Pad21)") (pinfunction "RXD2_PHYAD1") (pintype "bidirectional") (tstamp 36cf487d-a0a4-4617-aed6-743fc2bed768))
    (pad "22" smd roundrect (at 1.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 704 "unconnected-(U9-RXD1_PHYAD2-Pad22)") (pinfunction "RXD1_PHYAD2") (pintype "bidirectional") (tstamp 6df45579-a417-473c-90bb-6076a0c0cf30))
    (pad "23" smd roundrect (at 2.25 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 705 "unconnected-(U9-RXD0_DUPLEX-Pad23)") (pinfunction "RXD0_DUPLEX") (pintype "bidirectional") (tstamp e6da29f5-ec7c-4cf7-abae-ff86c0fd45d1))
    (pad "24" smd roundrect (at 2.75 4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 706 "unconnected-(U9-GND-Pad24)") (pinfunction "GND") (pintype "passive") (tstamp 8ea02a69-c71f-4b4e-aae9-3e0f96965b77))
    (pad "25" smd roundrect (at 4.1625 2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 707 "unconnected-(U9-VDDIO-Pad25)") (pinfunction "VDDIO") (pintype "power_in") (tstamp 501362f4-287a-4dec-ae22-51c116425b26))
    (pad "26" smd roundrect (at 4.1625 2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 708 "unconnected-(U9-NC-Pad26)") (pinfunction "NC") (pintype "no_connect") (tstamp a6be5264-5dd1-49ce-b46e-80b036bdf136))
    (pad "27" smd roundrect (at 4.1625 1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 709 "unconnected-(U9-RXDV_CONFIG2-Pad27)") (pinfunction "RXDV_CONFIG2") (pintype "bidirectional") (tstamp 610e851f-e4ac-46bf-a74a-83216b131927))
    (pad "28" smd roundrect (at 4.1625 1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 710 "unconnected-(U9-RXC_B-CAST-OFF-Pad28)") (pinfunction "RXC_B-CAST-OFF") (pintype "bidirectional") (tstamp 17bb7509-f453-4a98-876b-80f7e73ffa70))
    (pad "29" smd roundrect (at 4.1625 0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 711 "unconnected-(U9-RXER_ISO-Pad29)") (pinfunction "RXER_ISO") (pintype "bidirectional") (tstamp d34d5c6d-5db5-440e-984e-0a9afdd21450))
    (pad "30" smd roundrect (at 4.1625 0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 712 "unconnected-(U9-GND-Pad30)") (pinfunction "GND") (pintype "passive") (tstamp 768be68d-3b74-47f5-950c-68b4192d39a1))
    (pad "31" smd roundrect (at 4.1625 -0.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 713 "unconnected-(U9-VDD_1P2-Pad31)") (pinfunction "VDD_1P2") (pintype "power_out") (tstamp b41e74eb-82b5-4308-9eba-cd564e812d70))
    (pad "32" smd roundrect (at 4.1625 -0.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 714 "unconnected-(U9-INTRP_NAND-TREE-Pad32)") (pinfunction "INTRP_NAND-TREE") (pintype "bidirectional") (tstamp d6f7b7bf-80f5-454d-94e8-d70f8a20476c))
    (pad "33" smd roundrect (at 4.1625 -1.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 715 "unconnected-(U9-TXC-Pad33)") (pinfunction "TXC") (pintype "bidirectional") (tstamp 61c94c65-db80-40b4-971b-20ca56ca4757))
    (pad "34" smd roundrect (at 4.1625 -1.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 716 "unconnected-(U9-TXEN-Pad34)") (pinfunction "TXEN") (pintype "input") (tstamp b69658ff-8a02-497f-9a11-c76add3c6b77))
    (pad "35" smd roundrect (at 4.1625 -2.25) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 717 "unconnected-(U9-TXD0-Pad35)") (pinfunction "TXD0") (pintype "input") (tstamp 6382b2a0-c22f-4cc6-8df3-9d58b13a3fef))
    (pad "36" smd roundrect (at 4.1625 -2.75) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 718 "unconnected-(U9-TXD1-Pad36)") (pinfunction "TXD1") (pintype "input") (tstamp ad5a0c33-347b-410e-916c-077ccd721603))
    (pad "37" smd roundrect (at 2.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 719 "unconnected-(U9-GND-Pad37)") (pinfunction "GND") (pintype "passive") (tstamp 58582bd5-4ff6-494b-8e10-b26c42a2a92c))
    (pad "38" smd roundrect (at 2.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 720 "unconnected-(U9-TXD2-Pad38)") (pinfunction "TXD2") (pintype "input") (tstamp d4de885d-b913-4592-8ac5-1a5db19ddf16))
    (pad "39" smd roundrect (at 1.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 721 "unconnected-(U9-TXD3-Pad39)") (pinfunction "TXD3") (pintype "input") (tstamp b1543031-f077-4c3e-8562-99ed6837eb61))
    (pad "40" smd roundrect (at 1.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 722 "unconnected-(U9-COL_CONFIG0-Pad40)") (pinfunction "COL_CONFIG0") (pintype "bidirectional") (tstamp 5d4e5878-dc84-4b9b-9095-868d976f380d))
    (pad "41" smd roundrect (at 0.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 723 "unconnected-(U9-CRS_CONFIG1-Pad41)") (pinfunction "CRS_CONFIG1") (pintype "bidirectional") (tstamp eed69906-c957-45cd-92d4-e986577d9efb))
    (pad "42" smd roundrect (at 0.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 724 "unconnected-(U9-LED0_NWAYEN-Pad42)") (pinfunction "LED0_NWAYEN") (pintype "bidirectional") (tstamp d3195f67-6fe6-4afc-b0d8-2a715abf21eb))
    (pad "43" smd roundrect (at -0.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 725 "unconnected-(U9-LED1_SPEED-Pad43)") (pinfunction "LED1_SPEED") (pintype "bidirectional") (tstamp a8f0ed12-bfbf-4487-ba90-3db20e493661))
    (pad "44" smd roundrect (at -0.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 726 "unconnected-(U9-TEST_NC-Pad44)") (pinfunction "TEST_NC") (pintype "input") (tstamp bc4f13a3-3754-4d5d-840d-99d24a9aed11))
    (pad "45" smd roundrect (at -1.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 727 "unconnected-(U9-NC-Pad45)") (pinfunction "NC") (pintype "no_connect") (tstamp 3af4775c-9532-419b-8730-924d22c9b9fe))
    (pad "46" smd roundrect (at -1.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 728 "unconnected-(U9-NC-Pad46)") (pinfunction "NC") (pintype "no_connect") (tstamp 01ca5aaa-6c2c-4a0a-b14f-dafbd8ae7844))
    (pad "47" smd roundrect (at -2.25 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 729 "unconnected-(U9-RST#-Pad47)") (pinfunction "RST#") (pintype "input") (tstamp 314746de-a94f-407f-9348-55c31b61b196))
    (pad "48" smd roundrect (at -2.75 -4.1625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 730 "unconnected-(U9-NC-Pad48)") (pinfunction "NC") (pintype "no_connect") (tstamp 58c95ddc-695c-4d2e-970e-33f6e1248a55))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tstamp 836ed7d5-fab6-401e-9e35-d2e1a3695a96)
    (at 139.2 48.4)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Sheetfile" "ftdi.kicad_sch")
    (property "Sheetname" "ftdi")
    (path "/95d69960-5749-4bf0-ba13-8cc427d1e8e9/52bbd483-995c-4ac0-b875-6fa184f6d4d7")
    (attr smd)
    (fp_text reference "U17" (at 0 -3.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d403910-6e4b-4520-88d1-f83df19b7fc2)
    )
    (fp_text value "~" (at 0 3.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a3f313e-89cb-41e9-9af6-2e92c5300811)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp 5af9305a-54bd-42b1-99b2-1adb4cfc92c2)
    )
    (fp_line (start 0 -2.56) (end -3.45 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 408dce4c-6f3f-4528-8957-4b0393f4d58d))
    (fp_line (start 0 -2.56) (end 1.95 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de88d9dc-81dd-4e16-b9d8-c8612166355c))
    (fp_line (start 0 2.56) (end -1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c21c4fa2-19c5-4ca7-a72f-ab2525ab0c6a))
    (fp_line (start 0 2.56) (end 1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8c907e8-594e-47c2-94bb-ebcc084f24c0))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1389750f-4a7a-4ecd-86d3-0319a6622005))
    (fp_line (start -3.7 2.7) (end 3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30d4e283-a109-4c3d-bc71-15cbd4da6ba9))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f3a0cc6-c732-45dd-bc43-cea128b83b5f))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 36b35bbd-fcee-4639-862f-abb85a5dfbef))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 621df3a6-a31e-491c-ab04-332c87d945ef))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae5465f7-63cc-4ccf-9d0e-430334596fe3))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e52d5824-11fa-46ef-80ed-dd84b7e53533))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 97662318-3dbd-408e-a0db-665818aeda50))
    (fp_line (start 1.95 2.45) (end -1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 52fa4890-6870-41c0-b73a-966340a1653e))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 791 "unconnected-(U17-CS#-Pad1)") (pinfunction "CS#") (pintype "input") (tstamp 52134fc1-d56b-4bdb-98b7-2040d2c57ea4))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 792 "unconnected-(U17-S0{slash}SI01-Pad2)") (pinfunction "S0/SI01") (pintype "bidirectional") (tstamp 1992dcf3-1aab-4cbe-b692-f0f0978e4366))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 793 "unconnected-(U17-WP#{slash}SIO2-Pad3)") (pinfunction "WP#/SIO2") (pintype "bidirectional") (tstamp 66a8d29b-ed19-44f4-a7e3-846055ec2264))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 794 "unconnected-(U17-GND-Pad4)") (pinfunction "GND") (pintype "passive") (tstamp 6e54738a-4956-40c1-bf1b-43fcb49d2713))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 795 "unconnected-(U17-SI{slash}SIO0-Pad5)") (pinfunction "SI/SIO0") (pintype "bidirectional") (tstamp 35f8db40-c9d3-4beb-ba72-a95b8c9256fa))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 796 "unconnected-(U17-SCLK-Pad6)") (pinfunction "SCLK") (pintype "input") (tstamp 4e47ec83-257b-490c-8b71-df6404bee83e))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 797 "unconnected-(U17-HOLD#{slash}SIO3-Pad7)") (pinfunction "HOLD#/SIO3") (pintype "bidirectional") (tstamp 033f7d91-0c08-4529-aa4a-51abace267b4))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 798 "unconnected-(U17-VCC-Pad8)") (pinfunction "VCC") (pintype "power_in") (tstamp b1063190-8d34-46d3-920c-d6408a99a638))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_BGA:BGA-400_17.0x17.0mm_Layout20x20_P0.8mm" (layer "F.Cu")
    (tstamp 85257116-053c-4e29-9c2a-adc9641f67d7)
    (at 105.6 60.05)
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "power")
    (path "/03abecec-4724-420e-920e-986ba2580308/c452b95e-9914-4c2a-8325-90800dccf607")
    (attr smd)
    (fp_text reference "U1" (at 0 -11.2 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0d212235-7969-43fd-ac49-f0ebcfdd325e)
    )
    (fp_text value "~" (at 0 11.2 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4eb0d4e4-3281-4f84-897b-9c26f7582653)
    )
    (fp_text user "A1" (at -9.6 -10 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
      (tstamp afca234e-b6af-4797-905f-2e852cec5826)
    )
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2a9d3ccf-7dfe-48f5-96ab-ca26d11eaf67)
    )
    (fp_line (start -9.6 -9.6) (end -7.6 -9.6)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp acb3b5d7-2c06-4b7a-9b36-2542d589fd95))
    (fp_line (start -9.6 -7.6) (end -9.6 -9.6)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6dfa6593-e0a6-41c6-92c2-aeeaa1938024))
    (fp_line (start -9.2 -9.2) (end -9.2 9.2)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d2f365b5-11d7-411f-850b-5fd377d727f7))
    (fp_line (start -9.2 9.2) (end 9.2 9.2)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e5560be4-07ec-4fb3-bbbf-6a9620464c78))
    (fp_line (start 9.2 -9.2) (end -9.2 -9.2)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp f1462245-7077-4a57-8d40-dc664202faa5))
    (fp_line (start 9.2 9.2) (end 9.2 -9.2)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b4235492-f2f5-4267-b7fd-5269a355fdb5))
    (fp_line (start -10 -10) (end -10 10)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 89c18137-e279-46b6-b7d5-c820a85c21ce))
    (fp_line (start -10 10) (end 10 10)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 620b6679-f5c1-46cc-9ec6-4422cc73a1b6))
    (fp_line (start 10 -10) (end -10 -10)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c7e87898-30a6-4225-a6fc-d57427b45661))
    (fp_line (start 10 10) (end 10 -10)
      (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e46359de-33e4-476a-bc35-4b1c830d68f0))
    (fp_line (start -8.8 -7.6) (end -8.8 8.8)
      (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 26fa6770-0955-47be-980e-fda6c1083c0f))
    (fp_line (start -8.8 8.8) (end 8.8 8.8)
      (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp e6593de9-e789-45bd-85cb-086d34387107))
    (fp_line (start -7.6 -8.8) (end -8.8 -7.6)
      (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 5d3da5fa-da00-4d1f-9af2-fb56de632c89))
    (fp_line (start 8.8 -8.8) (end -7.6 -8.8)
      (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp b6602502-1482-4aa4-b097-a293a2fea93b))
    (fp_line (start 8.8 8.8) (end 8.8 -8.8)
      (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp ca8b26fb-80d0-4e3b-bd15-5423d44be701))
    (pad "A1" smd circle (at -7.6 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "unconnected-(U1A-GND-PadA1)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp e70671b0-92bb-4257-bdbb-e3e9c471ebfa))
    (pad "A2" smd circle (at -6.8 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "unconnected-(U1H-GPIOT_RXN13-PadA2)") (pinfunction "GPIOT_RXN13") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2ea1a22c-e22a-4ab6-a94d-c848210fd33f))
    (pad "A3" smd circle (at -6 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "unconnected-(U1H-GPIOT_RXP13-PadA3)") (pinfunction "GPIOT_RXP13") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp cbf41276-d7dd-4e47-afee-617fca939f89))
    (pad "A4" smd circle (at -5.2 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(U1G-GPIOT_RXN05-PadA4)") (pinfunction "GPIOT_RXN05") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0726d5f0-cc1d-47b4-ae78-7ef37443c419))
    (pad "A5" smd circle (at -4.4 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(U1G-GPIOT_RXP05-PadA5)") (pinfunction "GPIOT_RXP05") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 25b1ca68-a2af-467e-be93-163aa34e78b9))
    (pad "A6" smd circle (at -3.6 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "unconnected-(U1G-GPIOT_RXN06-PadA6)") (pinfunction "GPIOT_RXN06") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0229f1ad-e01a-4c1a-a24c-523369d45f42))
    (pad "A7" smd circle (at -2.8 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "unconnected-(U1G-GPIOT_RXP06-PadA7)") (pinfunction "GPIOT_RXP06") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b8fc11f0-39af-42fc-86da-f777849aa13d))
    (pad "A8" smd circle (at -2 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "unconnected-(U1G-GPIOT_RXP03-PadA8)") (pinfunction "GPIOT_RXP03") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fedce3a2-af5a-414b-90f8-c6afde31457e))
    (pad "A9" smd circle (at -1.2 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "unconnected-(U1G-GPIOT_RXP02-PadA9)") (pinfunction "GPIOT_RXP02") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f63f54b7-4209-447b-8f03-750b57e48697))
    (pad "A10" smd circle (at -0.4 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "unconnected-(U1G-GPIOT_RXN02-PadA10)") (pinfunction "GPIOT_RXN02") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 442e9d8f-2831-4ce7-b096-00ad369d7cdd))
    (pad "A11" smd circle (at 0.4 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "unconnected-(U1F-GPIOL_108_CBSEL0-PadA11)") (pinfunction "GPIOL_108_CBSEL0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f3221b55-9605-4674-b640-e090768959f7))
    (pad "A12" smd circle (at 1.2 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "unconnected-(U1F-GPIOL_109_CBSEL1-PadA12)") (pinfunction "GPIOL_109_CBSEL1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9e1e4aa7-ffe0-4995-b52b-e0f5bd8b521b))
    (pad "A13" smd circle (at 2 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "unconnected-(U1F-GPIOL_106-PadA13)") (pinfunction "GPIOL_106") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c7296151-0454-4a99-934a-8751f67b5d48))
    (pad "A14" smd circle (at 2.8 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "unconnected-(U1F-GPIOL_107-PadA14)") (pinfunction "GPIOL_107") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 96696ff8-9adb-409b-81f8-d9994b1ab8dc))
    (pad "A15" smd circle (at 3.6 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "unconnected-(U1F-GPIOL_105-PadA15)") (pinfunction "GPIOL_105") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 76bf3b70-d50e-43b2-b3cc-bd53730cd884))
    (pad "A16" smd circle (at 4.4 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "unconnected-(U1F-GPIOL_97-PadA16)") (pinfunction "GPIOL_97") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d02d0cc3-2a7d-4d7e-8046-42c704eba474))
    (pad "A17" smd circle (at 5.2 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(U1E-GPIOL_90-PadA17)") (pinfunction "GPIOL_90") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp be6cbc85-c40c-4ec8-8662-b9e3033743fd))
    (pad "A18" smd circle (at 6 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "unconnected-(U1E-GPIOL_88-PadA18)") (pinfunction "GPIOL_88") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp eb142027-79cc-4f09-a475-3c716a48556b))
    (pad "A19" smd circle (at 6.8 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "unconnected-(U1E-GPIOL_86-PadA19)") (pinfunction "GPIOL_86") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4f1ad169-d9fb-487c-868e-53d97da93fc6))
    (pad "A20" smd circle (at 7.6 -7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "unconnected-(U1A-GND-PadA20)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 7d4bff63-4c49-4f29-ab18-7adeb458ddf4))
    (pad "B1" smd circle (at -7.6 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "unconnected-(U1H-GPIOT_RXN16_EXTFB1-PadB1)") (pinfunction "GPIOT_RXN16_EXTFB1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 91aa9d8c-55d1-4964-b835-8c50c0578f76))
    (pad "B2" smd circle (at -6.8 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "unconnected-(U1H-GPIOT_RXP16_EXTFB1-PadB2)") (pinfunction "GPIOT_RXP16_EXTFB1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 689711ca-79b1-4e65-940d-298ff373e729))
    (pad "B3" smd circle (at -6 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "unconnected-(U1H-GPIOT_RXN15-PadB3)") (pinfunction "GPIOT_RXN15") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp adf39bd6-00b0-4c18-b00a-4d74967e07d5))
    (pad "B4" smd circle (at -5.2 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "unconnected-(U1A-GND-PadB4)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp e65a2448-3d3d-440c-8d06-df448dd1817e))
    (pad "B5" smd circle (at -4.4 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "unconnected-(U1G-GPIOT_RXN08_CLKN0-PadB5)") (pinfunction "GPIOT_RXN08_CLKN0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9f54d80e-8f69-4435-a4c1-1c3e6e9e4a79))
    (pad "B6" smd circle (at -3.6 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "unconnected-(U1G-GPIOT_RXP08_CLKP0-PadB6)") (pinfunction "GPIOT_RXP08_CLKP0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6c215e64-567b-4814-b324-1e5260b090fe))
    (pad "B7" smd circle (at -2.8 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "unconnected-(U1G-VCCIO2A-PadB7)") (pinfunction "VCCIO2A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 502fc007-8ad5-4475-8f80-f6f33c10fb8b))
    (pad "B8" smd circle (at -2 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "unconnected-(U1G-GPIOT_RXN03-PadB8)") (pinfunction "GPIOT_RXN03") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 28f30939-1b6d-48c5-b574-62618490d4f2))
    (pad "B9" smd circle (at -1.2 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "unconnected-(U1G-GPIOT_RXP04-PadB9)") (pinfunction "GPIOT_RXP04") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ede88149-484d-462f-bd40-7d4d1cff5963))
    (pad "B10" smd circle (at -0.4 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "unconnected-(U1G-VCCIO2A-PadB10)") (pinfunction "VCCIO2A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp b0173d50-a0fc-46b1-a259-fa56cd9aef10))
    (pad "B11" smd circle (at 0.4 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "unconnected-(U1G-GPIOT_RXP00-PadB11)") (pinfunction "GPIOT_RXP00") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp a9b048f2-c726-4520-9728-c80d560c8440))
    (pad "B12" smd circle (at 1.2 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "unconnected-(U1F-VCCIO1E-PadB12)") (pinfunction "VCCIO1E") (pintype "power_in") (solder_mask_margin 0.075) (tstamp a28b4c87-92b8-474b-8240-bfe8f1a141bd))
    (pad "B13" smd circle (at 2 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "unconnected-(U1F-GPIOL_112-PadB13)") (pinfunction "GPIOL_112") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 259bb6ad-5c01-4e5b-9cc1-2fbe75d75d2c))
    (pad "B14" smd circle (at 2.8 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "unconnected-(U1F-VCCIO1E-PadB14)") (pinfunction "VCCIO1E") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 2a65c5d4-f968-455a-9730-93f04fbcb9e9))
    (pad "B15" smd circle (at 3.6 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "unconnected-(U1F-GPIOL_96-PadB15)") (pinfunction "GPIOL_96") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d33441ae-7de9-49e6-a7df-8ad5904b61d3))
    (pad "B16" smd circle (at 4.4 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "unconnected-(U1E-GPIOL_87-PadB16)") (pinfunction "GPIOL_87") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1d5a60e4-2f91-40af-8ecd-72188c247cad))
    (pad "B17" smd circle (at 5.2 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "unconnected-(U1E-VCCIO1D-PadB17)") (pinfunction "VCCIO1D") (pintype "power_in") (solder_mask_margin 0.075) (tstamp aaa70d7b-d0b6-4853-bdbb-a17f2d2580c0))
    (pad "B18" smd circle (at 6 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "unconnected-(U1E-GPIOL_73_CLK7-PadB18)") (pinfunction "GPIOL_73_CLK7") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 647e2b28-a195-4d05-b429-d774952c79ce))
    (pad "B19" smd circle (at 6.8 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "unconnected-(U1E-GPIOL_77_CTRL7-PadB19)") (pinfunction "GPIOL_77_CTRL7") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 204987da-e043-4446-a432-99ff3d4afd6c))
    (pad "B20" smd circle (at 7.6 -6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "unconnected-(U1E-GPIOL_71_CLK5-PadB20)") (pinfunction "GPIOL_71_CLK5") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f3939846-6de6-46f9-a3b1-c6f9dcd50633))
    (pad "C1" smd circle (at -7.6 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "unconnected-(U1I-GPIOT_RXN18-PadC1)") (pinfunction "GPIOT_RXN18") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d2b73073-b58f-429f-a8f6-f32e9b5084b9))
    (pad "C2" smd circle (at -6.8 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "unconnected-(U1H-VCCIO2B-PadC2)") (pinfunction "VCCIO2B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 81e2ff2d-f5ba-439d-a588-23e90c244313))
    (pad "C3" smd circle (at -6 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "unconnected-(U1H-GPIOT_RXP15-PadC3)") (pinfunction "GPIOT_RXP15") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 940832c7-e17d-4006-8150-2c41ba0c21ce))
    (pad "C4" smd circle (at -5.2 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "unconnected-(U1H-GPIOT_RXP14-PadC4)") (pinfunction "GPIOT_RXP14") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 47e11beb-04fc-45a3-8ce5-83390cf6444c))
    (pad "C5" smd circle (at -4.4 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "unconnected-(U1H-GPIOT_RXN14-PadC5)") (pinfunction "GPIOT_RXN14") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 62bddb7b-574a-46d8-aa30-a676ce30d390))
    (pad "C6" smd circle (at -3.6 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "unconnected-(U1H-GPIOT_RXP10-PadC6)") (pinfunction "GPIOT_RXP10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0864102d-9188-4d1c-aab7-bab430ef46f2))
    (pad "C7" smd circle (at -2.8 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "unconnected-(U1H-GPIOT_RXN10-PadC7)") (pinfunction "GPIOT_RXN10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6fbeddf8-6219-41a1-a388-2467ca490792))
    (pad "C8" smd circle (at -2 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "unconnected-(U1H-VCCIO2B-PadC8)") (pinfunction "VCCIO2B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 24dc33c3-5f8e-46cd-847b-5f9d63ef8382))
    (pad "C9" smd circle (at -1.2 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "unconnected-(U1G-GPIOT_RXN04-PadC9)") (pinfunction "GPIOT_RXN04") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp aea53004-6167-4def-9743-14cec3be497d))
    (pad "C10" smd circle (at -0.4 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "unconnected-(U1G-GPIOT_RXP01-PadC10)") (pinfunction "GPIOT_RXP01") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 62826944-6567-428d-a45d-c4d13c257706))
    (pad "C11" smd circle (at 0.4 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "unconnected-(U1G-GPIOT_RXN00-PadC11)") (pinfunction "GPIOT_RXN00") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 630e606b-50a2-4da7-95ce-acb75d98ded1))
    (pad "C12" smd circle (at 1.2 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "unconnected-(U1F-GPIOL_111-PadC12)") (pinfunction "GPIOL_111") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4e781cee-1274-436e-a54d-5159ead5f196))
    (pad "C13" smd circle (at 2 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "unconnected-(U1F-GPIOL_110-PadC13)") (pinfunction "GPIOL_110") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d3cd832f-2147-4a41-bf28-320cc5cb7dd8))
    (pad "C14" smd circle (at 2.8 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "unconnected-(U1F-GPIOL_102_NSTATUS-PadC14)") (pinfunction "GPIOL_102_NSTATUS") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b3efccc2-40cc-42ae-9d17-8b9675581822))
    (pad "C15" smd circle (at 3.6 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "unconnected-(U1F-GPIOL_94-PadC15)") (pinfunction "GPIOL_94") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp bff5b534-14f5-4e6e-8cf7-be0affe0e929))
    (pad "C16" smd circle (at 4.4 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "unconnected-(U1E-GPIOL_93-PadC16)") (pinfunction "GPIOL_93") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp daf53c15-3f83-4503-bdd0-56637d427a63))
    (pad "C17" smd circle (at 5.2 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "unconnected-(U1E-GPIOL_84-PadC17)") (pinfunction "GPIOL_84") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c60a89b8-b880-404d-918a-1ab0fe0507a3))
    (pad "C18" smd circle (at 6 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "unconnected-(U1E-GPIOL_76_CTRL6-PadC18)") (pinfunction "GPIOL_76_CTRL6") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c434d2b7-e7dd-4c09-b17a-6ac14dfea02d))
    (pad "C19" smd circle (at 6.8 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "unconnected-(U1E-VCCIO1D-PadC19)") (pinfunction "VCCIO1D") (pintype "power_in") (solder_mask_margin 0.075) (tstamp b80c1857-1bcf-4bdd-b82a-c105381166e8))
    (pad "C20" smd circle (at 7.6 -6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "unconnected-(U1E-GPIOL_74_CTRL4-PadC20)") (pinfunction "GPIOL_74_CTRL4") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d41afadb-5415-4fc7-8fed-68a3197821a0))
    (pad "D1" smd circle (at -7.6 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "unconnected-(U1I-GPIOT_RXP18-PadD1)") (pinfunction "GPIOT_RXP18") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 05666622-ca9b-4781-9fcc-00dd06502e56))
    (pad "D2" smd circle (at -6.8 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "unconnected-(U1I-GPIOT_RXN21-PadD2)") (pinfunction "GPIOT_RXN21") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 53a3fae7-7431-4921-927c-6e53246e498e))
    (pad "D3" smd circle (at -6 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 190 "unconnected-(U1H-GPIOT_RXN17_CLKN1-PadD3)") (pinfunction "GPIOT_RXN17_CLKN1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d1352d2e-4490-49f1-83cc-4fb791e74727))
    (pad "D4" smd circle (at -5.2 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 191 "unconnected-(U1H-GPIOT_RXP17_CLKP1-PadD4)") (pinfunction "GPIOT_RXP17_CLKP1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f35cf26a-be0b-4c9e-8da9-2d49afcc5faa))
    (pad "D5" smd circle (at -4.4 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 192 "unconnected-(U1H-GPIOT_RXN11-PadD5)") (pinfunction "GPIOT_RXN11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 77c42540-c837-433f-ab5b-650837ac699d))
    (pad "D6" smd circle (at -3.6 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 193 "unconnected-(U1H-GPIOT_RXP11-PadD6)") (pinfunction "GPIOT_RXP11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 7b5a2fda-0f9f-4fe9-9da6-e3ade9285ab4))
    (pad "D7" smd circle (at -2.8 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 194 "unconnected-(U1H-GPIOT_RX09-PadD7)") (pinfunction "GPIOT_RX09") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 8f0bdced-ffea-46fb-95f2-d496d4a04852))
    (pad "D8" smd circle (at -2 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 195 "unconnected-(U1H-GPIOT_RXP09-PadD8)") (pinfunction "GPIOT_RXP09") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5922a175-2d35-4d16-8b0e-98ddf47e34a8))
    (pad "D9" smd circle (at -1.2 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "unconnected-(U1H-GPIOT_RXP12-PadD9)") (pinfunction "GPIOT_RXP12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 164878b6-7d3f-4442-9567-5c02c3e942f1))
    (pad "D10" smd circle (at -0.4 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "unconnected-(U1G-GPIOT_RXN01-PadD10)") (pinfunction "GPIOT_RXN01") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2ee500a1-076b-4713-bf94-447635193451))
    (pad "D11" smd circle (at 0.4 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 198 "unconnected-(U1A-GND-PadD11)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp c3ec65cd-47d5-4ca9-9a16-5d59dd9bd6eb))
    (pad "D12" smd circle (at 1.2 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 199 "unconnected-(U1F-GPIOL_113-PadD12)") (pinfunction "GPIOL_113") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 94856ac4-f22f-42e0-8504-23f11f576ee7))
    (pad "D13" smd circle (at 2 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 200 "unconnected-(U1F-GPIOL_114-PadD13)") (pinfunction "GPIOL_114") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ad7698e4-6014-4b54-a53c-f868fb5c95e1))
    (pad "D14" smd circle (at 2.8 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 201 "unconnected-(U1F-GPIOL_100-PadD14)") (pinfunction "GPIOL_100") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9a5b19b5-b389-4ee4-842a-ca14c0f5dd6a))
    (pad "D15" smd circle (at 3.6 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 202 "unconnected-(U1F-GPIOL_95-PadD15)") (pinfunction "GPIOL_95") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 33a5e73b-82d9-4cff-9c9d-8d13cccff90a))
    (pad "D16" smd circle (at 4.4 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 203 "unconnected-(U1E-GPIOL_92-PadD16)") (pinfunction "GPIOL_92") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ce65762e-cefd-4e9e-ae2b-325b73d724f1))
    (pad "D17" smd circle (at 5.2 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "unconnected-(U1E-GPIOL_79-PadD17)") (pinfunction "GPIOL_79") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1f299f9d-8609-4a40-91c4-e84eb56dac08))
    (pad "D18" smd circle (at 6 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "unconnected-(U1E-GPIOL_72_CLK6-PadD18)") (pinfunction "GPIOL_72_CLK6") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 924bf92b-41e7-47a2-ace0-c9ee4e5c431b))
    (pad "D19" smd circle (at 6.8 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 206 "unconnected-(U1D-GPIOL_63_CTRL1-PadD19)") (pinfunction "GPIOL_63_CTRL1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e228e1f6-5311-4867-b420-0e7d7be82bab))
    (pad "D20" smd circle (at 7.6 -5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 207 "unconnected-(U1D-GPIOL_66_CLK0-PadD20)") (pinfunction "GPIOL_66_CLK0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9c061415-7117-478b-be88-7272cd4e518d))
    (pad "E1" smd circle (at -7.6 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "unconnected-(U1I-GPIOT_RXP23-PadE1)") (pinfunction "GPIOT_RXP23") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c0085704-1d77-4ffc-8ea9-3aad74c2d6b9))
    (pad "E2" smd circle (at -6.8 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "unconnected-(U1I-GPIOT_RXP21-PadE2)") (pinfunction "GPIOT_RXP21") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fb0be340-08e1-48fa-a163-11dcd6e5afdc))
    (pad "E3" smd circle (at -6 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "unconnected-(U1I-GPIOT_RXN20-PadE3)") (pinfunction "GPIOT_RXN20") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 892d15c3-7f9e-4d8e-9dfa-26be5f06231a))
    (pad "E4" smd circle (at -5.2 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "unconnected-(U1I-GPIOT_RXP20-PadE4)") (pinfunction "GPIOT_RXP20") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1ee85f4a-5bba-49f7-8908-6b539e2ba4a9))
    (pad "E5" smd circle (at -4.4 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "unconnected-(U1I-VCCIO2C-PadE5)") (pinfunction "VCCIO2C") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 73e7f7f0-1afe-43d3-b3ae-f726d1acdb10))
    (pad "E6" smd circle (at -3.6 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "unconnected-(U1I-GPIOT_RXP19-PadE6)") (pinfunction "GPIOT_RXP19") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 66a3cb38-1808-4257-867e-5b7dacdd4c82))
    (pad "E7" smd circle (at -2.8 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 214 "unconnected-(U1I-GPIOT_RXN19-PadE7)") (pinfunction "GPIOT_RXN19") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e5773f81-b4ff-42d4-9a77-073e9c467100))
    (pad "E8" smd circle (at -2 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 215 "unconnected-(U1A-GND-PadE8)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 0b38e34f-1467-4f03-9a19-186ad4794599))
    (pad "E9" smd circle (at -1.2 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 216 "unconnected-(U1H-GPIOT_RXN12-PadE9)") (pinfunction "GPIOT_RXN12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp af26d850-80c7-42df-911e-bbe62287760b))
    (pad "E10" smd circle (at -0.4 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 217 "unconnected-(U1G-GPIOT_RXP07_EXTFB0-PadE10)") (pinfunction "GPIOT_RXP07_EXTFB0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6364c32c-fbfe-4153-b931-d626955f6957))
    (pad "E11" smd circle (at 0.4 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 218 "unconnected-(U1G-GPIOT_RXN07_EXTFB0-PadE11)") (pinfunction "GPIOT_RXN07_EXTFB0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 931fea4a-822f-45cc-8048-28ac665a7c61))
    (pad "E12" smd circle (at 1.2 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 219 "unconnected-(U1F-GPIOL_116-PadE12)") (pinfunction "GPIOL_116") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 47961bbe-8f43-4c01-85dd-39b7baf25101))
    (pad "E13" smd circle (at 2 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 220 "unconnected-(U1F-VCCIO1E-PadE13)") (pinfunction "VCCIO1E") (pintype "power_in") (solder_mask_margin 0.075) (tstamp eff1ddca-279e-42ed-8a0a-aced8b108472))
    (pad "E14" smd circle (at 2.8 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 221 "unconnected-(U1F-GPIOL_104-PadE14)") (pinfunction "GPIOL_104") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2c7bd4b5-30ba-4698-a476-53f06a6b6198))
    (pad "E15" smd circle (at 3.6 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 222 "unconnected-(U1F-GPIOL_99-PadE15)") (pinfunction "GPIOL_99") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 471cb400-9ea0-4868-a169-04cd970368ca))
    (pad "E16" smd circle (at 4.4 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 223 "unconnected-(U1E-VCCIO1D-PadE16)") (pinfunction "VCCIO1D") (pintype "power_in") (solder_mask_margin 0.075) (tstamp a1711f70-559a-4ac6-a291-a359d3738479))
    (pad "E17" smd circle (at 5.2 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 224 "unconnected-(U1E-GPIOL_75_CTRL5-PadE17)") (pinfunction "GPIOL_75_CTRL5") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 089e44e5-0a05-4d15-894c-53cafd347a1b))
    (pad "E18" smd circle (at 6 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 225 "unconnected-(U1D-GPIOL_68_CLK2-PadE18)") (pinfunction "GPIOL_68_CLK2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ecaf95c8-c4a7-424b-9ed7-e5e0deef49f4))
    (pad "E19" smd circle (at 6.8 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 226 "unconnected-(U1D-VCCIO1C-PadE19)") (pinfunction "VCCIO1C") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 06a84b55-1e96-4dd0-8029-4736d6904c5d))
    (pad "E20" smd circle (at 7.6 -4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 227 "unconnected-(U1D-GPIOL_67_CLK1-PadE20)") (pinfunction "GPIOL_67_CLK1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 230875bd-2713-4ce2-a065-d506d97da6fc))
    (pad "F1" smd circle (at -7.6 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 228 "unconnected-(U1I-GPIOT_RXN23-PadF1)") (pinfunction "GPIOT_RXN23") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 525d42d7-14da-4b14-88e6-76cb21114d98))
    (pad "F2" smd circle (at -6.8 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 229 "unconnected-(U1I-VCCIO2C-PadF2)") (pinfunction "VCCIO2C") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 049d210f-30ae-4470-bdf5-f6b88c911b6d))
    (pad "F3" smd circle (at -6 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 230 "unconnected-(U1I-GPIOT_RXN22-PadF3)") (pinfunction "GPIOT_RXN22") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3342135e-9c9f-417b-84cd-35efd4dbe920))
    (pad "F4" smd circle (at -5.2 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 231 "unconnected-(U1I-GPIOT_RXP24_EXTFB2-PadF4)") (pinfunction "GPIOT_RXP24_EXTFB2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3a9bf291-3f99-4a6f-8cf0-1e7560a96f8d))
    (pad "F5" smd circle (at -4.4 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 232 "unconnected-(U1I-GPIOT_RXN24_EXTFB2-PadF5)") (pinfunction "GPIOT_RXN24_EXTFB2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 8d5918a8-b0ec-42d3-bdc3-078fe90b9a17))
    (pad "F6" smd circle (at -3.6 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 233 "unconnected-(U1J-GPIOR_121_MREFCLK-PadF6)") (pinfunction "GPIOR_121_MREFCLK") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d660ef4d-522f-44b7-8d66-740acb17a7e2))
    (pad "F7" smd circle (at -2.8 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 234 "unconnected-(U1J-GPIOR_118_PLLIN0-PadF7)") (pinfunction "GPIOR_118_PLLIN0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f9562dac-5093-44b8-a49c-18d5674fe51c))
    (pad "F8" smd circle (at -2 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 235 "unconnected-(U1P-VCCA_TR-PadF8)") (pinfunction "VCCA_TR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp c2938201-3ffd-42b0-984c-841d458a2b82))
    (pad "F9" smd circle (at -1.2 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 236 "unconnected-(U1I-VCCIO2C-PadF9)") (pinfunction "VCCIO2C") (pintype "power_in") (solder_mask_margin 0.075) (tstamp fba0d4d1-8b2b-4371-8aa8-0bbc339494bf))
    (pad "F10" smd circle (at -0.4 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 237 "unconnected-(U1H-VCCIO2B-PadF10)") (pinfunction "VCCIO2B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 8ea52f2b-3906-45f1-b701-e22930391103))
    (pad "F11" smd circle (at 0.4 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 238 "unconnected-(U1G-VCCIO2A-PadF11)") (pinfunction "VCCIO2A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp f5aed25d-5360-43cd-965a-ac1ed8c8c085))
    (pad "F12" smd circle (at 1.2 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "unconnected-(U1F-GPIOL_115-PadF12)") (pinfunction "GPIOL_115") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp cb15ec5b-8a6d-4fde-834b-ce86c604cbd8))
    (pad "F13" smd circle (at 2 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 240 "unconnected-(U1F-GPIOL_117-PadF13)") (pinfunction "GPIOL_117") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 71e2a47d-acb4-41aa-89b8-68472a0baf19))
    (pad "F14" smd circle (at 2.8 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 241 "unconnected-(U1F-GPIOL_103_TEST_N-PadF14)") (pinfunction "GPIOL_103_TEST_N") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c4400cfc-ff43-4e74-b73a-436647d77d19))
    (pad "F15" smd circle (at 3.6 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 242 "unconnected-(U1F-GPIOL_98-PadF15)") (pinfunction "GPIOL_98") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b16aae40-44be-4342-aa72-bd81c7422c01))
    (pad "F16" smd circle (at 4.4 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 243 "unconnected-(U1E-GPIOL_85-PadF16)") (pinfunction "GPIOL_85") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c66d35c5-ef1b-4b50-a5c4-09b047b8ca5c))
    (pad "F17" smd circle (at 5.2 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 244 "unconnected-(U1E-GPIOL_82-PadF17)") (pinfunction "GPIOL_82") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 557e222c-a49c-4a90-91e6-12cfec9bf4e2))
    (pad "F18" smd circle (at 6 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 245 "unconnected-(U1D-GPIOL_69_CLK3-PadF18)") (pinfunction "GPIOL_69_CLK3") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9c3575c9-4aa3-4519-8d50-848746d2e08b))
    (pad "F19" smd circle (at 6.8 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 246 "unconnected-(U1D-GPIOL_64_CTRL2-PadF19)") (pinfunction "GPIOL_64_CTRL2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp bdc94987-d566-44ec-bff6-8b2f4de443f3))
    (pad "F20" smd circle (at 7.6 -3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 247 "unconnected-(U1D-GPIOL_58-PadF20)") (pinfunction "GPIOL_58") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4b5177d4-3ee2-4ad8-bef4-be2429c4d5a1))
    (pad "G1" smd circle (at -7.6 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 248 "unconnected-(U1I-GPIOT_RXN25_CLKIN2-PadG1)") (pinfunction "GPIOT_RXN25_CLKIN2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3ee5464d-224f-4378-a408-0c6df629bf23))
    (pad "G2" smd circle (at -6.8 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 249 "unconnected-(U1I-GPIOT_RXP25_CLKP2-PadG2)") (pinfunction "GPIOT_RXP25_CLKP2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d0045354-4002-49c1-91f5-1abbce95a2ba))
    (pad "G3" smd circle (at -6 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 250 "unconnected-(U1I-GPIOT_RXP22-PadG3)") (pinfunction "GPIOT_RXP22") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 00a23cf7-a951-4903-ab57-7cdc74835b6b))
    (pad "G4" smd circle (at -5.2 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 251 "unconnected-(U1J-GPIOR_127_CLK14-PadG4)") (pinfunction "GPIOR_127_CLK14") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 41562a0b-fb94-4efe-aaf0-e3ef1fdae629))
    (pad "G5" smd circle (at -4.4 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 252 "unconnected-(U1J-GPIOR_123_CTRL14-PadG5)") (pinfunction "GPIOR_123_CTRL14") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp dd3247b1-7bec-4cea-b1bf-821cbf716ad9))
    (pad "G6" smd circle (at -3.6 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 253 "unconnected-(U1J-GPIOR_119_PLLIN1-PadG6)") (pinfunction "GPIOR_119_PLLIN1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 94968d55-1d05-4fbd-8227-71a4d6f7f086))
    (pad "G7" smd circle (at -2.8 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 254 "unconnected-(U1J-GPIOR_120_PLLIN2-PadG7)") (pinfunction "GPIOR_120_PLLIN2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f8473698-5918-4ab7-9f15-7c641b95a8df))
    (pad "G8" smd circle (at -2 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 255 "unconnected-(U1A-GND-PadG8)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 2e17c011-e3f9-4406-bf45-bda75691fb6b))
    (pad "G9" smd circle (at -1.2 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 256 "unconnected-(U1A-GND-PadG9)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 2bde8b70-2f71-43a0-b0e3-89471b0562ea))
    (pad "G10" smd circle (at -0.4 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 257 "unconnected-(U1A-GND-PadG10)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 27c4a5d7-1117-436c-a158-e3ebd66f1218))
    (pad "G11" smd circle (at 0.4 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 258 "unconnected-(U1A-GND-PadG11)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp c098227d-025b-4b6c-aefb-eaa8b5bc3581))
    (pad "G12" smd circle (at 1.2 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 259 "unconnected-(U1A-GND-PadG12)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 74766578-a7e6-4f2b-bc30-6269c53f0598))
    (pad "G13" smd circle (at 2 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 260 "unconnected-(U1A-GND-PadG13)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp f0fecaca-665c-4ff7-b219-bf940187f7b4))
    (pad "G14" smd circle (at 2.8 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 261 "unconnected-(U1F-GPIOL_101-PadG14)") (pinfunction "GPIOL_101") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp a86166e1-22f8-4d1f-8656-bffc31ee3aa9))
    (pad "G15" smd circle (at 3.6 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 262 "unconnected-(U1E-GPIOL_91-PadG15)") (pinfunction "GPIOL_91") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 594b27ed-feb3-4128-91a1-46821e7ffc88))
    (pad "G16" smd circle (at 4.4 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 263 "unconnected-(U1E-GPIOL_89-PadG16)") (pinfunction "GPIOL_89") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f8685468-9302-45b6-a078-8f87398fd869))
    (pad "G17" smd circle (at 5.2 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 264 "unconnected-(U1E-GPIOL_70_CLK4-PadG17)") (pinfunction "GPIOL_70_CLK4") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 03d0b3bf-4f14-4fac-a625-963b803044e0))
    (pad "G18" smd circle (at 6 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 265 "unconnected-(U1D-GPIOL_65_CTRL3-PadG18)") (pinfunction "GPIOL_65_CTRL3") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3faf7719-2094-43f5-9ffd-ebd59b811426))
    (pad "G19" smd circle (at 6.8 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 266 "unconnected-(U1A-GND-PadG19)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp b25faa4b-edcb-495a-99eb-4ba52f8d22ad))
    (pad "G20" smd circle (at 7.6 -2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 267 "unconnected-(U1D-GPIOL_56-PadG20)") (pinfunction "GPIOL_56") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 06212271-3177-44c8-9637-28cb8e3900ca))
    (pad "H1" smd circle (at -7.6 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 268 "unconnected-(U1J-GPIOR_130_CLK11-PadH1)") (pinfunction "GPIOR_130_CLK11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4ca9a345-6cc3-42da-9809-8f00e7350bf8))
    (pad "H2" smd circle (at -6.8 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 269 "unconnected-(U1J-GPIOR_131_CLK10-PadH2)") (pinfunction "GPIOR_131_CLK10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 8085df22-b780-4bd2-a9c2-67270bf962a0))
    (pad "H3" smd circle (at -6 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 270 "unconnected-(U1J-GPIOR_124_CTRL13-PadH3)") (pinfunction "GPIOR_124_CTRL13") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4307509a-680f-4de2-a00c-08af10ad968d))
    (pad "H4" smd circle (at -5.2 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 271 "unconnected-(U1J-GPIOR_125_CTRL12-PadH4)") (pinfunction "GPIOR_125_CTRL12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5d90c25b-afdd-4add-a028-7d5488968472))
    (pad "H5" smd circle (at -4.4 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 272 "unconnected-(U1J-VCCIO3C_TR-PadH5)") (pinfunction "VCCIO3C_TR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 1ae91bee-8e06-4afb-ae0e-c866dfbbb924))
    (pad "H6" smd circle (at -3.6 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 273 "unconnected-(U1J-GPIOR_122_CTRL15-PadH6)") (pinfunction "GPIOR_122_CTRL15") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e6b74b06-7894-4ffd-b378-6223e68f37cb))
    (pad "H7" smd circle (at -2.8 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 274 "unconnected-(U1J-GPIOR_126_CLK15-PadH7)") (pinfunction "GPIOR_126_CLK15") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e80c48fd-0932-4307-b309-1b565fee6f41))
    (pad "H8" smd circle (at -2 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 275 "unconnected-(U1O-VCC-PadH8)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp d64bca46-908a-43d1-b912-84ffc4fea7a0))
    (pad "H9" smd circle (at -1.2 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 276 "unconnected-(U1O-VCC-PadH9)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 0b66a3a7-18fb-4840-930c-dc434913553b))
    (pad "H10" smd circle (at -0.4 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 277 "unconnected-(U1O-VCC-PadH10)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 0881bc1f-5773-433f-9add-acb12594ce46))
    (pad "H11" smd circle (at 0.4 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 278 "unconnected-(U1O-VCC-PadH11)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 608fe8bc-6046-481c-a364-0063486b1522))
    (pad "H12" smd circle (at 1.2 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 279 "unconnected-(U1O-VCC-PadH12)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 8d07b7a4-b5d8-423a-acd5-0ed39da408ea))
    (pad "H13" smd circle (at 2 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 280 "unconnected-(U1O-VCC-PadH13)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 1f47812a-7251-494e-a962-ad8a691d7575))
    (pad "H14" smd circle (at 2.8 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 281 "unconnected-(U1E-GPIOL_83-PadH14)") (pinfunction "GPIOL_83") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 37539e21-bee1-4f49-a7dc-fbcfce0cc760))
    (pad "H15" smd circle (at 3.6 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 282 "unconnected-(U1E-GPIOL_81-PadH15)") (pinfunction "GPIOL_81") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d6104418-c663-4c5d-b022-f04d43386fc5))
    (pad "H16" smd circle (at 4.4 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 283 "unconnected-(U1D-VCCIO1C-PadH16)") (pinfunction "VCCIO1C") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 2e81da82-596f-497c-8f31-50bb89972be5))
    (pad "H17" smd circle (at 5.2 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 284 "unconnected-(U1D-GPIOL_60-PadH17)") (pinfunction "GPIOL_60") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9463571e-d2d7-450a-8e83-04efd3f46f76))
    (pad "H18" smd circle (at 6 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 285 "unconnected-(U1D-GPIOL_62_CTRL0-PadH18)") (pinfunction "GPIOL_62_CTRL0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 45bccee3-c164-43fb-b64a-9ef79bbac384))
    (pad "H19" smd circle (at 6.8 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 286 "unconnected-(U1D-GPIOL_54-PadH19)") (pinfunction "GPIOL_54") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp da03ca3a-73bb-4403-8b0e-5d5721c83f70))
    (pad "H20" smd circle (at 7.6 -2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 287 "unconnected-(U1D-GPIOL_53-PadH20)") (pinfunction "GPIOL_53") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 7ff6f09d-70ff-465d-ac82-0249f943f766))
    (pad "J1" smd circle (at -7.6 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 288 "unconnected-(U1J-GPIOR_134_CTRL11-PadJ1)") (pinfunction "GPIOR_134_CTRL11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fc1f36e2-2e30-4469-925c-79b8310d32dd))
    (pad "J2" smd circle (at -6.8 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 289 "unconnected-(U1A-GND-PadJ2)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 7b28cd7e-77ec-4306-acdb-70282768750e))
    (pad "J3" smd circle (at -6 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 290 "unconnected-(U1J-GPIOR_135_CTRL10-PadJ3)") (pinfunction "GPIOR_135_CTRL10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e0740d58-77cc-4bdd-a357-f97b56523a45))
    (pad "J4" smd circle (at -5.2 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "unconnected-(U1J-GPIOR_132_CLK9-PadJ4)") (pinfunction "GPIOR_132_CLK9") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f8f22c2c-665c-4445-b039-0308ad8178cf))
    (pad "J5" smd circle (at -4.4 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 292 "unconnected-(U1J-GPIOR_133_CLK8-PadJ5)") (pinfunction "GPIOR_133_CLK8") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6b67da94-605c-4559-b346-bad2ef99e758))
    (pad "J6" smd circle (at -3.6 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 293 "unconnected-(U1J-GPIOR_129_CLK12-PadJ6)") (pinfunction "GPIOR_129_CLK12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp abcea9e6-176f-4abf-881c-8f7e9c560fbd))
    (pad "J7" smd circle (at -2.8 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 294 "unconnected-(U1J-VCCIO3C_TR-PadJ7)") (pinfunction "VCCIO3C_TR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp a7de1fe4-f407-437c-8fd7-ad72341669c1))
    (pad "J8" smd circle (at -2 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 295 "unconnected-(U1A-GND-PadJ8)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp c62fa908-e8a6-4ad1-8630-4cc8f1df3b1f))
    (pad "J9" smd circle (at -1.2 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 296 "unconnected-(U1A-GND-PadJ9)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp d19141ec-d3d3-4be8-b1fd-d78c3ac1b50f))
    (pad "J10" smd circle (at -0.4 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 297 "unconnected-(U1A-GND-PadJ10)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 7fa04245-5c4e-4356-8b77-e05696fbb527))
    (pad "J11" smd circle (at 0.4 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 298 "unconnected-(U1A-GND-PadJ11)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp f1e16779-0d34-45ee-9647-95920c007e43))
    (pad "J12" smd circle (at 1.2 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 299 "unconnected-(U1A-GND-PadJ12)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp f0f14fd9-63c6-4fb8-a3f3-c0d938df4a91))
    (pad "J13" smd circle (at 2 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 300 "unconnected-(U1A-GND-PadJ13)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 99f2019e-4c6d-4f03-9fdb-2a47b614e81e))
    (pad "J14" smd circle (at 2.8 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 301 "unconnected-(U1D-GPIOL_59-PadJ14)") (pinfunction "GPIOL_59") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp a45b4616-b177-416c-aadc-b43b2e81c9a8))
    (pad "J15" smd circle (at 3.6 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 302 "unconnected-(U1D-GPIOL_57-PadJ15)") (pinfunction "GPIOL_57") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f3c35c25-17a4-4b36-8f3c-21f0f9015e83))
    (pad "J16" smd circle (at 4.4 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 303 "unconnected-(U1D-GPIOL_51-PadJ16)") (pinfunction "GPIOL_51") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ef741cf4-2162-4ec1-a5cc-c2cc14c56620))
    (pad "J17" smd circle (at 5.2 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 304 "unconnected-(U1D-GPIOL_52-PadJ17)") (pinfunction "GPIOL_52") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0f188177-b978-43d2-bb41-58c2a080c021))
    (pad "J18" smd circle (at 6 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 305 "unconnected-(U1D-GPIOL_47-PadJ18)") (pinfunction "GPIOL_47") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e6201695-f39e-4fbe-9934-3172d0026116))
    (pad "J19" smd circle (at 6.8 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "unconnected-(U1D-VCCIO1C-PadJ19)") (pinfunction "VCCIO1C") (pintype "power_in") (solder_mask_margin 0.075) (tstamp df70dad0-7deb-4b98-949f-4104815ec2a6))
    (pad "J20" smd circle (at 7.6 -1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 307 "unconnected-(U1D-GPIOL_50-PadJ20)") (pinfunction "GPIOL_50") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d8939a33-d0b1-47da-ba67-38c28e0d466b))
    (pad "K1" smd circle (at -7.6 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 308 "unconnected-(U1K-DDR_BA2-PadK1)") (pinfunction "DDR_BA2") (pintype "output") (solder_mask_margin 0.075) (tstamp ca436bdc-a0ad-4fa4-ad67-71bc30c121a8))
    (pad "K2" smd circle (at -6.8 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 309 "unconnected-(U1K-DDR_BA2-PadK2)") (pinfunction "DDR_BA2") (pintype "output") (solder_mask_margin 0.075) (tstamp 54d8dba2-4b83-40b8-8967-395b1c51c8e3))
    (pad "K3" smd circle (at -6 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 310 "unconnected-(U1K-DDR_BA0-PadK3)") (pinfunction "DDR_BA0") (pintype "output") (solder_mask_margin 0.075) (tstamp 20bf61f6-1c5d-4c07-b65f-f5839c2057c8))
    (pad "K4" smd circle (at -5.2 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 311 "unconnected-(U1K-DDR_WE_N-PadK4)") (pinfunction "DDR_WE_N") (pintype "output") (solder_mask_margin 0.075) (tstamp 7ae65a67-0b11-468a-ba1c-6b44702b8445))
    (pad "K5" smd circle (at -4.4 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 312 "unconnected-(U1J-GPIOR_128_CLK13-PadK5)") (pinfunction "GPIOR_128_CLK13") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6bde6e10-7b5f-4c1c-8a12-1f69aa35f0ee))
    (pad "K6" smd circle (at -3.6 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 313 "unconnected-(U1J-GPIOR_136_CTRL9-PadK6)") (pinfunction "GPIOR_136_CTRL9") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5914b1f1-0416-448a-a42c-55d0c04e6802))
    (pad "K7" smd circle (at -2.8 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 314 "unconnected-(U1J-GPIOR_137_CTRL8-PadK7)") (pinfunction "GPIOR_137_CTRL8") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ee91fbe8-623d-444c-a847-0776322e2d56))
    (pad "K8" smd circle (at -2 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 315 "unconnected-(U1O-VCC-PadK8)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp b49bafcd-2d77-4e8b-8f54-9f1c4e1a1ee8))
    (pad "K9" smd circle (at -1.2 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 316 "unconnected-(U1O-VCC-PadK9)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 9d7dd71e-29f1-4a66-a3ef-5900b679e4e4))
    (pad "K10" smd circle (at -0.4 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 317 "unconnected-(U1O-VCC-PadK10)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp f322a5f0-ac72-4747-84ab-84fe3b6e8b77))
    (pad "K11" smd circle (at 0.4 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 318 "unconnected-(U1O-VCC-PadK11)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp e4e11fcb-df1e-418d-bd02-98a6173c1673))
    (pad "K12" smd circle (at 1.2 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 319 "unconnected-(U1O-VCC-PadK12)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 150cf590-2b77-4ecb-8302-2c32a1ebe0f6))
    (pad "K13" smd circle (at 2 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 320 "unconnected-(U1O-VCC-PadK13)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 4d951efa-5f97-4a66-851f-16d045427778))
    (pad "K14" smd circle (at 2.8 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 321 "unconnected-(U1D-GPIOL_49-PadK14)") (pinfunction "GPIOL_49") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 270a274f-184a-4af8-b021-b54daf9a1164))
    (pad "K15" smd circle (at 3.6 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 322 "unconnected-(U1C-GPIOL_45-PadK15)") (pinfunction "GPIOL_45") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 118bccd8-3309-4d9d-bd86-adcfe8da4cda))
    (pad "K16" smd circle (at 4.4 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 323 "unconnected-(U1C-GPIOL_44-PadK16)") (pinfunction "GPIOL_44") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b6ad1d67-b125-4945-aaaf-0e0118cf42dc))
    (pad "K17" smd circle (at 5.2 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 324 "unconnected-(U1C-GPIOL_43-PadK17)") (pinfunction "GPIOL_43") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 840d1383-cd4d-491b-980c-ac1191c30c9e))
    (pad "K18" smd circle (at 6 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 325 "unconnected-(U1C-GPIOL_42-PadK18)") (pinfunction "GPIOL_42") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1bb5fa5c-881f-408f-8ea2-1732072657db))
    (pad "K19" smd circle (at 6.8 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 326 "unconnected-(U1D-GPIOL_46-PadK19)") (pinfunction "GPIOL_46") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c79ba986-df33-4ef7-a9c2-ab562845d870))
    (pad "K20" smd circle (at 7.6 -0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 327 "unconnected-(U1D-GPIOL_48-PadK20)") (pinfunction "GPIOL_48") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6cda067a-a68d-4ad9-9da9-99c1cb01b2ce))
    (pad "L1" smd circle (at -7.6 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "unconnected-(U1K-DDR_DQ14-PadL1)") (pinfunction "DDR_DQ14") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp df23b1df-a378-448f-9221-1975f47c1f76))
    (pad "L2" smd circle (at -6.8 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 329 "unconnected-(U1K-DDR_DQ13-PadL2)") (pinfunction "DDR_DQ13") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 53ab43c5-1d71-4e29-8d72-95d236819ed8))
    (pad "L3" smd circle (at -6 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "unconnected-(U1K-DDR_DQ12-PadL3)") (pinfunction "DDR_DQ12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 195a6f84-9a91-4712-b167-fe735aea535e))
    (pad "L4" smd circle (at -5.2 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 331 "unconnected-(U1K-DDR_RST_N-PadL4)") (pinfunction "DDR_RST_N") (pintype "output") (solder_mask_margin 0.075) (tstamp 5e2a6a1e-4e6b-4da0-b689-6b57fbfc1d24))
    (pad "L5" smd circle (at -4.4 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 332 "unconnected-(U1A-GND-PadL5)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 3a11dfa4-a5cd-45e7-8884-904c9f0e2406))
    (pad "L6" smd circle (at -3.6 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 333 "unconnected-(U1K-DDR_ODT-PadL6)") (pinfunction "DDR_ODT") (pintype "output") (solder_mask_margin 0.075) (tstamp 0bddccc5-ec58-49d5-9341-594dce60f7d7))
    (pad "L7" smd circle (at -2.8 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 334 "unconnected-(U1K-VCCIO_DDR-PadL7)") (pinfunction "VCCIO_DDR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp edd27f8d-afe8-4794-b3c6-c37789c8de65))
    (pad "L8" smd circle (at -2 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 335 "unconnected-(U1A-GND-PadL8)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 3f69edad-fe80-4634-8e6e-87d773030ddd))
    (pad "L9" smd circle (at -1.2 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 336 "unconnected-(U1A-GND-PadL9)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 394e195c-c486-4978-80f3-efcbca68d52b))
    (pad "L10" smd circle (at -0.4 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 337 "unconnected-(U1A-GND-PadL10)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 3377cce8-fcc1-4514-8c1f-05ac799e8277))
    (pad "L11" smd circle (at 0.4 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 338 "unconnected-(U1A-GND-PadL11)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp c2856322-57d4-4c25-b5da-20ebbc4dc799))
    (pad "L12" smd circle (at 1.2 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 339 "unconnected-(U1A-GND-PadL12)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp cfe93eb0-a052-413f-8315-28e7afc23074))
    (pad "L13" smd circle (at 2 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 340 "unconnected-(U1A-GND-PadL13)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 816480b0-d644-4877-8372-7f9d17383872))
    (pad "L14" smd circle (at 2.8 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 341 "unconnected-(U1C-GPIOL_41-PadL14)") (pinfunction "GPIOL_41") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 23e051ea-2a4d-44b5-9307-01a26406921a))
    (pad "L15" smd circle (at 3.6 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 342 "unconnected-(U1C-GPIOL_37-PadL15)") (pinfunction "GPIOL_37") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e5b3f982-a883-44c5-8d1f-fdb00221fdcb))
    (pad "L16" smd circle (at 4.4 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 343 "unconnected-(U1C-VCCIO1B-PadL16)") (pinfunction "VCCIO1B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 0fc85dd5-0527-4cae-82af-b48a780df36d))
    (pad "L17" smd circle (at 5.2 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 344 "unconnected-(U1C-GPIOL_36-PadL17)") (pinfunction "GPIOL_36") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4986d99c-b8ad-4dd7-9622-516fb7774053))
    (pad "L18" smd circle (at 6 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 345 "unconnected-(U1C-GPIOL_40-PadL18)") (pinfunction "GPIOL_40") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c4eeaa42-75aa-4364-9411-eed72e4d0a90))
    (pad "L19" smd circle (at 6.8 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 346 "unconnected-(U1C-VCCIO1B-PadL19)") (pinfunction "VCCIO1B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp e3cd3b8b-2e8b-4cac-81bb-6cdd2b68bd60))
    (pad "L20" smd circle (at 7.6 0.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 347 "unconnected-(U1C-GPIOL_39-PadL20)") (pinfunction "GPIOL_39") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 82059876-51cd-4ce3-8271-3e60de1a4b52))
    (pad "M1" smd circle (at -7.6 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 348 "unconnected-(U1K-DDR_DQ15-PadM1)") (pinfunction "DDR_DQ15") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp a3d4d306-70d1-472a-96fb-6883fdc7633f))
    (pad "M2" smd circle (at -6.8 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 349 "unconnected-(U1A-GND-PadM2)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp cdf38bc9-1d2b-4f8d-8e11-b85361f77390))
    (pad "M3" smd circle (at -6 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 350 "unconnected-(U1K-DDR_DQS_N1-PadM3)") (pinfunction "DDR_DQS_N1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 972b1d17-80dd-4ae2-82d8-ddfe0c08d171))
    (pad "M4" smd circle (at -5.2 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 351 "unconnected-(U1K-DDR_RAS_N-PadM4)") (pinfunction "DDR_RAS_N") (pintype "output") (solder_mask_margin 0.075) (tstamp 52514394-ee83-42f6-8316-471b0765bd68))
    (pad "M5" smd circle (at -4.4 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 352 "unconnected-(U1K-DDR_A15-PadM5)") (pinfunction "DDR_A15") (pintype "output") (solder_mask_margin 0.075) (tstamp f43b2d6f-76b3-4d5c-8909-d9a9b65f257c))
    (pad "M6" smd circle (at -3.6 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 353 "unconnected-(U1K-DDR_A13-PadM6)") (pinfunction "DDR_A13") (pintype "output") (solder_mask_margin 0.075) (tstamp 6836c243-54e0-4e8c-8d40-be3421e52928))
    (pad "M7" smd circle (at -2.8 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 354 "unconnected-(U1A-GND-PadM7)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 307b5a69-6034-404a-be1b-6192cda08b92))
    (pad "M8" smd circle (at -2 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 355 "unconnected-(U1O-VCC-PadM8)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 4a70e536-7029-400a-85f4-f5dc1449eef3))
    (pad "M9" smd circle (at -1.2 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 356 "unconnected-(U1O-VCC-PadM9)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp e32fda7e-64ee-4870-b0ad-725171813f3d))
    (pad "M10" smd circle (at -0.4 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 357 "unconnected-(U1O-VCC-PadM10)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 1ee9fa92-4eae-40ba-a150-7e73251af0d0))
    (pad "M11" smd circle (at 0.4 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 358 "unconnected-(U1O-VCC-PadM11)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 7b1ee2d2-9bbb-4ab5-9531-c382891e360a))
    (pad "M12" smd circle (at 1.2 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 359 "unconnected-(U1O-VCC-PadM12)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 1af43e23-84a3-4dc2-b1d2-2d7c6d05c20b))
    (pad "M13" smd circle (at 2 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 360 "unconnected-(U1O-VCC-PadM13)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp a1f0a379-b7ce-4ec8-978d-57496c14f3f5))
    (pad "M14" smd circle (at 2.8 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 361 "unconnected-(U1C-GPIOL_21-PadM14)") (pinfunction "GPIOL_21") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d4034801-d223-443d-90d4-1906a815bd6d))
    (pad "M15" smd circle (at 3.6 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 362 "unconnected-(U1C-GPIOL_31-PadM15)") (pinfunction "GPIOL_31") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 50be210c-d6af-4642-8afa-68415a387ca4))
    (pad "M16" smd circle (at 4.4 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 363 "unconnected-(U1C-GPIOL_34-PadM16)") (pinfunction "GPIOL_34") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6b2a8077-3d0f-475b-a883-541a5148161b))
    (pad "M17" smd circle (at 5.2 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 364 "unconnected-(U1C-GPIOL_32-PadM17)") (pinfunction "GPIOL_32") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2a3a1a67-7712-4d12-b0b5-98850fbcf857))
    (pad "M18" smd circle (at 6 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 365 "unconnected-(U1C-GPIOL_33-PadM18)") (pinfunction "GPIOL_33") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5b573217-1311-473c-be3d-e38abececdd2))
    (pad "M19" smd circle (at 6.8 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 366 "unconnected-(U1C-GPIOL_38-PadM19)") (pinfunction "GPIOL_38") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp dcfee2a4-ca41-4f3d-8ae1-3c74094dd4ca))
    (pad "M20" smd circle (at 7.6 1.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 367 "unconnected-(U1C-GPIOL_35-PadM20)") (pinfunction "GPIOL_35") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f0f0b58a-4bed-4621-8a47-e021bf5ed274))
    (pad "N1" smd circle (at -7.6 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 368 "unconnected-(U1K-DDR_DM1-PadN1)") (pinfunction "DDR_DM1") (pintype "output") (solder_mask_margin 0.075) (tstamp f7c161ae-f76f-4695-a8f4-2a0cb376a4bd))
    (pad "N2" smd circle (at -6.8 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 369 "unconnected-(U1K-DDR_DQ11-PadN2)") (pinfunction "DDR_DQ11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 75fa5026-6038-4145-89f6-26f87d25516d))
    (pad "N3" smd circle (at -6 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 370 "unconnected-(U1K-DDR_DQS1-PadN3)") (pinfunction "DDR_DQS1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 10a7a90a-fa6b-4f78-86f9-70d25048e4aa))
    (pad "N4" smd circle (at -5.2 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 371 "unconnected-(U1K-DDR_A14-PadN4)") (pinfunction "DDR_A14") (pintype "output") (solder_mask_margin 0.075) (tstamp 57e257ac-2406-4e62-96de-b42c84747850))
    (pad "N5" smd circle (at -4.4 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 372 "unconnected-(U1K-DDR_A11-PadN5)") (pinfunction "DDR_A11") (pintype "output") (solder_mask_margin 0.075) (tstamp c1294674-5e56-40ba-82f5-f77f7359efd5))
    (pad "N6" smd circle (at -3.6 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 373 "unconnected-(U1K-DDR_CKE-PadN6)") (pinfunction "DDR_CKE") (pintype "output") (solder_mask_margin 0.075) (tstamp cd256556-5dd0-4988-801f-847bb083dd9b))
    (pad "N7" smd circle (at -2.8 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 374 "unconnected-(U1K-VCCIO_DDR-PadN7)") (pinfunction "VCCIO_DDR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp f4f0da60-d0c0-4097-896e-31410b9d075f))
    (pad "N8" smd circle (at -2 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 375 "unconnected-(U1A-GND-PadN8)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 3c9ef198-69cc-4c3c-9ad8-ffe2016130a7))
    (pad "N9" smd circle (at -1.2 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 376 "unconnected-(U1A-GND-PadN9)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 87496b88-ee9d-4d99-9800-773698aff86c))
    (pad "N10" smd circle (at -0.4 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 377 "unconnected-(U1A-GND-PadN10)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 872c4541-b098-4169-a580-119938d5a83c))
    (pad "N11" smd circle (at 0.4 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 378 "unconnected-(U1A-GND-PadN11)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp d239d0d2-a8f2-42c1-a0f5-343c79602008))
    (pad "N12" smd circle (at 1.2 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 379 "unconnected-(U1A-GND-PadN12)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp c6ff4937-76db-4320-98a5-e84e7dba83a7))
    (pad "N13" smd circle (at 2 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 380 "unconnected-(U1A-GND-PadN13)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 73945353-a319-4070-90ea-278f1c5fc4e6))
    (pad "N14" smd circle (at 2.8 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 381 "unconnected-(U1C-GPIOL_17_EXTFB0-PadN14)") (pinfunction "GPIOL_17_EXTFB0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2ab78afb-03b0-4d1b-be23-297df308f085))
    (pad "N15" smd circle (at 3.6 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 382 "unconnected-(U1C-GPIOL_20_CDI5-PadN15)") (pinfunction "GPIOL_20_CDI5") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c9da6f7b-c9ea-4f1c-82cc-6f2ca9b5c952))
    (pad "N16" smd circle (at 4.4 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 383 "unconnected-(U1C-GPIOL_27-PadN16)") (pinfunction "GPIOL_27") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2d9681d2-1aa9-4b70-839f-b039d338daf6))
    (pad "N17" smd circle (at 5.2 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 384 "unconnected-(U1C-GPIOL_30-PadN17)") (pinfunction "GPIOL_30") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 52089476-90ef-47e5-a601-47c5dbfb3a46))
    (pad "N18" smd circle (at 6 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 385 "unconnected-(U1C-GPIOL_28-PadN18)") (pinfunction "GPIOL_28") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 98cb44c7-22fe-4f29-84a3-48de355fb788))
    (pad "N19" smd circle (at 6.8 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 386 "unconnected-(U1C-VCCIO1B-PadN19)") (pinfunction "VCCIO1B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp dae8fb38-6b5b-480d-8e2b-a333fe6a7d7f))
    (pad "N20" smd circle (at 7.6 2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 387 "unconnected-(U1C-GPIOL_29-PadN20)") (pinfunction "GPIOL_29") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp cb1c8c12-ad71-4b72-b9dc-8d75044d1667))
    (pad "P1" smd circle (at -7.6 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 388 "unconnected-(U1K-DDR_DQ8-PadP1)") (pinfunction "DDR_DQ8") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3817e681-6752-45cc-b9c9-0b69511c0e06))
    (pad "P2" smd circle (at -6.8 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 389 "unconnected-(U1K-DDR_DQ9-PadP2)") (pinfunction "DDR_DQ9") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 97d3d2ad-4549-41b4-a41e-2a2fec23b437))
    (pad "P3" smd circle (at -6 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 390 "unconnected-(U1K-DDR_D10-PadP3)") (pinfunction "DDR_D10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 095c3d6d-157b-4716-a8e0-d2125635f1c3))
    (pad "P4" smd circle (at -5.2 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 391 "unconnected-(U1K-DDR_A12-PadP4)") (pinfunction "DDR_A12") (pintype "output") (solder_mask_margin 0.075) (tstamp 08ff87ef-fc82-4f00-b7d3-9f4c561856c7))
    (pad "P5" smd circle (at -4.4 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 392 "unconnected-(U1K-VCCIO_DDR-PadP5)") (pinfunction "VCCIO_DDR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 8341b73d-23f2-42aa-bd20-98f212f43d2f))
    (pad "P6" smd circle (at -3.6 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 393 "unconnected-(U1K-DDR_CAS_N-PadP6)") (pinfunction "DDR_CAS_N") (pintype "output") (solder_mask_margin 0.075) (tstamp da2978d4-6165-4255-9f95-6a59e95ba729))
    (pad "P7" smd circle (at -2.8 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 394 "unconnected-(U1A-GND-PadP7)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 4adb9f3e-46be-43b0-b976-f7f10a040646))
    (pad "P8" smd circle (at -2 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 395 "unconnected-(U1O-VCC-PadP8)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 1fa51ab0-51e1-41e2-b0e3-1fb154084589))
    (pad "P9" smd circle (at -1.2 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 396 "unconnected-(U1O-VCC-PadP9)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 92721cd6-74eb-45cb-9e3d-7552d1f76a10))
    (pad "P10" smd circle (at -0.4 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 397 "unconnected-(U1O-VCC-PadP10)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp afa8caee-6e65-40b6-9565-25e200d3e841))
    (pad "P11" smd circle (at 0.4 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 398 "unconnected-(U1O-VCC-PadP11)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 83548d2f-289e-4667-a3dc-b226f6df86dd))
    (pad "P12" smd circle (at 1.2 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 399 "unconnected-(U1O-VCC-PadP12)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp f659efc2-053f-45d3-a2d7-b0ece8555ec8))
    (pad "P13" smd circle (at 2 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 400 "unconnected-(U1O-VCC-PadP13)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 4ebca951-ed82-40c1-8108-b5ef638cd4af))
    (pad "P14" smd circle (at 2.8 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 401 "unconnected-(U1B-GPIOL_10-PadP14)") (pinfunction "GPIOL_10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 400632a5-764c-4a10-8734-fd092ec9fabf))
    (pad "P15" smd circle (at 3.6 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 402 "unconnected-(U1C-GPIOL_14_CDI2-PadP15)") (pinfunction "GPIOL_14_CDI2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fb150590-804d-435c-af9f-347ddfab42d8))
    (pad "P16" smd circle (at 4.4 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 403 "unconnected-(U1C-GPIOL_19_PLLIN1-PadP16)") (pinfunction "GPIOL_19_PLLIN1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f320a7fa-35bb-4db5-b28e-6077e76fd2d4))
    (pad "P17" smd circle (at 5.2 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 404 "unconnected-(U1A-GND-PadP17)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 763fecaf-2801-49a1-ae0a-9f95672d4b06))
    (pad "P18" smd circle (at 6 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 405 "unconnected-(U1C-GPIOL_22_CDI6-PadP18)") (pinfunction "GPIOL_22_CDI6") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2da050ec-c5d9-4a29-8e16-463db127c1b5))
    (pad "P19" smd circle (at 6.8 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 406 "unconnected-(U1C-GPIOL_26-PadP19)") (pinfunction "GPIOL_26") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5ae48ee5-f2ff-4448-81ac-9338093170d7))
    (pad "P20" smd circle (at 7.6 2.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 407 "unconnected-(U1C-GPIOL_25-PadP20)") (pinfunction "GPIOL_25") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 97f3ce68-a87f-42a6-9385-44d63e32ccf5))
    (pad "R1" smd circle (at -7.6 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 408 "unconnected-(U1K-DDR_A8-PadR1)") (pinfunction "DDR_A8") (pintype "output") (solder_mask_margin 0.075) (tstamp fc19b6b2-144d-48d4-98c1-2e46ad83a6fe))
    (pad "R2" smd circle (at -6.8 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 409 "unconnected-(U1K-VCCIO_DDR-PadR2)") (pinfunction "VCCIO_DDR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp ca24d110-b989-46e1-adc5-ba8cb9506c6e))
    (pad "R3" smd circle (at -6 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 410 "unconnected-(U1K-DDR_CK-PadR3)") (pinfunction "DDR_CK") (pintype "output") (solder_mask_margin 0.075) (tstamp 6e6c5481-a0b1-4d3e-ad87-f9959af16866))
    (pad "R4" smd circle (at -5.2 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 411 "unconnected-(U1K-DDR_CK_N-PadR4)") (pinfunction "DDR_CK_N") (pintype "output") (solder_mask_margin 0.075) (tstamp 8c64a48b-2850-4e23-ace2-7b7919609f27))
    (pad "R5" smd circle (at -4.4 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 412 "unconnected-(U1K-DDR_A10-PadR5)") (pinfunction "DDR_A10") (pintype "output") (solder_mask_margin 0.075) (tstamp d5edaa2d-80f8-42cf-a321-352d0c4fde8d))
    (pad "R6" smd circle (at -3.6 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 413 "unconnected-(U1K-DDR_CS_N-PadR6)") (pinfunction "DDR_CS_N") (pintype "output") (solder_mask_margin 0.075) (tstamp c9583f03-e1fa-40cd-a1fa-d8d2f6336c23))
    (pad "R7" smd circle (at -2.8 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 414 "unconnected-(U1K-VCCIO_DDR-PadR7)") (pinfunction "VCCIO_DDR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp eb0f5c98-9744-4e15-bacf-7c4f2d564493))
    (pad "R8" smd circle (at -2 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 415 "unconnected-(U1P-VCCA_BR-PadR8)") (pinfunction "VCCA_BR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 6744b2e6-6935-49a1-a5df-0ff81cb8a1c9))
    (pad "R9" smd circle (at -1.2 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 416 "unconnected-(U1N-VCCIO_BR-PadR9)") (pinfunction "VCCIO_BR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp b4a47979-ef97-4a53-84cd-1e4898b3a6b7))
    (pad "R10" smd circle (at -0.4 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 417 "unconnected-(U1L-REF_RES_4A-PadR10)") (pinfunction "REF_RES_4A") (pintype "output") (solder_mask_margin 0.075) (tstamp 4ea0849c-b4bc-4d68-a392-14c41f8447ee))
    (pad "R11" smd circle (at 0.4 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 418 "unconnected-(U1A-GND-PadR11)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp f893ea5c-1eff-426a-8990-5e358c4dad16))
    (pad "R12" smd circle (at 1.2 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 419 "unconnected-(U1M-REF_RES_4B-PadR12)") (pinfunction "REF_RES_4B") (pintype "output") (solder_mask_margin 0.075) (tstamp 0d41a7a1-0af6-4ad4-9a00-e1a9707815f2))
    (pad "R13" smd circle (at 2 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 420 "unconnected-(U1P-VCCA_BL-PadR13)") (pinfunction "VCCA_BL") (pintype "power_in") (solder_mask_margin 0.075) (tstamp bbfdb7bb-0df9-4567-9854-12698f984bdd))
    (pad "R14" smd circle (at 2.8 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 421 "unconnected-(U1B-GPIOL_03-PadR14)") (pinfunction "GPIOL_03") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp cc915b1a-5b99-4954-b703-02f949f9ee30))
    (pad "R15" smd circle (at 3.6 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 422 "unconnected-(U1B-VCCIO1A-PadR15)") (pinfunction "VCCIO1A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp d0583303-a815-49b9-bb7a-32fc816d2f80))
    (pad "R16" smd circle (at 4.4 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 423 "unconnected-(U1C-GPIOL_15_PLLIN0-PadR16)") (pinfunction "GPIOL_15_PLLIN0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 553b9869-4248-421a-b2f2-0071d2c5505f))
    (pad "R17" smd circle (at 5.2 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 424 "unconnected-(U1C-GPIOL_16_CDI3-PadR17)") (pinfunction "GPIOL_16_CDI3") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5ecd13ba-5384-41ce-8a79-ebcfa6896e77))
    (pad "R18" smd circle (at 6 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 425 "unconnected-(U1C-GPIOL_18_CDI4-PadR18)") (pinfunction "GPIOL_18_CDI4") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 8099a2a1-518e-4895-8f56-710d635e82f7))
    (pad "R19" smd circle (at 6.8 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 426 "unconnected-(U1A-GND-PadR19)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 63282568-e9a2-42c7-986d-2da7701c569a))
    (pad "R20" smd circle (at 7.6 3.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 427 "unconnected-(U1C-GPIOL_23-PadR20)") (pinfunction "GPIOL_23") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0a255cc7-edf5-467b-9a0b-9c10d7e948e6))
    (pad "T1" smd circle (at -7.6 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 428 "unconnected-(U1K-DDR_A7-PadT1)") (pinfunction "DDR_A7") (pintype "output") (solder_mask_margin 0.075) (tstamp adff9ee1-6e4b-4a16-a8a0-2816f51059dd))
    (pad "T2" smd circle (at -6.8 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 429 "unconnected-(U1K-DDR_A9-PadT2)") (pinfunction "DDR_A9") (pintype "output") (solder_mask_margin 0.075) (tstamp 9df3a0ec-09e2-4e63-bedd-8e1d6455b541))
    (pad "T3" smd circle (at -6 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 430 "unconnected-(U1K-DDR_A4-PadT3)") (pinfunction "DDR_A4") (pintype "output") (solder_mask_margin 0.075) (tstamp b11488bd-be7a-41f7-b157-d133fbff2c8c))
    (pad "T4" smd circle (at -5.2 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 431 "unconnected-(U1K-DDR_A6-PadT4)") (pinfunction "DDR_A6") (pintype "output") (solder_mask_margin 0.075) (tstamp bd05ce2b-1a0f-4d4d-8f59-cd87e9a445da))
    (pad "T5" smd circle (at -4.4 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 432 "unconnected-(U1K-DDR_A5-PadT5)") (pinfunction "DDR_A5") (pintype "output") (solder_mask_margin 0.075) (tstamp 5428e019-73f2-4255-865e-32a19327f45a))
    (pad "T6" smd circle (at -3.6 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 433 "unconnected-(U1K-DDR_A3-PadT6)") (pinfunction "DDR_A3") (pintype "output") (solder_mask_margin 0.075) (tstamp f92b6f9f-b239-4d03-bf88-4a6e0280c2b4))
    (pad "T7" smd circle (at -2.8 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 434 "unconnected-(U1N-GPIOR_141-PadT7)") (pinfunction "GPIOR_141") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d6f4ad18-e48e-43b9-9239-9b0db88439da))
    (pad "T8" smd circle (at -2 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 435 "unconnected-(U1N-GPIOR_138_PLLIN0-PadT8)") (pinfunction "GPIOR_138_PLLIN0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 7554c936-22fc-42fd-a826-5bbb7ad3e17c))
    (pad "T9" smd circle (at -1.2 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 436 "unconnected-(U1N-GPIOR_139_PLLIN1-PadT9)") (pinfunction "GPIOR_139_PLLIN1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp e8b695b2-ba33-46d4-a6e7-a3b2a13d9d47))
    (pad "T10" smd circle (at -0.4 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 437 "unconnected-(U1L-GPIOB_TXN10-PadT10)") (pinfunction "GPIOB_TXN10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f47e781e-e6a1-4bba-ae0d-d5a6b7575646))
    (pad "T11" smd circle (at 0.4 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 438 "unconnected-(U1L-GPIOB_TXP10-PadT11)") (pinfunction "GPIOB_TXP10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6e8b723a-08a5-4f16-b3fc-c15639e49e53))
    (pad "T12" smd circle (at 1.2 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 439 "unconnected-(U1M-GPIOB_TXN05_CDI26-PadT12)") (pinfunction "GPIOB_TXN05_CDI26") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b57c7b66-7c98-4151-b390-018dc7242a50))
    (pad "T13" smd circle (at 2 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 440 "unconnected-(U1M-GPIOB_TXP05_CDI27-PadT13)") (pinfunction "GPIOB_TXP05_CDI27") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 06ead374-3830-46e7-969b-5fea056aa640))
    (pad "T14" smd circle (at 2.8 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 441 "unconnected-(U1M-VCCIO4B-PadT14)") (pinfunction "VCCIO4B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp bf9b7f65-7097-4bf7-a647-99a057bcab62))
    (pad "T15" smd circle (at 3.6 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 442 "unconnected-(U1B-GPIOL_02-PadT15)") (pinfunction "GPIOL_02") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0ef8ebd4-806f-418e-9b86-5162bffa6b50))
    (pad "T16" smd circle (at 4.4 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 443 "unconnected-(U1B-GPIOL_04_CSI-PadT16)") (pinfunction "GPIOL_04_CSI") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b82f95bf-d263-4b16-a4f9-9dc2fcbd947c))
    (pad "T17" smd circle (at 5.2 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 444 "unconnected-(U1B-GPIOL_05_CSO-PadT17)") (pinfunction "GPIOL_05_CSO") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c18bf16d-b8b8-4712-b966-184b09fab09a))
    (pad "T18" smd circle (at 6 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 445 "unconnected-(U1B-GPIOL_12_CBUS1-PadT18)") (pinfunction "GPIOL_12_CBUS1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 68e1a7bc-0cc6-4f07-b511-cd027960acc4))
    (pad "T19" smd circle (at 6.8 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 446 "unconnected-(U1B-CDONE-PadT19)") (pinfunction "CDONE") (pintype "output") (solder_mask_margin 0.075) (tstamp 7827a80a-7aff-496e-a272-bde44c8beae5))
    (pad "T20" smd circle (at 7.6 4.4) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 447 "unconnected-(U1C-GPIOL_24_CDI7-PadT20)") (pinfunction "GPIOL_24_CDI7") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d9f2a46d-3f2d-4da1-9f6c-31309efa67a8))
    (pad "U1" smd circle (at -7.6 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 448 "unconnected-(U1K-DDR_DQS_N0-PadU1)") (pinfunction "DDR_DQS_N0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp a3f36495-a3c4-47a2-b871-65ff7223548c))
    (pad "U2" smd circle (at -6.8 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 449 "unconnected-(U1K-DDR_DQ3-PadU2)") (pinfunction "DDR_DQ3") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 85d30bfc-21f9-4ff1-8ff8-d2ec055e6031))
    (pad "U3" smd circle (at -6 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 450 "unconnected-(U1K-DDR_DQ0-PadU3)") (pinfunction "DDR_DQ0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp db0e0e5f-1a0f-4700-8d36-cde2a539f80a))
    (pad "U4" smd circle (at -5.2 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 451 "unconnected-(U1K-DDR_A0-PadU4)") (pinfunction "DDR_A0") (pintype "output") (solder_mask_margin 0.075) (tstamp 07f9d21a-7d7e-4c40-89e2-74d9f77c38c3))
    (pad "U5" smd circle (at -4.4 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 452 "unconnected-(U1A-GND-PadU5)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp de6d3e62-e43e-473d-9efe-c28111454ccd))
    (pad "U6" smd circle (at -3.6 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 453 "unconnected-(U1L-GPIOB_TXN17_CDI10-PadU6)") (pinfunction "GPIOB_TXN17_CDI10") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9ed12922-68d7-4e5b-adf9-4b6bdbd46c15))
    (pad "U7" smd circle (at -2.8 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 454 "unconnected-(U1L-GPIOB_TXP17_CDI11-PadU7)") (pinfunction "GPIOB_TXP17_CDI11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 669200f5-c1b1-4346-913e-2cd12102658c))
    (pad "U8" smd circle (at -2 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 455 "unconnected-(U1A-GND-PadU8)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp d99acd95-2b37-4146-94d1-d9735f225c42))
    (pad "U9" smd circle (at -1.2 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 456 "unconnected-(U1N-GPIOR_139_PLLIN2-PadU9)") (pinfunction "GPIOR_139_PLLIN2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp defb3c28-2676-4dfc-9ff8-bc08935692a6))
    (pad "U10" smd circle (at -0.4 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 457 "unconnected-(U1L-GPIOB_TXN15_CDI14-PadU10)") (pinfunction "GPIOB_TXN15_CDI14") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fb16aa69-2077-4eb1-bd36-9707578000d9))
    (pad "U11" smd circle (at 0.4 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 458 "unconnected-(U1L-VCCIO4A-PadU11)") (pinfunction "VCCIO4A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 5ffc64a6-d843-4b47-8e44-03b8c64d2183))
    (pad "U12" smd circle (at 1.2 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 459 "unconnected-(U1M-GPIOB_TXN06_CDI24-PadU12)") (pinfunction "GPIOB_TXN06_CDI24") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 246b2d24-3881-42ae-916a-4597eecb0e3a))
    (pad "U13" smd circle (at 2 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 460 "unconnected-(U1M-GPIOB_TXP07_CDI23-PadU13)") (pinfunction "GPIOB_TXP07_CDI23") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4a3e0b8d-0d12-4297-9cf2-bb353d6a87d2))
    (pad "U14" smd circle (at 2.8 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 461 "unconnected-(U1M-GPIOB_TXP02-PadU14)") (pinfunction "GPIOB_TXP02") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 97689170-67b6-40a3-a308-ec8a827d1a27))
    (pad "U15" smd circle (at 3.6 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 462 "unconnected-(U1M-GPIOB_TXN00-PadU15)") (pinfunction "GPIOB_TXN00") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ef9d1b31-4ecd-4d68-924f-2c48e1123b62))
    (pad "U16" smd circle (at 4.4 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 463 "unconnected-(U1A-GND-PadU16)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp f670c79b-1b32-454f-b95d-0e9edb635f10))
    (pad "U17" smd circle (at 5.2 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 464 "unconnected-(U1B-GPIOL_06-PadU17)") (pinfunction "GPIOL_06") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 48bd55a7-6ae0-4537-877a-7d67e4d813b5))
    (pad "U18" smd circle (at 6 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 465 "unconnected-(U1B-GPIOL_11_CBUS0-PadU18)") (pinfunction "GPIOL_11_CBUS0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6f54c228-82f7-4cad-9535-be451fe6f5ae))
    (pad "U19" smd circle (at 6.8 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 466 "unconnected-(U1B-~{CRESET_N}-PadU19)") (pinfunction "~{CRESET_N}") (pintype "output") (solder_mask_margin 0.075) (tstamp e9816b3e-c824-4af6-b30a-70761d93e572))
    (pad "U20" smd circle (at 7.6 5.2) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 467 "unconnected-(U1B-TMS-PadU20)") (pinfunction "TMS") (pintype "input") (solder_mask_margin 0.075) (tstamp dae6eb92-9080-4924-a5c2-b44c9434250f))
    (pad "V1" smd circle (at -7.6 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 468 "unconnected-(U1K-DDR_DQS0-PadV1)") (pinfunction "DDR_DQS0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d16d4a24-ad86-40e8-9f4a-a887fc78659c))
    (pad "V2" smd circle (at -6.8 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 469 "unconnected-(U1A-GND-PadV2)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp e5273abb-9874-4ead-bb7f-b480b737436c))
    (pad "V3" smd circle (at -6 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 470 "unconnected-(U1K-DDR_DQ2-PadV3)") (pinfunction "DDR_DQ2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 44fce068-1574-49fc-8a2c-cb4f6c38db15))
    (pad "V4" smd circle (at -5.2 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 471 "unconnected-(U1K-DDR_VREF-PadV4)") (pinfunction "DDR_VREF") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 95c66601-99dc-4411-82a0-4c9fcde04ba0))
    (pad "V5" smd circle (at -4.4 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 472 "unconnected-(U1K-DDR_A2-PadV5)") (pinfunction "DDR_A2") (pintype "output") (solder_mask_margin 0.075) (tstamp 6595f0a2-31a7-4365-b54a-3dd11226559c))
    (pad "V6" smd circle (at -3.6 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 473 "unconnected-(U1L-GPIOB_TXP18_EXTFB_CDI9-PadV6)") (pinfunction "GPIOB_TXP18_EXTFB_CDI9") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3799973e-a47b-4248-aa48-dfef6ade7434))
    (pad "V7" smd circle (at -2.8 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 474 "unconnected-(U1L-GPIOB_TXN18_CDI8-PadV7)") (pinfunction "GPIOB_TXN18_CDI8") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0140afc2-a800-49dd-8740-a73a301a9a0b))
    (pad "V8" smd circle (at -2 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 475 "unconnected-(U1L-GPIOB_TXN19-PadV8)") (pinfunction "GPIOB_TXN19") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 0d6c0a18-646b-4d91-971d-f168df667aab))
    (pad "V9" smd circle (at -1.2 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 476 "unconnected-(U1L-GPIOB_TXP19_CLK2-PadV9)") (pinfunction "GPIOB_TXP19_CLK2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 479e6d29-9442-4835-b5ce-b0c3543ed761))
    (pad "V10" smd circle (at -0.4 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 477 "unconnected-(U1L-GPIOB_TXP15_CLK1_CDI15-PadV10)") (pinfunction "GPIOB_TXP15_CLK1_CDI15") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9b2d6faa-6bf7-4597-8800-03985ca25f8c))
    (pad "V11" smd circle (at 0.4 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 478 "unconnected-(U1L-GPIOB_TXN11-PadV11)") (pinfunction "GPIOB_TXN11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c011fc4e-70ac-4179-8852-39e0ea581ecf))
    (pad "V12" smd circle (at 1.2 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 479 "unconnected-(U1M-GPIOB_TXP06_CDI25-PadV12)") (pinfunction "GPIOB_TXP06_CDI25") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 064d02a4-8281-403b-a129-bc60192f0c77))
    (pad "V13" smd circle (at 2 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 480 "unconnected-(U1M-GPIOB_TXN07_CDI22-PadV13)") (pinfunction "GPIOB_TXN07_CDI22") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 99797689-4904-4f9d-85a6-2a09bda9d7c8))
    (pad "V14" smd circle (at 2.8 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 481 "unconnected-(U1M-GPIOB_TXN02-PadV14)") (pinfunction "GPIOB_TXN02") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b95075f4-d364-4db1-9a3d-3957ad6ccde4))
    (pad "V15" smd circle (at 3.6 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 482 "unconnected-(U1M-GPIOB_TXP00-PadV15)") (pinfunction "GPIOB_TXP00") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 31691755-af03-4360-a201-b92db34ebf1f))
    (pad "V16" smd circle (at 4.4 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 483 "unconnected-(U1M-GPIOB_TXN03_CDI30-PadV16)") (pinfunction "GPIOB_TXN03_CDI30") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b36b4734-4b02-404d-8def-49835e724f54))
    (pad "V17" smd circle (at 5.2 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 484 "unconnected-(U1B-GPIOL_07-PadV17)") (pinfunction "GPIOL_07") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6b972311-9ebb-477d-b0cd-1410d6c552ea))
    (pad "V18" smd circle (at 6 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 485 "unconnected-(U1B-GPIOL_13_CBUS2-PadV18)") (pinfunction "GPIOL_13_CBUS2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 79d18d8b-e815-4a6d-add4-3d6425254542))
    (pad "V19" smd circle (at 6.8 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 486 "unconnected-(U1B-VCCIO1A-PadV19)") (pinfunction "VCCIO1A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 97bcfff1-1286-42c1-9526-c8e69e83992b))
    (pad "V20" smd circle (at 7.6 6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 487 "unconnected-(U1B-TDO-PadV20)") (pinfunction "TDO") (pintype "output") (solder_mask_margin 0.075) (tstamp 9899c208-c29d-4746-a98f-b804ea40ad9e))
    (pad "W1" smd circle (at -7.6 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 488 "unconnected-(U1K-DDR_DM0-PadW1)") (pinfunction "DDR_DM0") (pintype "output") (solder_mask_margin 0.075) (tstamp a91fd4c2-414a-4cc0-9b24-87851e6b38bc))
    (pad "W2" smd circle (at -6.8 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 489 "unconnected-(U1K-DDR_DQ4-PadW2)") (pinfunction "DDR_DQ4") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9f3cfd13-6f33-48a1-85d2-cb967c811c64))
    (pad "W3" smd circle (at -6 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 490 "unconnected-(U1K-DDR_DQ1-PadW3)") (pinfunction "DDR_DQ1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 958d7dee-d2f9-4ec8-b597-e0be6189dd7b))
    (pad "W4" smd circle (at -5.2 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 491 "unconnected-(U1K-VCCIO_DDR-PadW4)") (pinfunction "VCCIO_DDR") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 466ec926-07db-4397-802b-bb3dbab28aa8))
    (pad "W5" smd circle (at -4.4 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 492 "unconnected-(U1K-DDR_A1-PadW5)") (pinfunction "DDR_A1") (pintype "output") (solder_mask_margin 0.075) (tstamp 79dbc6f2-f1ba-48f8-8c59-4625f7f4e920))
    (pad "W6" smd circle (at -3.6 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 493 "unconnected-(U1L-GPIOB_TXN14_CDI16-PadW6)") (pinfunction "GPIOB_TXN14_CDI16") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 03ccf9d6-686e-40fa-bc2a-d80f2ec7a7b1))
    (pad "W7" smd circle (at -2.8 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 494 "unconnected-(U1L-VCCIO4A-PadW7)") (pinfunction "VCCIO4A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 83a26f0d-f37c-48d6-85bd-067f857f7af7))
    (pad "W8" smd circle (at -2 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 495 "unconnected-(U1L-GPIOB_TXN16_CDI12-PadW8)") (pinfunction "GPIOB_TXN16_CDI12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5d42a961-340a-4881-940f-4b3695ad9ec7))
    (pad "W9" smd circle (at -1.2 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 496 "unconnected-(U1L-GPIOB_TXP16_CDI13-PadW9)") (pinfunction "GPIOB_TXP16_CDI13") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp be21ec61-7b70-4b31-852b-12340212ac16))
    (pad "W10" smd circle (at -0.4 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 497 "unconnected-(U1L-VCCIO4A-PadW10)") (pinfunction "VCCIO4A") (pintype "power_in") (solder_mask_margin 0.075) (tstamp be3258fe-0aab-4e72-b7a5-c8eb500877df))
    (pad "W11" smd circle (at 0.4 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 498 "unconnected-(U1L-GPIOB_TXP11-PadW11)") (pinfunction "GPIOB_TXP11") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c901b3e8-dd60-443f-b380-e795c6707b5d))
    (pad "W12" smd circle (at 1.2 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 499 "unconnected-(U1M-VCCIO4B-PadW12)") (pinfunction "VCCIO4B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp f19b6fa5-c681-48c0-8da2-8c4e83ac8406))
    (pad "W13" smd circle (at 2 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 500 "unconnected-(U1M-GPIOB_TXN08_CDI20-PadW13)") (pinfunction "GPIOB_TXN08_CDI20") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3e59985b-1fdb-40ac-b7f7-7577711ac8e4))
    (pad "W14" smd circle (at 2.8 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 501 "unconnected-(U1M-GPIOB_TXN04_CDI28-PadW14)") (pinfunction "GPIOB_TXN04_CDI28") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6c31e692-4753-4e30-9661-b154f1709981))
    (pad "W15" smd circle (at 3.6 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 502 "unconnected-(U1M-VCCIO4B-PadW15)") (pinfunction "VCCIO4B") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 96b0750c-aea3-4217-aae3-eb2d97c678cc))
    (pad "W16" smd circle (at 4.4 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 503 "unconnected-(U1M-GPIOB_TXP03_CDI31-PadW16)") (pinfunction "GPIOB_TXP03_CDI31") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 2d3cad4b-a326-41a3-8301-4c967364200a))
    (pad "W17" smd circle (at 5.2 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 504 "unconnected-(U1A-VND-PadW17)") (pinfunction "VND") (pintype "passive") (solder_mask_margin 0.075) (tstamp a392cc89-3a85-49b3-a4eb-e28ef34b78d0))
    (pad "W18" smd circle (at 6 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 505 "unconnected-(U1B-GPIOL_00_SS_N-PadW18)") (pinfunction "GPIOL_00_SS_N") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1d5603be-3fe6-4e5c-abbe-c8aba1b81c09))
    (pad "W19" smd circle (at 6.8 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 506 "unconnected-(U1B-GPIOL_01_CCK-PadW19)") (pinfunction "GPIOL_01_CCK") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b01279d2-4552-413c-ae1b-1b28aa5d68ed))
    (pad "W20" smd circle (at 7.6 6.8) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 507 "unconnected-(U1B-TCK-PadW20)") (pinfunction "TCK") (pintype "input") (solder_mask_margin 0.075) (tstamp 9677e0ec-9145-4d08-8e07-237b44b18699))
    (pad "Y1" smd circle (at -7.6 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 508 "unconnected-(U1A-GND-PadY1)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 67793894-9837-4d3e-b3fe-577d07716bcc))
    (pad "Y2" smd circle (at -6.8 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 509 "unconnected-(U1K-DDR_DQ7-PadY2)") (pinfunction "DDR_DQ7") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1bf7fb3a-8061-4811-99f1-3a615e57c2c8))
    (pad "Y3" smd circle (at -6 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 510 "unconnected-(U1K-DDR_DQ5-PadY3)") (pinfunction "DDR_DQ5") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 95c9a3b9-00dc-4771-add4-4faf1e6a049c))
    (pad "Y4" smd circle (at -5.2 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 511 "unconnected-(U1K-DDR_DQ6-PadY4)") (pinfunction "DDR_DQ6") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 74c43c33-b0b6-4a87-bb99-f439cf9c3d38))
    (pad "Y5" smd circle (at -4.4 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 512 "unconnected-(U1K-DDR_ZQ-PadY5)") (pinfunction "DDR_ZQ") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp aa9f0f03-441c-4485-b224-b325df215c2e))
    (pad "Y6" smd circle (at -3.6 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 513 "unconnected-(U1L-GPIOB_TXP14_EXTFB1_CDI17-PadY6)") (pinfunction "GPIOB_TXP14_EXTFB1_CDI17") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b9e5ab00-18dd-4c32-a8b2-6bae7e183945))
    (pad "Y7" smd circle (at -2.8 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 514 "unconnected-(U1L-GPIOB_TXP13_CDI19-PadY7)") (pinfunction "GPIOB_TXP13_CDI19") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 8e3067f3-53ea-47f2-9f64-0f205b78fb4f))
    (pad "Y8" smd circle (at -2 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 515 "unconnected-(U1L-GPIOB_TXN13_CDI18-PadY8)") (pinfunction "GPIOB_TXN13_CDI18") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp c5e32056-0525-4c83-b7f9-fa1ffe79f1a6))
    (pad "Y9" smd circle (at -1.2 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 516 "unconnected-(U1L-GPIOB_TXN12-PadY9)") (pinfunction "GPIOB_TXN12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp ad3ab06c-22e2-4cc9-bb2b-79fbbe77d62b))
    (pad "Y10" smd circle (at -0.4 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 517 "unconnected-(U1L-GPIOB_TXP12-PadY10)") (pinfunction "GPIOB_TXP12") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fe387a46-eb62-4a88-9d0d-ad405a30306c))
    (pad "Y11" smd circle (at 0.4 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 518 "unconnected-(U1M-GPIOB_TXP09_CLK0-PadY11)") (pinfunction "GPIOB_TXP09_CLK0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 9e6f9f08-eb70-4eef-ab2e-358cc0c6b331))
    (pad "Y12" smd circle (at 1.2 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 519 "unconnected-(U1M-GPIOB_TXN09-PadY12)") (pinfunction "GPIOB_TXN09") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 3d0879ba-2981-4c1b-a202-1f2961d364e3))
    (pad "Y13" smd circle (at 2 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 520 "unconnected-(U1M-GPIOB_TXP08_EXTFB0_CDI21-PadY13)") (pinfunction "GPIOB_TXP08_EXTFB0_CDI21") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 835a9961-b810-47d6-9f58-addc1aa23168))
    (pad "Y14" smd circle (at 2.8 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 521 "unconnected-(U1M-GPIOB_TXP04_CDI29-PadY14)") (pinfunction "GPIOB_TXP04_CDI29") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 11745c78-e8b9-4f51-9fe7-c16f216d3286))
    (pad "Y15" smd circle (at 3.6 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 522 "unconnected-(U1M-GPIOB_TXN01-PadY15)") (pinfunction "GPIOB_TXN01") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp a5848f8c-ba60-4b2f-bc68-278a36b18bd9))
    (pad "Y16" smd circle (at 4.4 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 523 "unconnected-(U1M-GPIOB_TXP01-PadY16)") (pinfunction "GPIOB_TXP01") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 131511d9-2382-412d-923a-eb0797d4273d))
    (pad "Y17" smd circle (at 5.2 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 524 "unconnected-(U1B-GPIOL_08_CDI0-PadY17)") (pinfunction "GPIOL_08_CDI0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp fd6026c3-ed20-46de-9461-9138438ee579))
    (pad "Y18" smd circle (at 6 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 525 "unconnected-(U1B-GPIOL_09_CDI1-PadY18)") (pinfunction "GPIOL_09_CDI1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 739b849c-59fe-4691-aa1e-488cd67da57f))
    (pad "Y19" smd circle (at 6.8 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 526 "unconnected-(U1B-TDI-PadY19)") (pinfunction "TDI") (pintype "input") (solder_mask_margin 0.075) (tstamp 4ab53c34-254f-4acb-bfc5-9655d1763192))
    (pad "Y20" smd circle (at 7.6 7.6) (size 0.25 0.25) (property pad_prop_bga) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 527 "unconnected-(U1A-GND-PadY20)") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.075) (tstamp 93812a65-b6f9-4a55-b520-8b2418e7f13e))
    (model ":KICAD7_3DMODEL_DIR:Package_BGA.3dshapes/BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.9411764706 0.9411764706 0.9411764706))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:TSOT-23-5" (layer "F.Cu")
    (tstamp 8616c60c-38f2-42b1-b42d-d7d71d23b6a5)
    (at 170.3625 38.55)
    (descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSOT TO_SOT_SMD")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "power")
    (path "/03abecec-4724-420e-920e-986ba2580308/4cdee754-ec81-4f09-822a-68ccffecfdb6")
    (attr smd)
    (fp_text reference "U6" (at 0 -2.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0ed4f66-254a-4701-9c65-e3e285068c1f)
    )
    (fp_text value "~" (at 0 2.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ffba669b-94cb-4d23-9a51-cd1635f737e9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 0007a2c0-3f69-49d6-b406-2078ced1b287)
    )
    (fp_line (start 0 -1.56) (end -1.8 -1.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 540a0afa-3d9b-4595-a2af-bf9158395045))
    (fp_line (start 0 -1.56) (end 0.8 -1.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f430c5b-3714-4b63-89d1-0306edbc966b))
    (fp_line (start 0 1.56) (end -0.8 1.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2efc89a5-a2e1-4524-8ced-1d2e483bce72))
    (fp_line (start 0 1.56) (end 0.8 1.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72f8689e-a5a3-4157-9a81-91997ffad273))
    (fp_line (start -2.05 -1.7) (end -2.05 1.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 87ff20be-6dff-4d1d-8363-66883c3d09ef))
    (fp_line (start -2.05 1.7) (end 2.05 1.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c208fb62-5d74-4dd5-b1e9-266bb8b35307))
    (fp_line (start 2.05 -1.7) (end -2.05 -1.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c76257a-416d-4b1c-b8c2-c1427eecbc65))
    (fp_line (start 2.05 1.7) (end 2.05 -1.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f358f228-cf7c-4699-9971-f7048253f813))
    (fp_line (start -0.8 -1.05) (end -0.4 -1.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 33e5fadb-2d9f-4b5d-a324-9db08861a62f))
    (fp_line (start -0.8 1.45) (end -0.8 -1.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a73520dd-4419-4e0f-8fe5-0ccaf98ca4e8))
    (fp_line (start -0.4 -1.45) (end 0.8 -1.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3bf6daa1-f185-4769-9f8c-a7862d4655de))
    (fp_line (start 0.8 -1.45) (end 0.8 1.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d3ac0989-8818-4aee-955d-e040cf6fe71d))
    (fp_line (start 0.8 1.45) (end -0.8 1.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0e307c2a-82d7-429f-b13e-4d467ba53d9a))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 560 "unconnected-(U6-VIN-Pad1)") (pinfunction "VIN") (pintype "power_in") (tstamp 2c05503a-27c9-4f64-bf64-a13b4eadc1c7))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 561 "unconnected-(U6-GND-Pad2)") (pinfunction "GND") (pintype "passive") (tstamp ebf27ee3-18ca-4c5f-ad1f-6ba6f1c487b2))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 562 "unconnected-(U6-EN-Pad3)") (pinfunction "EN") (pintype "input") (tstamp 096b6b25-8119-4230-8554-7ada81af5381))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 563 "unconnected-(U6-ADJ-Pad4)") (pinfunction "ADJ") (pintype "input") (tstamp 1dcee22b-6825-4659-a389-cecf1d3e7742))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 564 "unconnected-(U6-VOUT-Pad5)") (pinfunction "VOUT") (pintype "power_out") (tstamp 74e8b242-008d-404c-9b20-be5e936a9180))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tstamp 87e11c04-f861-482c-b012-996c75761cd6)
    (at 69.15 55.1 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/b36eb261-dd9c-4a8f-9dab-abcc0de977a2")
    (attr through_hole)
    (fp_text reference "SW2" (at 0.945 -4.615 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 701f11f8-14cd-483a-9161-50188e604010)
    )
    (fp_text value "SW_Push" (at 3.75 6.7 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47126342-1889-418e-8288-7a504d477dce)
    )
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 22e68de1-691f-4167-9743-fb5a81d2f53c)
    )
    (fp_line (start -0.25 1.5) (end -0.25 3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 373faa3e-8b20-4d59-ae05-438ea58a93ef))
    (fp_line (start 1 5.5) (end 5.5 5.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8bdd01b-2ac3-4104-9554-6ba6d51333f5))
    (fp_line (start 5.5 -1) (end 1 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 354ead0d-ec23-41b3-87d1-a502e14e7677))
    (fp_line (start 6.75 3) (end 6.75 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e07c697-b693-49ae-adf8-7a16b42d38cf))
    (fp_line (start -1.5 -1.5) (end -1.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30bda271-5897-4d2b-a76c-ba4c53cea01d))
    (fp_line (start -1.5 -1.25) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8ba9c362-3b80-45cd-8baa-af627895909c))
    (fp_line (start -1.5 5.75) (end -1.5 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ecdc7175-1b38-41e3-90b1-2854f2a7a200))
    (fp_line (start -1.5 5.75) (end -1.5 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8056d6e6-5016-4470-b0dc-7363df996756))
    (fp_line (start -1.5 6) (end -1.25 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1d6acc83-b972-4a61-95b8-942bac73261b))
    (fp_line (start -1.25 -1.5) (end 7.75 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 092035f5-ba52-47ed-9fbf-e96fa353e240))
    (fp_line (start 7.75 -1.5) (end 8 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7209b893-7f61-4021-99f2-cbb1583df8b4))
    (fp_line (start 7.75 6) (end -1.25 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a2046f0e-9a9c-4aa7-9cf2-d188b0e277bd))
    (fp_line (start 7.75 6) (end 8 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 81b2405e-7b20-4146-8cf2-15dc50422c52))
    (fp_line (start 8 -1.5) (end 8 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b9d2595b-3513-47e6-9767-6bc97378bbad))
    (fp_line (start 8 -1.25) (end 8 5.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd627b97-4986-41fe-8dc7-ad0947550b6b))
    (fp_line (start 8 6) (end 8 5.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 88321c52-9b1d-4981-baf2-412a3d94bd39))
    (fp_line (start 0.25 -0.75) (end 3.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 425b0544-7456-407d-a43b-71ea140bf406))
    (fp_line (start 0.25 5.25) (end 0.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7adc68d1-4094-459e-9114-ede8b42a080d))
    (fp_line (start 3.25 -0.75) (end 6.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7bc70660-7e2d-4180-bacb-e049b1e46fe1))
    (fp_line (start 6.25 -0.75) (end 6.25 5.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff8c9561-49f9-4a17-a92e-0400fa19b04b))
    (fp_line (start 6.25 5.25) (end 0.25 5.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 47a0dc59-a26a-4888-8a80-1e56880971dd))
    (fp_circle (center 3.25 2.25) (end 1.25 2.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp bcaff6e6-9ebc-45d5-9ac3-f716af3e5006))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 124 "unconnected-(SW2-Pad1)") (pinfunction "1") (pintype "passive") (tstamp d4422ebf-804c-4970-8195-be7dd239ed9e))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 124 "unconnected-(SW2-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 7880e51f-9bf9-4547-8e9d-f12c4900de25))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 125 "unconnected-(SW2-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 093e9e42-d845-421d-b4fc-450f458adffb))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 125 "unconnected-(SW2-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 43b96b68-d0a9-44a7-a25b-ca6914037994))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-40_W15.24mm_Socket_LongPads" (layer "F.Cu")
    (tstamp 8a60d493-37ca-4356-883f-5ea82da3db05)
    (at 39.01 25.61)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "CMOS 6502 Processor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/b576d505-467a-4d98-8479-9819a9b39180")
    (attr through_hole)
    (fp_text reference "U7" (at 7.62 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 063df640-eb4a-47f8-b1d5-ed48f7acc0a1)
    )
    (fp_text value "W65C02P" (at 7.62 50.59) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6fa02b21-80cb-4ff7-a7a0-d48143edad82)
    )
    (fp_text user "${REFERENCE}" (at 7.62 24.13) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f03d971c-aebc-4ef9-b41a-e4fdfba49228)
    )
    (fp_line (start -1.44 -1.39) (end -1.44 49.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e265ed1-c172-4522-a9a2-6aae728d791b))
    (fp_line (start -1.44 49.65) (end 16.68 49.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6e1480b1-9c15-4b27-af5a-ea3d7f74a8b8))
    (fp_line (start 1.56 -1.33) (end 1.56 49.59)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e24fc701-d391-48da-babf-b858dcf4baea))
    (fp_line (start 1.56 49.59) (end 13.68 49.59)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9c5ed801-908f-4b45-9a3e-49e4dcc40260))
    (fp_line (start 6.62 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 22870715-f684-49f0-b217-662478b3b313))
    (fp_line (start 13.68 -1.33) (end 8.62 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81f281f3-b8d5-49ca-bfe1-3a49bc521ccd))
    (fp_line (start 13.68 49.59) (end 13.68 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 05dc6f1d-474e-46cf-b4eb-8eed0aaf1ab6))
    (fp_line (start 16.68 -1.39) (end -1.44 -1.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f5e83a8-0797-4741-869c-f53616507b03))
    (fp_line (start 16.68 49.65) (end 16.68 -1.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 55716e74-233a-45ca-abb5-d4ea9844c4cf))
    (fp_arc (start 8.62 -1.33) (mid 7.62 -0.33) (end 6.62 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d90ea4f-a06a-4cc9-b036-6abd36faf2fb))
    (fp_line (start -1.55 -1.6) (end -1.55 49.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d6aa4cd8-32a4-4875-b6e3-7e3cd64ae2b9))
    (fp_line (start -1.55 49.85) (end 16.8 49.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d9809a63-9d1e-4f76-97b7-bb7183ce1df3))
    (fp_line (start 16.8 -1.6) (end -1.55 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 937c4066-1dbb-465b-9ccb-50d507c66e5c))
    (fp_line (start 16.8 49.85) (end 16.8 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c76e5566-6e18-452a-8e66-fe893b2c02b5))
    (fp_line (start -1.27 -1.33) (end -1.27 49.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f24bfea0-7028-4a86-9a08-2a58ae92b477))
    (fp_line (start -1.27 49.59) (end 16.51 49.59)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 352fce87-1740-4478-9e2b-f9b4db5acdcf))
    (fp_line (start 0.255 -0.27) (end 1.255 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f858c488-d5d3-4f19-9770-4dbd9fc7dda4))
    (fp_line (start 0.255 49.53) (end 0.255 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 05eb7a8b-5b65-4b1a-b50f-cb93c281f1cd))
    (fp_line (start 1.255 -1.27) (end 14.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca09d9c8-72cd-4032-89fa-4d9e0a89cd1f))
    (fp_line (start 14.985 -1.27) (end 14.985 49.53)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e5af833-7476-4351-a174-d23404098053))
    (fp_line (start 14.985 49.53) (end 0.255 49.53)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dab6ae28-8f4c-4166-9641-1e76b32005a9))
    (fp_line (start 16.51 -1.33) (end -1.27 -1.33)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 903e83d2-ab38-4828-b409-d3fef495c890))
    (fp_line (start 16.51 49.59) (end 16.51 -1.33)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77a7181b-078a-4ff2-839b-539955dc9620))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 565 "/cpu/~{CPU_VPB}") (pinfunction "~{VPB}") (pintype "output") (tstamp d545ec7a-4ab4-4fbb-944d-84fd03560a94))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 566 "/cpu/CPU_RDY") (pinfunction "RDY") (pintype "input") (tstamp 80c72dde-4427-461d-867c-20acd997afd2))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 567 "unconnected-(U7-PHI1O-Pad3)") (pinfunction "PHI1O") (pintype "output+no_connect") (tstamp 49d3fc3e-9a7e-469f-be62-e30cd26fd3ba))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 568 "/cpu/~{CPU_IRQB}") (pinfunction "~{IRQB}") (pintype "input") (tstamp 7da7b6d4-49dd-4b03-9925-32e33847c764))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 569 "/cpu/~{CPU_MLB}") (pinfunction "~{MLB}") (pintype "output") (tstamp e409e7fa-3458-457a-8e88-a117bb8f701e))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 570 "/cpu/~{CPU_NMIB}") (pinfunction "~{NMIB}") (pintype "input") (tstamp a5ec0b4d-6450-4d12-a331-7412b905cf0d))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 571 "/cpu/CPU_SYNC") (pinfunction "SYNC") (pintype "output") (tstamp 1a921cf4-a761-4523-8602-be6d652e117a))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 572 "+3V3") (pinfunction "VDD") (pintype "power_in") (tstamp 179a6a51-2238-40d2-b1c8-8e7a1e0423d1))
    (pad "9" thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 573 "/cpu/CPU_ADDR0") (pinfunction "A0") (pintype "output") (tstamp 79ad555d-ff96-4540-8e8b-ce576690a8c7))
    (pad "10" thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 574 "/cpu/CPU_ADDR1") (pinfunction "A1") (pintype "output") (tstamp 8977c53e-ec28-4f4a-830d-f17a81bd24c8))
    (pad "11" thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 575 "/cpu/CPU_ADDR2") (pinfunction "A2") (pintype "output") (tstamp 5a788089-d143-4b5d-8259-df48d32802a6))
    (pad "12" thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 576 "/cpu/CPU_ADDR3") (pinfunction "A3") (pintype "output") (tstamp 49778f3b-c21d-4277-b8d8-96f78b5adcd7))
    (pad "13" thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 577 "/cpu/CPU_ADDR4") (pinfunction "A4") (pintype "output") (tstamp 3cfdedcd-cf3b-4bca-bd57-03d7be7b4ff3))
    (pad "14" thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 578 "/cpu/CPU_ADDR5") (pinfunction "A5") (pintype "output") (tstamp 5f9baf2f-907a-4c68-8705-ccd18c2ab610))
    (pad "15" thru_hole oval (at 0 35.56) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 579 "/cpu/CPU_ADDR6") (pinfunction "A6") (pintype "output") (tstamp fce41dcf-b4a0-450b-8e2e-357714b7a20b))
    (pad "16" thru_hole oval (at 0 38.1) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 580 "/cpu/CPU_ADDR7") (pinfunction "A7") (pintype "output") (tstamp d69a6db6-4078-4c81-b634-d2380b75e58b))
    (pad "17" thru_hole oval (at 0 40.64) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 581 "/cpu/CPU_ADDR8") (pinfunction "A8") (pintype "output") (tstamp fa40eed4-2329-451a-a597-1412670beecc))
    (pad "18" thru_hole oval (at 0 43.18) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 582 "/cpu/CPU_ADDR9") (pinfunction "A9") (pintype "output") (tstamp 00a4028c-86c8-4d7f-86ab-9f5cdcde9111))
    (pad "19" thru_hole oval (at 0 45.72) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 583 "/cpu/CPU_ADDR10") (pinfunction "A10") (pintype "output") (tstamp bcb3fdef-0639-485f-b0c2-febdfc350931))
    (pad "20" thru_hole oval (at 0 48.26) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 584 "/cpu/CPU_ADDR11") (pinfunction "A11") (pintype "output") (tstamp 26af3546-3640-49fa-acb9-6091aa295ae7))
    (pad "21" thru_hole oval (at 15.24 48.26) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 585 "GND") (pinfunction "VSS") (pintype "input") (tstamp 6e63abdf-7ed0-4868-98c5-1a844d6c5e4b))
    (pad "22" thru_hole oval (at 15.24 45.72) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 586 "/cpu/CPU_ADDR12") (pinfunction "A12") (pintype "output") (tstamp 770a60d9-5d60-4470-a0c2-1385fce62536))
    (pad "23" thru_hole oval (at 15.24 43.18) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 587 "/cpu/CPU_ADDR13") (pinfunction "A13") (pintype "output") (tstamp e452db94-8923-4749-b8c1-59e234e158fc))
    (pad "24" thru_hole oval (at 15.24 40.64) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 588 "/cpu/CPU_ADDR14") (pinfunction "A14") (pintype "output") (tstamp 3b378122-2732-4072-a4ee-15601f8f9d29))
    (pad "25" thru_hole oval (at 15.24 38.1) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 589 "/cpu/CPU_ADDR15") (pinfunction "A15") (pintype "output") (tstamp 5c374100-4a28-436c-a275-d14293daf125))
    (pad "26" thru_hole oval (at 15.24 35.56) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 590 "/cpu/CPU_DATA7") (pinfunction "D7") (pintype "bidirectional") (tstamp 8cd38d1c-783c-4072-896c-5fea9b3f5141))
    (pad "27" thru_hole oval (at 15.24 33.02) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 591 "/cpu/CPU_DATA6") (pinfunction "D6") (pintype "bidirectional") (tstamp ea0f6948-aa88-49a3-96d6-b6f40bd47c9d))
    (pad "28" thru_hole oval (at 15.24 30.48) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 592 "/cpu/CPU_DATA5") (pinfunction "D5") (pintype "bidirectional") (tstamp 78a7ce1a-c22e-42c2-bb7a-e4a6812b77c0))
    (pad "29" thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 593 "/cpu/CPU_DATA4") (pinfunction "D4") (pintype "bidirectional") (tstamp 6afd50b1-b7d9-42f7-a310-2725bd23f8d1))
    (pad "30" thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 594 "/cpu/CPU_DATA3") (pinfunction "D3") (pintype "bidirectional") (tstamp ba62bbaa-07d3-41e0-a123-e427dea2cbd9))
    (pad "31" thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 595 "/cpu/CPU_DATA2") (pinfunction "D2") (pintype "bidirectional") (tstamp c2584692-9b5e-4d51-a5a6-20ea5b7c2b0e))
    (pad "32" thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 596 "/cpu/CPU_DATA1") (pinfunction "D1") (pintype "bidirectional") (tstamp f90daefe-c746-47d9-9a1f-c66362b808e3))
    (pad "33" thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 597 "/cpu/CPU_DATA0") (pinfunction "D0") (pintype "bidirectional") (tstamp 37507a94-2a1d-4caa-b063-d0d3cf198858))
    (pad "34" thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 598 "/cpu/~{CPU_RWB}") (pinfunction "~{RWB}") (pintype "output") (tstamp 5a0d1f79-8a51-4b88-bf5d-88580069e9ae))
    (pad "35" thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 599 "unconnected-(U7-NC-Pad35)") (pinfunction "NC") (pintype "no_connect") (tstamp e71c0004-453d-4150-b5a1-9d00078d2d99))
    (pad "36" thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 600 "/cpu/CPU_BE") (pinfunction "BE") (pintype "input") (tstamp 0d92198f-deba-4a49-be26-3f2eaf948f83))
    (pad "37" thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 601 "/cpu/CPU_PHI2") (pinfunction "PHI2") (pintype "input") (tstamp bc37e02f-833e-49ec-aaba-96a94abbaf77))
    (pad "38" thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 602 "Net-(U7-~{SOB})") (pinfunction "~{SOB}") (pintype "input") (tstamp 1cfa24e0-3457-4d87-8d92-01d5f3fc859a))
    (pad "39" thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 603 "unconnected-(U7-PHI2O-Pad39)") (pinfunction "PHI2O") (pintype "output+no_connect") (tstamp f14143c9-3af2-445b-96ce-8a76ae10c9bb))
    (pad "40" thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 604 "/cpu/~{CPU_RESB}") (pinfunction "~{RESB}") (pintype "input") (tstamp 219c4d06-eb27-41cb-b395-1be27228c11f))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
      (offset (xyz 0 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp 926c93cc-1f94-4877-b312-01ec82e36e80)
    (at 75.14 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/1b6b6b4d-d070-46c8-861b-0daecfe35386")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ccee6a9f-b715-4b98-bb24-02516bb88dfb)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61fc32a8-6e96-43d5-a3bd-6b9ce9c28ad0)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 4257bd42-486b-4443-a617-f8663732eebf)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23f57d70-42de-4405-b31e-9051591aca00))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3a2b17a0-8c01-4589-b0c9-66a922d8ab00))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fa68786a-6af0-4933-8c4b-ca083cc5cd5a))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6d58ae5d-3291-49f6-877d-dba87b5a5c6c))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 621a17ac-9ebe-458e-8fa4-e94873cdb938))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 28fe877e-4e68-49bf-a921-7de5a2e1bb71))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76aead93-e0f2-4270-99f2-f98d474286ca))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c825bee4-4acc-428b-bfb5-f917fc1d4b44))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b410fd7c-e4e3-4394-b481-1635a9513eaf))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4629820e-f2d4-4850-a644-a811077efd03))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 32554e08-2d52-44a2-ab71-25e7fcb3885b))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d8aacfb4-4e43-4a7a-b2ab-7e57bb04d7d3))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "unconnected-(D4-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 41b84fab-cb49-4a3f-aa88-9db7356d21ab))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "unconnected-(D4-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp e175d7bd-1b0e-42d0-b7f7-798915cda59f))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tstamp 93c63e6f-f495-4f5c-a3b0-1410d8dc3ed7)
    (at 163.5625 24.95)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "power")
    (path "/03abecec-4724-420e-920e-986ba2580308/c53deff5-9fc8-433f-be38-77a50b5753ee")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a789da4-caf9-4fb3-9677-ab1da3d02fbc)
    )
    (fp_text value "~" (at 0 3.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e2035b86-feed-49a3-a2f1-7a4dd167dc2c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp f3b3f72f-05e1-42b6-abdd-ef939269ba60)
    )
    (fp_line (start 0 -2.56) (end -3.45 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b29719c8-7476-4da9-8173-11921234f771))
    (fp_line (start 0 -2.56) (end 1.95 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ff1bb1a-a0e7-42f7-9d12-64fd48252355))
    (fp_line (start 0 2.56) (end -1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c1907441-7558-4d44-9c46-7bc5e0c30113))
    (fp_line (start 0 2.56) (end 1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9a3221c-7434-45af-9df0-b1a6bf1c8ef1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3271c489-f89e-4f3c-aaae-bf3c155920f4))
    (fp_line (start -3.7 2.7) (end 3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 82f8cdfe-750e-492c-b4bc-50e54672106d))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 769f7579-9be6-4b95-8fac-791217ffeebb))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6a546673-f53f-4a22-a575-d511da718362))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b5468d6a-21ab-447d-94f3-c4df0e4332d9))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 04ec6fc0-b965-47cd-8d9c-9071a2c3444c))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea2fb0fe-2ec5-4d73-9698-cbd86025d069))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a5a058cd-4019-430a-8c7a-fc4a0e26ca52))
    (fp_line (start 1.95 2.45) (end -1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a4e2a3b-63af-46da-9f3a-517e85c69ccf))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 536 "unconnected-(U3-SW-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp 4dd9ebd8-799a-405d-90d3-e74904b9dde5))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 537 "unconnected-(U3-PGND-Pad2)") (pinfunction "PGND") (pintype "passive") (tstamp c55ec93e-f8d6-48aa-93a0-f883984412b4))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 538 "unconnected-(U3-VINA-Pad3)") (pinfunction "VINA") (pintype "power_in") (tstamp 0ea83ea6-384f-48e9-930a-9eafb6e7a540))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 539 "unconnected-(U3-EN-Pad4)") (pinfunction "EN") (pintype "input") (tstamp 8f997e50-f33e-40de-92f1-0e3317a3a59b))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 540 "unconnected-(U3-FB-Pad5)") (pinfunction "FB") (pintype "input") (tstamp 173a70e4-7e44-4a17-a5fc-2935b99d0e4b))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 541 "unconnected-(U3-AGND-Pad6)") (pinfunction "AGND") (pintype "passive") (tstamp 8bde9cab-d039-445b-a952-82c56d34b1cf))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 542 "unconnected-(U3-GND-Pad7)") (pinfunction "GND") (pintype "passive") (tstamp 8bb8772a-4e99-42f1-85c8-aa28df3f926e))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 543 "unconnected-(U3-VINSW-Pad8)") (pinfunction "VINSW") (pintype "power_in") (tstamp 7a8c42d3-74b5-4292-850d-859799871a8d))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Display_7Segment:LTS-4802B" (layer "F.Cu")
    (tstamp 96a0e913-24bb-46e8-9d98-a66633811f44)
    (at 73 90.34)
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/40f2559a-79d8-423b-8462-953cc6e6de48")
    (attr through_hole)
    (fp_text reference "U13" (at 0 -2.54 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3a23485c-c24e-4c07-9523-f52f76bd9068)
    )
    (fp_text value "~" (at 3.58 13.1 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 47012bbf-b548-4d0b-a72a-5de3284a3b52)
    )
    (fp_text user "${REFERENCE}" (at 3.58 4.01 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c0154eb-d0d6-4ecd-a31f-0d764449da55)
    )
    (fp_rect (start -1.04 -1.07) (end 8.66 11.83)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 9820f9b6-76d5-40fa-aad3-f54a7cd3442b))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 761 "unconnected-(U13-CA-Pad1)") (pinfunction "CA") (pintype "passive") (tstamp 4c382d89-5bf2-4d15-af09-d81ccd0d087d))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 762 "unconnected-(U13-F-Pad2)") (pinfunction "F") (pintype "passive") (tstamp 3eb43ea5-f4ff-4867-9ab1-b1f48f089f95))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 763 "unconnected-(U13-G-Pad3)") (pinfunction "G") (pintype "passive") (tstamp 2c7fd6f1-62ce-4c88-bbf6-a9ec8de1419f))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 764 "unconnected-(U13-E-Pad4)") (pinfunction "E") (pintype "passive") (tstamp a97321e7-013c-441e-9c3c-35b2bfaad4e5))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 765 "unconnected-(U13-D-Pad5)") (pinfunction "D") (pintype "passive") (tstamp 6f749e87-ec10-4190-b00b-edcf6a293259))
    (pad "6" thru_hole circle (at 7.62 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 766 "unconnected-(U13-CA-Pad6)") (pinfunction "CA") (pintype "passive") (tstamp 993a4aa2-af9c-49da-8562-7d96ee9dc047))
    (pad "7" thru_hole circle (at 7.62 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 767 "unconnected-(U13-DP-Pad7)") (pinfunction "DP") (pintype "passive") (tstamp f1925f94-82e7-401e-a4cd-abbfc6d33b48))
    (pad "8" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 768 "unconnected-(U13-C-Pad8)") (pinfunction "C") (pintype "passive") (tstamp 80526353-d5b3-4b53-82df-9a2bf4e4ce5e))
    (pad "9" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 769 "unconnected-(U13-B-Pad9)") (pinfunction "B") (pintype "passive") (tstamp 8d412cd8-f792-47bc-82eb-21a59a8c48b5))
    (pad "10" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 770 "unconnected-(U13-A-Pad10)") (pinfunction "A") (pintype "passive") (tstamp 9d7cb9bd-e23e-4c33-a982-1f0cfdc18659))
    (model ":KICAD7_3DMODEL_DIR:Display_7Segment.3dshapes/LTS-4802BJR-H1_LTO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_THT:SW_DIP_SPSTx08_Slide_6.7x21.88mm_W7.62mm_P2.54mm_LowProfile" (layer "F.Cu")
    (tstamp 96e6fcc9-4240-4f3b-b4c7-254e6aa3c685)
    (at 69 74.07 90)
    (descr "8x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x21.88mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile")
    (tags "DIP Switch SPST Slide 7.62mm 300mil LowProfile")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "8x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
    (property "ki_keywords" "dip switch")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/d0e637f6-3f43-43a9-a187-c0b47d7eadaf")
    (attr through_hole)
    (fp_text reference "SW1" (at 0.585 -6.765 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7bd4463b-5969-4363-a2ea-41ae68b595f4)
    )
    (fp_text value "SW_DIP_x08" (at 3.81 20.89 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 248ecb93-6edb-453e-b068-3f5eedbc48f7)
    )
    (fp_text user "on" (at 5.085 -5.015 90) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 10865e9a-895a-4fdc-ab2a-99470fe60d6e)
    )
    (fp_text user "${REFERENCE}" (at 6.39 8.89) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 1ac8f71b-8233-4899-a78e-d7d18b426745)
    )
    (fp_line (start 0.16 -2.35) (end 0.16 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1d1680e3-3cf9-4e31-aefe-9c9134d95ec3))
    (fp_line (start 0.16 -2.35) (end 1.543 -2.35)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6b98f1e-7004-479c-9ac2-4859fcf2c0d2))
    (fp_line (start 0.4 -2.11) (end 0.4 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 28be74fc-4b45-414d-afbe-320f643ee577))
    (fp_line (start 0.4 -2.11) (end 7.221 -2.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 564c600d-1b55-4337-9de9-e7470b2ef153))
    (fp_line (start 0.4 1.04) (end 0.4 1.551)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1415d51f-d582-4bef-91d5-4889b9f45bad))
    (fp_line (start 0.4 3.53) (end 0.4 4.091)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ba2e917-0555-449c-a584-871c6825a49f))
    (fp_line (start 0.4 6.07) (end 0.4 6.631)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e99f561b-11d5-4918-9085-c41260aedbc0))
    (fp_line (start 0.4 8.61) (end 0.4 9.17)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b6f8d6b5-4c5b-4dc0-b1ac-3b375611dccc))
    (fp_line (start 0.4 11.15) (end 0.4 11.71)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c19ccf8-350d-42bb-ab79-2e5327027262))
    (fp_line (start 0.4 13.69) (end 0.4 14.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fbfe648c-ed83-4438-94e5-f0c09fce58b2))
    (fp_line (start 0.4 16.23) (end 0.4 16.79)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 75f5023a-d09c-4d53-8896-978a73f8c3b6))
    (fp_line (start 0.4 18.77) (end 0.4 19.891)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 28029052-7ee9-4289-818c-91ee6e63408e))
    (fp_line (start 0.4 19.891) (end 7.221 19.891)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 60bf1a92-16ce-4f6d-8cc7-7ab9f1eebd45))
    (fp_line (start 2 -0.635) (end 2 0.635)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp acc5e114-1b74-4fce-8d35-d4ee49ee9d5d))
    (fp_line (start 2 -0.515) (end 3.206667 -0.515)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec9d38f3-63d5-4e96-9888-4d36059694ad))
    (fp_line (start 2 -0.395) (end 3.206667 -0.395)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba5a8ac5-a477-48f4-a23f-faee29d4d555))
    (fp_line (start 2 -0.275) (end 3.206667 -0.275)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ea80804-46ca-46c8-8764-c3895b64c646))
    (fp_line (start 2 -0.155) (end 3.206667 -0.155)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d5b0ed2-297f-4db2-bdff-34386c915af0))
    (fp_line (start 2 -0.035) (end 3.206667 -0.035)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2979e2b-f37c-412f-8540-092279ba2cf2))
    (fp_line (start 2 0.085) (end 3.206667 0.085)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ed4ddf6e-1dff-4a73-aebb-3fc14b8fca0a))
    (fp_line (start 2 0.205) (end 3.206667 0.205)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 71924fc4-4cee-49fe-a0a1-4eb1494de6bf))
    (fp_line (start 2 0.325) (end 3.206667 0.325)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 985ef665-d4da-4762-beac-452158ac8917))
    (fp_line (start 2 0.445) (end 3.206667 0.445)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c638c31-206a-41c8-857c-75f1cbfcc9b3))
    (fp_line (start 2 0.565) (end 3.206667 0.565)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6e90dd1e-e402-43d4-8e05-4d18a75515e6))
    (fp_line (start 2 0.635) (end 5.62 0.635)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e89edc94-7ac4-4c56-9db3-8a0386415295))
    (fp_line (start 2 1.905) (end 2 3.175)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 667f865d-ee54-4939-a778-4aa9b2e2e469))
    (fp_line (start 2 2.025) (end 3.206667 2.025)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 37c28472-ec77-42be-920e-948011f2650b))
    (fp_line (start 2 2.145) (end 3.206667 2.145)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c5c87511-6e0a-409e-b43c-b3cb7d53ce9f))
    (fp_line (start 2 2.265) (end 3.206667 2.265)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5badcbb5-c458-45bc-bed5-60866e9cda15))
    (fp_line (start 2 2.385) (end 3.206667 2.385)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3371b6cb-1321-4b4f-9ed0-0b6855262cb6))
    (fp_line (start 2 2.505) (end 3.206667 2.505)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 866042d7-6a2f-404e-a1ba-e0cafc7ed246))
    (fp_line (start 2 2.625) (end 3.206667 2.625)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cc9ec552-487b-4188-8394-2d16caee6f55))
    (fp_line (start 2 2.745) (end 3.206667 2.745)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1a12080f-b531-4ce1-85a8-f4dd4af983f8))
    (fp_line (start 2 2.865) (end 3.206667 2.865)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af491b00-1d8e-4d33-8a8c-61548c8fd484))
    (fp_line (start 2 2.985) (end 3.206667 2.985)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c2f47c5-56f9-4c49-880a-597bb0794124))
    (fp_line (start 2 3.105) (end 3.206667 3.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 461ca082-e6b8-44e9-a088-2f5b3cdb620c))
    (fp_line (start 2 3.175) (end 5.62 3.175)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cd00c54c-c03f-4137-9bb7-6d47493d3244))
    (fp_line (start 2 4.445) (end 2 5.715)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c41c7bd-3292-40c4-bedf-4eef2047164c))
    (fp_line (start 2 4.565) (end 3.206667 4.565)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 120890d7-01ea-4c15-928c-09b32c038bd3))
    (fp_line (start 2 4.685) (end 3.206667 4.685)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6d35c885-d375-4eb7-9f6b-e66518add6d5))
    (fp_line (start 2 4.805) (end 3.206667 4.805)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41e09a31-a912-41c5-9ddc-5b442d015232))
    (fp_line (start 2 4.925) (end 3.206667 4.925)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 75c3d48e-afb5-488a-bf57-bc86246271bb))
    (fp_line (start 2 5.045) (end 3.206667 5.045)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81a70fba-222c-4366-8d78-9c316a4c049d))
    (fp_line (start 2 5.165) (end 3.206667 5.165)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2320aac4-4fe2-470f-abcf-cddc724a1dab))
    (fp_line (start 2 5.285) (end 3.206667 5.285)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 853b6bf8-8414-4f3f-9481-aa2bed646b4e))
    (fp_line (start 2 5.405) (end 3.206667 5.405)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3cc5c945-9178-4e6a-9e1e-7a0598d051a7))
    (fp_line (start 2 5.525) (end 3.206667 5.525)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 801da751-8ed6-4da0-ac25-02ff4ce757f7))
    (fp_line (start 2 5.645) (end 3.206667 5.645)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 252cdfa2-bfd8-4393-a4c5-e0b374d24951))
    (fp_line (start 2 5.715) (end 5.62 5.715)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9e96975-0fb8-47a3-b40d-7a2d2d46ed16))
    (fp_line (start 2 6.985) (end 2 8.255)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3b747616-81f0-4cd5-bf7c-9249bf30e0e1))
    (fp_line (start 2 7.105) (end 3.206667 7.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fa36316d-0cad-4931-9e7f-26ca5d76b1ef))
    (fp_line (start 2 7.225) (end 3.206667 7.225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c48521a2-246b-49c3-86a3-11b8f5969cc7))
    (fp_line (start 2 7.345) (end 3.206667 7.345)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b93733a8-a7f6-49c1-9c15-ef0dc9ae4f59))
    (fp_line (start 2 7.465) (end 3.206667 7.465)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cc5fffbe-84b7-4460-985e-e84cc18a0d33))
    (fp_line (start 2 7.585) (end 3.206667 7.585)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 89057a34-f7fc-4671-9502-a73f7ef9f147))
    (fp_line (start 2 7.705) (end 3.206667 7.705)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0264ced7-4522-429a-be4f-bd7817de5341))
    (fp_line (start 2 7.825) (end 3.206667 7.825)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 98dc1e72-533d-4254-ae96-7b344227b58c))
    (fp_line (start 2 7.945) (end 3.206667 7.945)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 86b99337-c3c4-42f4-8938-a77b46e31c6c))
    (fp_line (start 2 8.065) (end 3.206667 8.065)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d054fa9-63aa-4248-b099-ba7e01130ee3))
    (fp_line (start 2 8.185) (end 3.206667 8.185)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f5f37cd1-a152-4f8a-895e-9fe6a27812db))
    (fp_line (start 2 8.255) (end 5.62 8.255)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 54a32512-7313-466b-a272-3476d1e16de9))
    (fp_line (start 2 9.525) (end 2 10.795)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0339ed5c-4edb-4d7d-9435-4c4ed29ee886))
    (fp_line (start 2 9.645) (end 3.206667 9.645)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 239811a0-56ec-41c8-9456-35a4f3165ae3))
    (fp_line (start 2 9.765) (end 3.206667 9.765)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ad4071a-5892-4a35-b7b9-c477deba0f80))
    (fp_line (start 2 9.885) (end 3.206667 9.885)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 27c5daed-e7df-4819-8789-e8ce28ca0128))
    (fp_line (start 2 10.005) (end 3.206667 10.005)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b123f8f2-cae1-46e4-9e3e-9d78bdf8b522))
    (fp_line (start 2 10.125) (end 3.206667 10.125)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a87fd859-39ac-4b3b-9188-13f81e4a2e66))
    (fp_line (start 2 10.245) (end 3.206667 10.245)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2597c4fd-e44b-4c50-a004-8a8f6e4fbbbc))
    (fp_line (start 2 10.365) (end 3.206667 10.365)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6313361-c6e6-407b-9fba-c981762f0c66))
    (fp_line (start 2 10.485) (end 3.206667 10.485)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51c6c615-aab2-456a-864a-66bc9f2c0b28))
    (fp_line (start 2 10.605) (end 3.206667 10.605)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 45584230-5261-4942-af34-f072ee1eefea))
    (fp_line (start 2 10.725) (end 3.206667 10.725)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9cef699-8ec3-410f-92b0-a94cbea8ee6f))
    (fp_line (start 2 10.795) (end 5.62 10.795)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b68416ce-d7f6-4fc5-86ae-37ea6867708f))
    (fp_line (start 2 12.065) (end 2 13.335)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 89f00324-2005-4fc0-b634-b0dfa6264e8a))
    (fp_line (start 2 12.185) (end 3.206667 12.185)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f91de886-a944-407a-95a4-71d9d2c2b092))
    (fp_line (start 2 12.305) (end 3.206667 12.305)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cbd6f02a-6db1-43ef-97f7-b7b443016385))
    (fp_line (start 2 12.425) (end 3.206667 12.425)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1b5cc240-c2bf-4465-98c0-1b75a820307d))
    (fp_line (start 2 12.545) (end 3.206667 12.545)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1252ae70-a49d-49a8-9bd5-073563d808df))
    (fp_line (start 2 12.665) (end 3.206667 12.665)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0316da75-8804-4ddc-8bea-00823f8fbdc4))
    (fp_line (start 2 12.785) (end 3.206667 12.785)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8120d96c-45f3-41d9-92d1-1f865e11937a))
    (fp_line (start 2 12.905) (end 3.206667 12.905)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 624871a7-14c2-4113-aefd-d1df7093a4f6))
    (fp_line (start 2 13.025) (end 3.206667 13.025)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d4731205-2667-4808-887d-1a803a141aa5))
    (fp_line (start 2 13.145) (end 3.206667 13.145)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d0486b90-dca8-4716-aba9-29a2f06be360))
    (fp_line (start 2 13.265) (end 3.206667 13.265)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 036df1be-95a0-44cc-9cdd-2c4190214d38))
    (fp_line (start 2 13.335) (end 5.62 13.335)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f98cea57-2b19-40a8-a3e2-6590e063468e))
    (fp_line (start 2 14.605) (end 2 15.875)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp edfead94-4588-4d27-b5ed-81c0d464068c))
    (fp_line (start 2 14.725) (end 3.206667 14.725)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1fa79404-b207-4f12-ad7e-6f69597ed076))
    (fp_line (start 2 14.845) (end 3.206667 14.845)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 253da89f-2201-4914-909c-4198b56fb5d4))
    (fp_line (start 2 14.965) (end 3.206667 14.965)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9049cc45-a9b5-4e68-a007-44726c84f723))
    (fp_line (start 2 15.085) (end 3.206667 15.085)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f436da7c-9b07-4392-b3d1-0823dfd9a734))
    (fp_line (start 2 15.205) (end 3.206667 15.205)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7259e282-f98b-4ea0-8b97-d5dc20e54789))
    (fp_line (start 2 15.325) (end 3.206667 15.325)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 616537ae-05d3-432b-9e69-7fd516d049c4))
    (fp_line (start 2 15.445) (end 3.206667 15.445)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f04d442-c0c8-4b11-9733-fb3d9205f30b))
    (fp_line (start 2 15.565) (end 3.206667 15.565)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 099f4d40-35f6-479d-bdb5-357e28eec08e))
    (fp_line (start 2 15.685) (end 3.206667 15.685)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 92acd0e1-72d2-4d5c-a190-d178d4d0adc6))
    (fp_line (start 2 15.805) (end 3.206667 15.805)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2b5b4d1b-36cd-4599-a012-1320168de9bd))
    (fp_line (start 2 15.875) (end 5.62 15.875)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6c34641-b702-42e5-bbac-b9da25fea794))
    (fp_line (start 2 17.145) (end 2 18.415)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fdaeb85c-d06e-4a65-96a2-f1f97397bb01))
    (fp_line (start 2 17.265) (end 3.206667 17.265)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6fd247d6-9f61-4509-ae90-ec2446a5bf68))
    (fp_line (start 2 17.385) (end 3.206667 17.385)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e40608a3-64b8-42e2-80f9-25b6807810ff))
    (fp_line (start 2 17.505) (end 3.206667 17.505)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7fe89a71-5821-42d3-9a0f-3b9771f15c11))
    (fp_line (start 2 17.625) (end 3.206667 17.625)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c0f7e91b-5ce0-49cc-9051-93e0da1bdc89))
    (fp_line (start 2 17.745) (end 3.206667 17.745)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 731ad29a-0c56-47bc-bc9f-794f8a44728c))
    (fp_line (start 2 17.865) (end 3.206667 17.865)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8cd923e0-e5f3-404e-b84a-65f49cf9d0af))
    (fp_line (start 2 17.985) (end 3.206667 17.985)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec17bcb8-32f3-4bed-ba48-a39d250c96fc))
    (fp_line (start 2 18.105) (end 3.206667 18.105)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b73ea623-8035-420a-81ec-98a8536a5ec5))
    (fp_line (start 2 18.225) (end 3.206667 18.225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 747fb3a5-e21b-4354-a0fb-6f5859d8f95b))
    (fp_line (start 2 18.345) (end 3.206667 18.345)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 87cc34db-91ba-4116-9a11-caa9b458c636))
    (fp_line (start 2 18.415) (end 5.62 18.415)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ab36dfa8-3314-4a5f-bae4-4429da518fe5))
    (fp_line (start 3.206667 -0.635) (end 3.206667 0.635)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f5d6685c-3ed8-41b0-a3cd-5a8fcf3a4c21))
    (fp_line (start 3.206667 1.905) (end 3.206667 3.175)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c0eb90d5-cdc4-4ae4-9f33-26ba7a87213a))
    (fp_line (start 3.206667 4.445) (end 3.206667 5.715)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 27faac9e-76ff-4b39-924c-a0507f481064))
    (fp_line (start 3.206667 6.985) (end 3.206667 8.255)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c6d54c56-7c12-4fcf-a0f5-66d09fe6a84b))
    (fp_line (start 3.206667 9.525) (end 3.206667 10.795)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fd2f1bc3-a2cd-4da0-9b6c-e4b8ca14661b))
    (fp_line (start 3.206667 12.065) (end 3.206667 13.335)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8abc6e49-fe4b-49e6-9ee6-b43a5f93cd82))
    (fp_line (start 3.206667 14.605) (end 3.206667 15.875)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 667c5fa4-9212-48de-a931-772ebbae19d1))
    (fp_line (start 3.206667 17.145) (end 3.206667 18.415)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0874e9e1-7aa2-4cd0-a864-0b7ba143d834))
    (fp_line (start 5.62 -0.635) (end 2 -0.635)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a6c17181-65fa-4d0f-8a7b-660499faec23))
    (fp_line (start 5.62 0.635) (end 5.62 -0.635)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7a892e82-3d5a-4aa4-8be2-a20c7da11577))
    (fp_line (start 5.62 1.905) (end 2 1.905)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a2f5a004-41ac-495e-9e32-b909e9b8c45e))
    (fp_line (start 5.62 3.175) (end 5.62 1.905)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e876bcbb-1512-4178-b13c-3804054c89bd))
    (fp_line (start 5.62 4.445) (end 2 4.445)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d0977ca2-0570-406d-ba00-297cf5ba3733))
    (fp_line (start 5.62 5.715) (end 5.62 4.445)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 556c57c3-7e38-4195-a1a2-2da561536c5b))
    (fp_line (start 5.62 6.985) (end 2 6.985)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 76a1576e-e21f-4c42-974e-0eae220d522d))
    (fp_line (start 5.62 8.255) (end 5.62 6.985)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7552bf95-2cc6-49b7-9f89-f8c30636fd93))
    (fp_line (start 5.62 9.525) (end 2 9.525)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 603bc33f-65b3-4574-bacb-b393f37feaf8))
    (fp_line (start 5.62 10.795) (end 5.62 9.525)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 328e8a45-3d0e-4b1c-b75c-f3482ca511f3))
    (fp_line (start 5.62 12.065) (end 2 12.065)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 973cf2a0-7b5c-4859-b2af-abb3daea75e7))
    (fp_line (start 5.62 13.335) (end 5.62 12.065)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 01effaee-4844-41ce-9fe1-754fea247967))
    (fp_line (start 5.62 14.605) (end 2 14.605)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb751d72-f3b8-4d70-9adf-da9bdbc9a356))
    (fp_line (start 5.62 15.875) (end 5.62 14.605)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 952dfcaf-6f1b-44a4-996a-bae2d2c8b13e))
    (fp_line (start 5.62 17.145) (end 2 17.145)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2eaf2cb3-ed94-40d4-8a3f-071d7dd36516))
    (fp_line (start 5.62 18.415) (end 5.62 17.145)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c0958c59-8997-4266-888b-ab9c545b6fc6))
    (fp_line (start 7.221 -2.11) (end 7.221 -0.99)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b34ed126-09ac-4cf0-96b8-ebadfc950f92))
    (fp_line (start 7.221 0.991) (end 7.221 1.551)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 14bbf696-831d-47f7-a839-1c1e18c328bc))
    (fp_line (start 7.221 3.531) (end 7.221 4.091)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 64a7de2e-b56e-44c6-9a06-2384cc37ab5a))
    (fp_line (start 7.221 6.071) (end 7.221 6.631)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12b69b11-65a8-41df-9a28-b4a1c3957c1a))
    (fp_line (start 7.221 8.611) (end 7.221 9.171)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f5a44118-5a97-4017-8aa6-ccea74ef6222))
    (fp_line (start 7.221 11.151) (end 7.221 11.711)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c5d5228-94a2-438f-ae21-7489afb4e723))
    (fp_line (start 7.221 13.691) (end 7.221 14.251)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f499913-84b3-44c1-bf7f-bfe158856fef))
    (fp_line (start 7.221 16.231) (end 7.221 16.79)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 67969465-a002-49ca-b8a2-246c2d979c02))
    (fp_line (start 7.221 18.771) (end 7.221 19.891)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a203270c-59f2-4c69-92ad-381cbd4d9b3e))
    (fp_line (start -1.1 -2.4) (end -1.1 20.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 83f53f4f-34ed-4922-a162-2b6ac028f958))
    (fp_line (start -1.1 20.15) (end 8.7 20.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 84546109-84c4-41ec-83ec-21c5a404cb63))
    (fp_line (start 8.7 -2.4) (end -1.1 -2.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 59aab24e-ee9e-46e9-bf36-2ab9a694a84d))
    (fp_line (start 8.7 20.15) (end 8.7 -2.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 08531fd2-ec85-4649-b109-f399fae72e40))
    (fp_line (start 0.46 -1.05) (end 1.46 -2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a180cafe-a8e8-4f67-91cb-bbceb960a53b))
    (fp_line (start 0.46 19.83) (end 0.46 -1.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1525914c-7ee8-4f38-9682-84328434ca40))
    (fp_line (start 1.46 -2.05) (end 7.16 -2.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82ee1839-c4d1-413f-88b0-db554dff249b))
    (fp_line (start 2 -0.635) (end 2 0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 34104614-532b-4b13-a963-ddf8f1d7eba0))
    (fp_line (start 2 -0.535) (end 3.206667 -0.535)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a4feff46-d633-4c14-b5d6-4758af52496e))
    (fp_line (start 2 -0.435) (end 3.206667 -0.435)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42417a22-0553-44cc-93f9-4215aae8b8c3))
    (fp_line (start 2 -0.335) (end 3.206667 -0.335)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86f8583b-70ef-491a-947d-00fc8d65ca62))
    (fp_line (start 2 -0.235) (end 3.206667 -0.235)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e99b5f1-b70a-4b61-aebe-ddbd094169dc))
    (fp_line (start 2 -0.135) (end 3.206667 -0.135)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 61a6dfd5-82f5-43ef-a8ab-a4dfaa5afa66))
    (fp_line (start 2 -0.035) (end 3.206667 -0.035)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc9f49b3-65c6-4249-9911-9c7a49a30752))
    (fp_line (start 2 0.065) (end 3.206667 0.065)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fdbe4356-179b-4095-aaa8-27e1bad23eb4))
    (fp_line (start 2 0.165) (end 3.206667 0.165)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2044a221-78c5-4caf-8914-d14be9171fac))
    (fp_line (start 2 0.265) (end 3.206667 0.265)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0af16c2c-ef11-4cf3-b524-acdeb822011f))
    (fp_line (start 2 0.365) (end 3.206667 0.365)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9d60c53-4ead-4d83-861b-d38ecadeffb7))
    (fp_line (start 2 0.465) (end 3.206667 0.465)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp edbb0eb9-e324-47b7-8c73-d75b3f0ffe12))
    (fp_line (start 2 0.565) (end 3.206667 0.565)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1fc3e111-a5f0-4ce4-8c3b-7d9efa3fde86))
    (fp_line (start 2 0.635) (end 5.62 0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8155dc5e-13cf-4fdb-a4db-14be2750b75e))
    (fp_line (start 2 1.905) (end 2 3.175)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5793d900-3ae6-4a8a-af17-40edde7a6309))
    (fp_line (start 2 2.005) (end 3.206667 2.005)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e6ca02f7-9600-4f89-b9a0-c0a3d41ae1da))
    (fp_line (start 2 2.105) (end 3.206667 2.105)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp de7886c2-cd7a-46f4-a0df-bef92d56fd42))
    (fp_line (start 2 2.205) (end 3.206667 2.205)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1bfcbcbe-0180-4727-bba4-e1b1d7b8bf35))
    (fp_line (start 2 2.305) (end 3.206667 2.305)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a12b4b1d-794f-43bb-ae1b-8e380c684cbf))
    (fp_line (start 2 2.405) (end 3.206667 2.405)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b013080-9bbc-41ec-86fb-8f20c9be5bd5))
    (fp_line (start 2 2.505) (end 3.206667 2.505)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a3ddb487-498b-41e9-9174-62286829ceb0))
    (fp_line (start 2 2.605) (end 3.206667 2.605)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e226c592-1000-4872-948a-ad61e5da1b22))
    (fp_line (start 2 2.705) (end 3.206667 2.705)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e6a6d684-295c-4874-9689-7faa4a7c5775))
    (fp_line (start 2 2.805) (end 3.206667 2.805)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 53ea5452-7b54-493a-a9fe-0efd829e948d))
    (fp_line (start 2 2.905) (end 3.206667 2.905)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ff06a5e7-7e1a-4aef-8e3a-18d96ae55152))
    (fp_line (start 2 3.005) (end 3.206667 3.005)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 46bb34c6-edda-4f7d-9887-fb4bccd5b5a5))
    (fp_line (start 2 3.105) (end 3.206667 3.105)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 34495eb8-a0f6-4f6b-99d4-9ee9c1c2db41))
    (fp_line (start 2 3.175) (end 5.62 3.175)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3089496-c925-48a8-8f5f-e8f731219515))
    (fp_line (start 2 4.445) (end 2 5.715)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e7eeef70-7106-4e76-860c-4f09843d2507))
    (fp_line (start 2 4.545) (end 3.206667 4.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 155c4da8-22f6-4ed8-802e-9c13a571a974))
    (fp_line (start 2 4.645) (end 3.206667 4.645)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e0448705-b19b-43d2-a93d-dd9cd02c94c0))
    (fp_line (start 2 4.745) (end 3.206667 4.745)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cf4da12f-a4eb-4e15-8d49-648470cd2b4f))
    (fp_line (start 2 4.845) (end 3.206667 4.845)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aeb34c75-de04-4076-9b66-ca3d4c99e907))
    (fp_line (start 2 4.945) (end 3.206667 4.945)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c2358c6-c1db-4694-969e-2f19ecd7d4bc))
    (fp_line (start 2 5.045) (end 3.206667 5.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06237fe7-3d5f-4e22-a357-d163525962b5))
    (fp_line (start 2 5.145) (end 3.206667 5.145)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d4c01b4-51ac-43a8-94c5-f4c03b768373))
    (fp_line (start 2 5.245) (end 3.206667 5.245)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 920f0cc7-3e43-4556-b361-14a55729cda5))
    (fp_line (start 2 5.345) (end 3.206667 5.345)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f273183d-5a77-4c21-8056-8a87aea40664))
    (fp_line (start 2 5.445) (end 3.206667 5.445)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2bfd8ae4-a9d7-4004-88c4-b7f73f92cc2e))
    (fp_line (start 2 5.545) (end 3.206667 5.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9711b66e-bbbb-46a9-944f-5d518477b38b))
    (fp_line (start 2 5.645) (end 3.206667 5.645)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49b727b3-dcec-4893-9a8d-6f658fd2ca88))
    (fp_line (start 2 5.715) (end 5.62 5.715)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cdc0e21b-818b-4379-8da1-e19c1f01ea00))
    (fp_line (start 2 6.985) (end 2 8.255)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8150e26e-2195-4f15-9c9a-81b874c68fc7))
    (fp_line (start 2 7.085) (end 3.206667 7.085)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 53c8613e-e22d-46db-a120-65fd9728f2d4))
    (fp_line (start 2 7.185) (end 3.206667 7.185)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 242b19ad-8c76-4825-b01f-d7a8d091dd40))
    (fp_line (start 2 7.285) (end 3.206667 7.285)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d90d020d-65aa-4f9e-aac1-99bf3814fe00))
    (fp_line (start 2 7.385) (end 3.206667 7.385)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 800e68fc-30a1-4b6c-af13-33ec047035bc))
    (fp_line (start 2 7.485) (end 3.206667 7.485)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4810421f-529b-449e-a40c-380278e74921))
    (fp_line (start 2 7.585) (end 3.206667 7.585)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64e9de0f-c6f0-426c-b68a-b1938d2c0e8d))
    (fp_line (start 2 7.685) (end 3.206667 7.685)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8dae8eb-10ea-43f5-9ce4-ae5d44b033f3))
    (fp_line (start 2 7.785) (end 3.206667 7.785)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 88eb02de-d827-409a-b037-95e363e333cc))
    (fp_line (start 2 7.885) (end 3.206667 7.885)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 587cc7dd-8070-4171-8a93-67a35ab9372a))
    (fp_line (start 2 7.985) (end 3.206667 7.985)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cf04cc34-2d25-4c89-97b3-9f90c8551382))
    (fp_line (start 2 8.085) (end 3.206667 8.085)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 36c660db-9c99-4182-879c-d5d0252509fd))
    (fp_line (start 2 8.185) (end 3.206667 8.185)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb920632-ff1f-491f-bb47-34ec32fc9d92))
    (fp_line (start 2 8.255) (end 5.62 8.255)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1b4eb226-1b5e-4b6c-a067-2b4cb87c6919))
    (fp_line (start 2 9.525) (end 2 10.795)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aee08859-a90f-4d3f-93da-ac5d636cf5d2))
    (fp_line (start 2 9.625) (end 3.206667 9.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 61839a82-0958-464d-8456-9c4aad7d98ed))
    (fp_line (start 2 9.725) (end 3.206667 9.725)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48aa3565-a8e7-403d-989f-0f54ba8faebf))
    (fp_line (start 2 9.825) (end 3.206667 9.825)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 05f2387e-9b53-4de3-8ffa-cd420a702246))
    (fp_line (start 2 9.925) (end 3.206667 9.925)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 83bb273c-324c-48bd-b937-d74347341af8))
    (fp_line (start 2 10.025) (end 3.206667 10.025)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc1d16de-9cdc-4772-bb39-e19ba374c6e0))
    (fp_line (start 2 10.125) (end 3.206667 10.125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 36d45cc1-ee60-41da-a5bd-c18bb85e38b9))
    (fp_line (start 2 10.225) (end 3.206667 10.225)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 350d7e2b-9f15-4007-ad86-0c2b881043db))
    (fp_line (start 2 10.325) (end 3.206667 10.325)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b68fde5a-2c69-4343-9bc2-faf0bb9beaf9))
    (fp_line (start 2 10.425) (end 3.206667 10.425)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41eaaa88-c9b0-49bb-a9d1-71ac7e226140))
    (fp_line (start 2 10.525) (end 3.206667 10.525)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9cfd04cd-b207-4745-940e-d997e2de6ecd))
    (fp_line (start 2 10.625) (end 3.206667 10.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6bf446a2-f600-4e2c-bd2e-114a04b78ce7))
    (fp_line (start 2 10.725) (end 3.206667 10.725)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09280ad0-3ea5-49de-a37f-fb06beb00d7b))
    (fp_line (start 2 10.795) (end 5.62 10.795)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e7ae218-0aeb-4e27-bf3c-dc3c64f69dbe))
    (fp_line (start 2 12.065) (end 2 13.335)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2ab8a5f-d293-460a-8a64-6872dd30ac75))
    (fp_line (start 2 12.165) (end 3.206667 12.165)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 34a657f7-c4e4-4924-991e-d0da90ab7615))
    (fp_line (start 2 12.265) (end 3.206667 12.265)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 259a328f-b213-4043-8d50-35eb7d802348))
    (fp_line (start 2 12.365) (end 3.206667 12.365)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 48d2783f-54ba-42de-8fca-1b0cf2e1989e))
    (fp_line (start 2 12.465) (end 3.206667 12.465)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6536af01-35cd-4518-b72b-ad825af4b4c8))
    (fp_line (start 2 12.565) (end 3.206667 12.565)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d86dcc0-f088-4c3b-91bb-7eae03d5e0cc))
    (fp_line (start 2 12.665) (end 3.206667 12.665)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ccee181-eb57-450c-9248-bb0e6e2f0dc6))
    (fp_line (start 2 12.765) (end 3.206667 12.765)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ff38453-d678-4ba0-8024-2401cdb78762))
    (fp_line (start 2 12.865) (end 3.206667 12.865)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37da7ff5-4e36-4357-b8e5-9a4a00298c19))
    (fp_line (start 2 12.965) (end 3.206667 12.965)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e8e04503-2eef-4b16-a7e1-da97b5100a92))
    (fp_line (start 2 13.065) (end 3.206667 13.065)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 35f955b0-fea2-4943-ba09-e88fc0393eea))
    (fp_line (start 2 13.165) (end 3.206667 13.165)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c8441c8-191d-4cba-9241-a76aeb1ca3ce))
    (fp_line (start 2 13.265) (end 3.206667 13.265)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d4d7729-6bd0-43b9-aa4d-4a1c28e069ba))
    (fp_line (start 2 13.335) (end 5.62 13.335)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 54572930-6ffb-4b08-93f7-ed3c5d56ac19))
    (fp_line (start 2 14.605) (end 2 15.875)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 45abf33e-8808-42e4-8d94-70853c5b4b7f))
    (fp_line (start 2 14.705) (end 3.206667 14.705)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 87545dfd-65d8-40f4-97f5-295dac1c5736))
    (fp_line (start 2 14.805) (end 3.206667 14.805)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e9b78fc-dff6-43a3-a93d-c8ec5a4d3e4f))
    (fp_line (start 2 14.905) (end 3.206667 14.905)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c17cedaf-6d60-4f46-9391-71235c514a0b))
    (fp_line (start 2 15.005) (end 3.206667 15.005)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a47fb3bf-b0ed-4762-9576-7204e6c59ea4))
    (fp_line (start 2 15.105) (end 3.206667 15.105)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3488cdbd-9271-4775-bac1-35fba3535bed))
    (fp_line (start 2 15.205) (end 3.206667 15.205)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee43f5e0-0a03-4730-bfcc-dad8e9f0443f))
    (fp_line (start 2 15.305) (end 3.206667 15.305)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9770f50-8e07-474b-a39c-0bb82a289423))
    (fp_line (start 2 15.405) (end 3.206667 15.405)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 259f671f-3581-4f28-bb64-f9b4791530e1))
    (fp_line (start 2 15.505) (end 3.206667 15.505)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 88c1bb36-c0fb-407a-87dc-b393ca3cde7c))
    (fp_line (start 2 15.605) (end 3.206667 15.605)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2cec4acf-e8aa-4de2-8a29-11df5ad86bc2))
    (fp_line (start 2 15.705) (end 3.206667 15.705)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1813d6e-4dd2-46e2-8eef-0a6877129d08))
    (fp_line (start 2 15.805) (end 3.206667 15.805)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp be94123f-028e-4e03-b038-a452a22905f8))
    (fp_line (start 2 15.875) (end 5.62 15.875)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1d474990-4b2c-4d3e-86db-0b8b2f32dbcf))
    (fp_line (start 2 17.145) (end 2 18.415)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8bfddfe3-2818-4661-bce2-f3d2e134ba76))
    (fp_line (start 2 17.245) (end 3.206667 17.245)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc3eddee-33a7-4c55-add4-bff3df8fce48))
    (fp_line (start 2 17.345) (end 3.206667 17.345)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 70fd046d-ebb9-4b1d-abd8-217608cf7850))
    (fp_line (start 2 17.445) (end 3.206667 17.445)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1fdc494f-5e65-4a8f-bc44-bfdf8037d6f2))
    (fp_line (start 2 17.545) (end 3.206667 17.545)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 682df302-8caa-4f49-be8f-5f384417bd6e))
    (fp_line (start 2 17.645) (end 3.206667 17.645)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4cdcfd9d-7053-452b-837a-993636c71ca7))
    (fp_line (start 2 17.745) (end 3.206667 17.745)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f30a93d9-3e3c-4272-93a5-1b3ad12316ac))
    (fp_line (start 2 17.845) (end 3.206667 17.845)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 16924f32-0e56-4af0-9172-d2ee5aa6e1f5))
    (fp_line (start 2 17.945) (end 3.206667 17.945)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 96745936-9836-47f9-a2ed-112f017f801d))
    (fp_line (start 2 18.045) (end 3.206667 18.045)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e47f3304-8ee0-4c5e-906d-761bba91e87b))
    (fp_line (start 2 18.145) (end 3.206667 18.145)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b3acb77-caea-44cf-8825-432ea02ec677))
    (fp_line (start 2 18.245) (end 3.206667 18.245)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b628948-1298-4a6b-b47f-7177a9b3cc89))
    (fp_line (start 2 18.345) (end 3.206667 18.345)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc23c8b8-2b79-4e43-98cd-17524a4f03bb))
    (fp_line (start 2 18.415) (end 5.62 18.415)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fd58d717-5a24-45c1-b2e7-af332f41af7d))
    (fp_line (start 3.206667 -0.635) (end 3.206667 0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0fa9be68-df80-4161-aa03-15580ab673ab))
    (fp_line (start 3.206667 1.905) (end 3.206667 3.175)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2c3b10bf-a119-43a1-8287-2eb94b711e11))
    (fp_line (start 3.206667 4.445) (end 3.206667 5.715)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d9edbcdb-e51d-4b78-abce-d85980bc7fe4))
    (fp_line (start 3.206667 6.985) (end 3.206667 8.255)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp acb378a1-e411-4bb6-b3d4-d22d21b861b4))
    (fp_line (start 3.206667 9.525) (end 3.206667 10.795)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 912ffe05-a5a4-46a1-afa4-23605b95afd0))
    (fp_line (start 3.206667 12.065) (end 3.206667 13.335)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c6a2047-afad-42bd-b3f9-68defbcaaa3e))
    (fp_line (start 3.206667 14.605) (end 3.206667 15.875)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d000e95-1932-44f6-b421-cb7fd0e9ee0b))
    (fp_line (start 3.206667 17.145) (end 3.206667 18.415)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1787e78e-286a-4805-a648-c309088022a5))
    (fp_line (start 5.62 -0.635) (end 2 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf65651a-ff4e-425e-af5a-3dd4694b1acb))
    (fp_line (start 5.62 0.635) (end 5.62 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69292fe3-7aee-4537-a84d-8183f3f7b205))
    (fp_line (start 5.62 1.905) (end 2 1.905)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77449b42-03d2-4b67-838d-2eb6b4682c77))
    (fp_line (start 5.62 3.175) (end 5.62 1.905)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fccb652-bb1d-48c7-94b7-aed09470b8bf))
    (fp_line (start 5.62 4.445) (end 2 4.445)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8cbecfad-b340-40f8-ac32-eea1bb493eaa))
    (fp_line (start 5.62 5.715) (end 5.62 4.445)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 39d45570-7e1b-48aa-8c18-72da648357f9))
    (fp_line (start 5.62 6.985) (end 2 6.985)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d037d642-b70f-463a-bade-2cd408f11688))
    (fp_line (start 5.62 8.255) (end 5.62 6.985)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 239ff98e-3d6c-4b67-830d-b2b6a0ab1074))
    (fp_line (start 5.62 9.525) (end 2 9.525)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1049971f-9f2a-4e43-97fb-c82cff40dd59))
    (fp_line (start 5.62 10.795) (end 5.62 9.525)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 495381f5-22eb-48aa-adda-c1dc76bd634b))
    (fp_line (start 5.62 12.065) (end 2 12.065)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b0846369-6752-4f10-a4ba-0f8781343229))
    (fp_line (start 5.62 13.335) (end 5.62 12.065)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8b18b96-4163-42b6-939e-cd5fb676436a))
    (fp_line (start 5.62 14.605) (end 2 14.605)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fbcbe3f5-6c2d-491d-bf4e-15e1f1e5ed57))
    (fp_line (start 5.62 15.875) (end 5.62 14.605)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ea43ac3-01d8-4048-9021-a2d0c6921fbb))
    (fp_line (start 5.62 17.145) (end 2 17.145)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb627a16-8b12-40be-9e27-e88adc8404ae))
    (fp_line (start 5.62 18.415) (end 5.62 17.145)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9845d632-82e9-4e13-895c-a2d171417ed0))
    (fp_line (start 7.16 -2.05) (end 7.16 19.83)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b66a223e-3d5f-48bc-946e-3258af37a5af))
    (fp_line (start 7.16 19.83) (end 0.46 19.83)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 53c06116-5efc-4aa9-8e1c-9a3c62ab71c1))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 108 "unconnected-(SW1-Pad1)") (pintype "passive") (tstamp 1ea2c485-5e4d-4902-a61a-82864c2b67fa))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 109 "unconnected-(SW1-Pad2)") (pintype "passive") (tstamp 371a390d-b225-457d-bf24-0b5190acae9a))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 110 "unconnected-(SW1-Pad3)") (pintype "passive") (tstamp 402d8985-eac1-42d9-ba0a-832dad2d7d88))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(SW1-Pad4)") (pintype "passive") (tstamp 88f13405-8034-48f7-a4ee-4d0ef095f1a5))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 112 "unconnected-(SW1-Pad5)") (pintype "passive") (tstamp 3669ab3f-887b-4a7d-ab9c-717ac9588783))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "unconnected-(SW1-Pad6)") (pintype "passive") (tstamp 2036aa1b-ffa6-416d-8595-27b5f2a1b5c4))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 114 "unconnected-(SW1-Pad7)") (pintype "passive") (tstamp bb1cfa5f-991d-4c56-8b06-f605e71e4213))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "unconnected-(SW1-Pad8)") (pintype "passive") (tstamp 53725ea9-564b-47f4-b0cb-b3bf746854c2))
    (pad "9" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 116 "unconnected-(SW1-Pad9)") (pintype "passive") (tstamp 80691a6e-7bd2-4b8e-a434-bdb04bdf3c72))
    (pad "10" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 117 "unconnected-(SW1-Pad10)") (pintype "passive") (tstamp 18a0305d-b887-4a72-b6a0-efd098a7771e))
    (pad "11" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 118 "unconnected-(SW1-Pad11)") (pintype "passive") (tstamp c18fb0e7-00b7-424d-bdf5-8db38c2d1f40))
    (pad "12" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 119 "unconnected-(SW1-Pad12)") (pintype "passive") (tstamp f2f0075a-0de6-414c-b72e-d10b2f22819f))
    (pad "13" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 120 "unconnected-(SW1-Pad13)") (pintype "passive") (tstamp 98aa4067-7c07-4223-a093-c30b66e30f4b))
    (pad "14" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 121 "unconnected-(SW1-Pad14)") (pintype "passive") (tstamp 3fab1712-4322-4aac-ba68-33c5db9da94c))
    (pad "15" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 122 "unconnected-(SW1-Pad15)") (pintype "passive") (tstamp 61e1c39e-fccd-485c-b96d-cba259dcd018))
    (pad "16" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(SW1-Pad16)") (pintype "passive") (tstamp 36adf77e-fbd1-44d1-abd0-b2d2c5ea7fda))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx08_Slide_6.7x21.88mm_W7.62mm_P2.54mm_LowProfile.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tstamp 9bcb1e68-903b-41a0-a5c2-316bae6b36a8)
    (at 163.5625 31.4)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "power")
    (path "/03abecec-4724-420e-920e-986ba2580308/8d318114-19a0-44bf-8b55-0b8ed0e64490")
    (attr smd)
    (fp_text reference "U4" (at 0 -3.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6811e54e-9195-4ea9-9914-e920b3bd0750)
    )
    (fp_text value "~" (at 0 3.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ebf99a8f-3a1f-4cfb-b2e3-298ead254ec2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp 44b91dd6-1ee2-4070-a667-5b0b8d9629b3)
    )
    (fp_line (start 0 -2.56) (end -3.45 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 528ed4b6-828e-4157-9d42-73975e5ece66))
    (fp_line (start 0 -2.56) (end 1.95 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ae5a426d-edf1-455c-a73a-1d21c079b1ee))
    (fp_line (start 0 2.56) (end -1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dc60ecb7-a00a-43da-8c49-2530a519edd9))
    (fp_line (start 0 2.56) (end 1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 32ff6523-a01e-4b7c-a563-c6a1ec637f0d))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b476311c-6269-46a8-bac6-d6f0d2fcce7f))
    (fp_line (start -3.7 2.7) (end 3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 20e2ca8a-6d55-4dd3-8086-5bc44815010e))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 53c89162-a9fe-4a09-b813-4485936dfb43))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bfc41944-8576-4e27-8ffc-65f1a9aa711a))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25838514-8fb4-4147-8115-ba650a4d63ca))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 46b348c7-e8e4-4f28-a6bf-610dd9152ccb))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09078681-cda4-49da-aa5f-1676a1b48fea))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d60a1a96-bd06-4571-a4e6-209b654a50fc))
    (fp_line (start 1.95 2.45) (end -1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1efef975-25a6-4a4d-be2d-a872ca6e2b56))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 544 "unconnected-(U4-SW-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp b538ebd6-e3e1-4fe8-b546-8c425da966af))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 545 "unconnected-(U4-PGND-Pad2)") (pinfunction "PGND") (pintype "passive") (tstamp a768fa0a-b5a8-45a1-8412-63bce4d44fc7))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 546 "unconnected-(U4-VINA-Pad3)") (pinfunction "VINA") (pintype "power_in") (tstamp c6aa0160-6fcf-48c6-a48b-021622f8fc94))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 547 "unconnected-(U4-EN-Pad4)") (pinfunction "EN") (pintype "input") (tstamp 2abcea91-01f6-489e-8da3-a991c36046fb))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 548 "unconnected-(U4-FB-Pad5)") (pinfunction "FB") (pintype "input") (tstamp 4c1a95c4-4e47-44f4-b483-6d6321db7722))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 549 "unconnected-(U4-AGND-Pad6)") (pinfunction "AGND") (pintype "passive") (tstamp e07914d5-d7a4-4a34-bea7-c76f44c77c05))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 550 "unconnected-(U4-GND-Pad7)") (pinfunction "GND") (pintype "passive") (tstamp 02c44ca9-797f-4cc7-9d0a-3e9998cb1390))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 551 "unconnected-(U4-VINSW-Pad8)") (pinfunction "VINSW") (pintype "power_in") (tstamp 171fcca1-c6b2-4f25-ae50-1869d96745cd))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Display_7Segment:LTS-4802B" (layer "F.Cu")
    (tstamp 9d88e9d4-152e-424f-ac33-25e0abc88963)
    (at 51.5 90.34)
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/986d55df-5cbd-4b55-90d5-bdcef9364103")
    (attr through_hole)
    (fp_text reference "U11" (at 0 -2.54 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 36e2d072-dd90-4da4-bef1-21a10bc97fbe)
    )
    (fp_text value "~" (at 3.58 13.1 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81d9a69b-47d5-43e0-8939-c0787c24e5ba)
    )
    (fp_text user "${REFERENCE}" (at 3.58 4.01 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 611b12bf-9479-4213-9bcd-068f014c1159)
    )
    (fp_rect (start -1.04 -1.07) (end 8.66 11.83)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp a09504f0-7e87-414b-ab0e-f8bd98ebc28a))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 741 "unconnected-(U11-CA-Pad1)") (pinfunction "CA") (pintype "passive") (tstamp 157b6876-fde7-495c-9dd2-a87c4cdf3176))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 742 "unconnected-(U11-F-Pad2)") (pinfunction "F") (pintype "passive") (tstamp ef9004e8-b170-4312-8367-aa4045fcb648))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 743 "unconnected-(U11-G-Pad3)") (pinfunction "G") (pintype "passive") (tstamp 96060c66-bdb5-499d-bcbc-fd5d2a292b91))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 744 "unconnected-(U11-E-Pad4)") (pinfunction "E") (pintype "passive") (tstamp d1d44f4c-dc43-4377-95d9-f0b82c4b6f66))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 745 "unconnected-(U11-D-Pad5)") (pinfunction "D") (pintype "passive") (tstamp 47efd3b0-fc42-4de2-a83b-5f056c31fefc))
    (pad "6" thru_hole circle (at 7.62 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 746 "unconnected-(U11-CA-Pad6)") (pinfunction "CA") (pintype "passive") (tstamp 3eab6248-0b16-47c1-8d5f-0af4aff29170))
    (pad "7" thru_hole circle (at 7.62 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 747 "unconnected-(U11-DP-Pad7)") (pinfunction "DP") (pintype "passive") (tstamp 2fa017f8-9cde-4324-90e4-7bd5e9a6f5c8))
    (pad "8" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 748 "unconnected-(U11-C-Pad8)") (pinfunction "C") (pintype "passive") (tstamp ddc088d0-66e4-46bb-85fd-ae87a88b6850))
    (pad "9" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 749 "unconnected-(U11-B-Pad9)") (pinfunction "B") (pintype "passive") (tstamp 32eea67e-99b0-4893-82de-d8076514a47c))
    (pad "10" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 750 "unconnected-(U11-A-Pad10)") (pinfunction "A") (pintype "passive") (tstamp a3379fa2-e981-4ccd-948f-8de30cedca81))
    (model ":KICAD7_3DMODEL_DIR:Display_7Segment.3dshapes/LTS-4802BJR-H1_LTO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_USB:GCT_USB4085-GF-A_REVB" (layer "F.Cu")
    (tstamp 9dd458c1-ff4e-41e3-b88f-4d3852143cfb)
    (at 174 62.925 90)
    (property "MANUFACTURER" "Global Connector Technology")
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.16mm")
    (property "PARTREV" "B")
    (property "SNAPEDA_PN" "USB4085-GF-A")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "ftdi.kicad_sch")
    (property "Sheetname" "ftdi")
    (path "/95d69960-5749-4bf0-ba13-8cc427d1e8e9/1f89b073-ac2e-4f3c-9ffd-18724cb2794c")
    (attr through_hole)
    (fp_text reference "J4" (at -1.85 -8.555 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 936ce48e-eea4-4d3d-9401-ea4e2cb4691e)
    )
    (fp_text value "USB4085-GF-A_REVB" (at 8.31 -6.95 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 43d7a045-becc-4a9b-8900-303c939f3a5e)
    )
    (fp_text user "PCB EDGE" (at 5.315 1.57 90) (layer "F.Fab")
        (effects (font (size 0.64 0.64) (thickness 0.15)))
      (tstamp 8c9f62be-493d-42fa-8947-bb0913d07be0)
    )
    (fp_line (start -4.47 -1.85) (end -4.47 -1.17)
      (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp f042ec44-766d-48af-be53-60f9a32d2534))
    (fp_line (start -4.47 1.39) (end -4.47 1.74)
      (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 7441d56a-8ba1-4637-b996-20a2af59c6d1))
    (fp_line (start -4.47 1.74) (end 4.47 1.74)
      (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 17e5c196-b989-4c79-84e0-7f52edca2770))
    (fp_line (start 4.47 -1.85) (end 4.47 -1.17)
      (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp b85c88f7-9709-4f74-981c-c99442ed21f5))
    (fp_line (start 4.47 1.74) (end 4.47 1.39)
      (stroke (width 0.2) (type solid)) (layer "F.SilkS") (tstamp 532cfe5e-a332-40fb-969d-0a8d7ebd074a))
    (fp_circle (center -2.975 -5.7) (end -2.875 -5.7)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.SilkS") (tstamp 293f4edd-3cb3-4e18-a583-1d2ee7941482))
    (fp_line (start -5.025 -5.17) (end 5.025 -5.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d83916ff-f87b-43cf-ad4e-dd76f6b3e510))
    (fp_line (start -5.025 4.5) (end -5.025 -5.17)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5dbfb691-cee5-49c2-93d0-911f7181214c))
    (fp_line (start 5.025 -5.17) (end 5.025 4.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0bce2df8-ecf4-40f7-b6f7-5785ecc5d057))
    (fp_line (start 5.025 4.5) (end -5.025 4.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 316f8b1a-b5b2-4436-9285-d3a23d02927e))
    (fp_line (start -4.47 -4.92) (end 4.47 -4.92)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1be8b451-cb2c-4b0d-844b-59f6d3d7004f))
    (fp_line (start -4.47 1.74) (end -4.47 -4.92)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b9f3dc9b-45f5-4c54-9b2b-621e5ef81326))
    (fp_line (start -4.47 1.74) (end 10.5 1.74)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d11f607-715b-4cb8-8b43-2e18dd699644))
    (fp_line (start -4.47 4.25) (end -4.47 1.74)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f0c0c97-4030-4dce-a322-09c3a7775475))
    (fp_line (start 4.47 -4.92) (end 4.47 4.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp afa35021-681e-417e-92b6-58cc5b08d8ee))
    (fp_line (start 4.47 4.25) (end -4.47 4.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 441c74b7-50a1-4c4a-9cdb-c5df66681dee))
    (fp_circle (center -2.975 -5.7) (end -2.875 -5.7)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.Fab") (tstamp c04098ca-42e7-496c-bfb2-9713908e2644))
    (pad "A1" thru_hole circle (at -2.975 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 70 "unconnected-(J4-GND-PadA1)") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102) (tstamp ea91d23a-5255-4abd-bc21-a3783214cce9))
    (pad "A4" thru_hole circle (at -2.125 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(J4-VBUS-PadA4)") (pinfunction "VBUS") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 25cde0b2-e712-4e52-8710-e8c6b546e2e8))
    (pad "A5" thru_hole circle (at -1.275 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(J4-CC1-PadA5)") (pinfunction "CC1") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 1fcfbedf-35de-4476-90e4-7075fccd4f21))
    (pad "A6" thru_hole circle (at -0.425 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 73 "unconnected-(J4-DP1-PadA6)") (pinfunction "DP1") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp b0753ba0-7d5d-44f4-aa5e-3ca6a49495ac))
    (pad "A7" thru_hole circle (at 0.425 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 74 "unconnected-(J4-DN1-PadA7)") (pinfunction "DN1") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 0b81727f-83b3-49e0-92b0-8a6f8fcc35a6))
    (pad "A8" thru_hole circle (at 1.275 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 75 "unconnected-(J4-SBU1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 8df28bf4-41d3-4896-b54d-1e663463da5d))
    (pad "A9" thru_hole circle (at 2.125 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 76 "unconnected-(J4-VBUS__1-PadA9)") (pinfunction "VBUS__1") (pintype "power_in") (solder_mask_margin 0.102) (tstamp c0fcf79e-99cd-4694-8d7f-962aef5da40d))
    (pad "A12" thru_hole circle (at 2.975 -4.36 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 77 "unconnected-(J4-GND__1-PadA12)") (pinfunction "GND__1") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 238d02d2-0274-47c4-afeb-25c8fa29ff5c))
    (pad "B1" thru_hole circle (at 2.975 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 78 "unconnected-(J4-GND__2-PadB1)") (pinfunction "GND__2") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 379236be-0bc2-4f6c-a63e-7460f56bcef6))
    (pad "B4" thru_hole circle (at 2.125 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 79 "unconnected-(J4-VBUS__2-PadB4)") (pinfunction "VBUS__2") (pintype "power_in") (solder_mask_margin 0.102) (tstamp db3a33b2-ee03-4aa7-9ea5-4f6cf7dc1a2d))
    (pad "B5" thru_hole circle (at 1.275 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 80 "unconnected-(J4-CC2-PadB5)") (pinfunction "CC2") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp ba2c5678-940c-402e-8be0-b97b80244200))
    (pad "B6" thru_hole circle (at 0.425 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 81 "unconnected-(J4-DP2-PadB6)") (pinfunction "DP2") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp a29571cc-b16b-4f1d-b41f-99283471e9c0))
    (pad "B7" thru_hole circle (at -0.425 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 82 "unconnected-(J4-DN2-PadB7)") (pinfunction "DN2") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 2a77ef20-4d1c-4a9d-a1c7-6a60ed10fe8d))
    (pad "B8" thru_hole circle (at -1.275 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 83 "unconnected-(J4-SBU2-PadB8)") (pinfunction "SBU2") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 1b7d9d7a-2207-46ea-be00-41899e8a7294))
    (pad "B9" thru_hole circle (at -2.125 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 84 "unconnected-(J4-VBUS__3-PadB9)") (pinfunction "VBUS__3") (pintype "power_in") (solder_mask_margin 0.102) (tstamp aa7f6ea6-7c2f-4cf4-9393-d5266ba0dc3c))
    (pad "B12" thru_hole circle (at -2.975 -3.01 90) (size 0.65 0.65) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 85 "unconnected-(J4-GND__3-PadB12)") (pinfunction "GND__3") (pintype "power_in") (solder_mask_margin 0.102) (tstamp ae29e9c2-53f7-48ca-b20b-086d7d87a780))
    (pad "S1" thru_hole oval (at -4.325 0 90) (size 0.9 1.7) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 86 "unconnected-(J4-SHELL-PadS1)") (pinfunction "SHELL") (pintype "passive") (solder_mask_margin 0.102) (tstamp a25eb255-8851-4801-bfdb-1ac0a8bf371f))
    (pad "S2" thru_hole oval (at 4.325 0 90) (size 0.9 1.7) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 87 "unconnected-(J4-SHELL__1-PadS2)") (pinfunction "SHELL__1") (pintype "passive") (solder_mask_margin 0.102) (tstamp fbd05bce-66b2-40ae-9a56-467468341595))
    (pad "S3" thru_hole oval (at -4.325 -3.38 90) (size 0.9 2.4) (drill oval 0.6 2.1) (layers "*.Cu" "*.Mask")
      (net 88 "unconnected-(J4-SHELL__2-PadS3)") (pinfunction "SHELL__2") (pintype "passive") (solder_mask_margin 0.102) (tstamp 365207b6-4d9f-4047-a970-9d337f6b0299))
    (pad "S4" thru_hole oval (at 4.325 -3.38 90) (size 0.9 2.4) (drill oval 0.6 2.1) (layers "*.Cu" "*.Mask")
      (net 89 "unconnected-(J4-SHELL__3-PadS4)") (pinfunction "SHELL__3") (pintype "passive") (solder_mask_margin 0.102) (tstamp 93b701c1-72c8-4939-9a4e-9d326404af6c))
    (model ":KICAD7_3DMODEL_DIR:Connector_USB.3dshapes/USB4085-GF-A_REVB.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tstamp a5f5dbb0-0ca9-45d8-8725-61d7fb4abcac)
    (at 163.5625 18.5)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "power")
    (path "/03abecec-4724-420e-920e-986ba2580308/980f3953-046e-451a-955e-c084c4e9f9e5")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp db460af3-f774-4630-a766-2be936917673)
    )
    (fp_text value "~" (at 0 3.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9d423be0-ce0f-4f7e-b847-e4f9c53ccc14)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp 5e6c05d0-1a4c-45d7-abf6-c520aa681faf)
    )
    (fp_line (start 0 -2.56) (end -3.45 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6de86524-1f27-42fd-848f-a8dc880c3ddd))
    (fp_line (start 0 -2.56) (end 1.95 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 503e9ea2-ee71-4007-93b3-5c8bb2652f13))
    (fp_line (start 0 2.56) (end -1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0cb92e4d-822d-4a8c-8e72-586e7eaea100))
    (fp_line (start 0 2.56) (end 1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f067cf14-b2a0-4c01-a9fc-255780fcbe28))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c14a1dfb-87bb-4c5d-9968-cddc15012d42))
    (fp_line (start -3.7 2.7) (end 3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d947d6ed-e36f-44cd-9a02-70b057b99c60))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0956804a-0d23-455b-8c72-cc4765f7e8f0))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 20827e9c-ccb5-49cc-af5f-447f199fbf21))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6cfd4e65-4bf2-4419-83ea-2e8446fdb676))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3aa80520-b39b-4077-b63f-e9857c12aeae))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9a1f5a6-ac6f-4779-8d7a-b40917db16e3))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5fbeaa9a-d91f-4da2-9c62-a74612c61e63))
    (fp_line (start 1.95 2.45) (end -1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6dee12fe-7c74-4797-8892-770753b02dc3))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 528 "unconnected-(U2-SW-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp d273f624-1a9c-4838-a388-f2072cafac7f))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 529 "unconnected-(U2-PGND-Pad2)") (pinfunction "PGND") (pintype "passive") (tstamp b260123c-c2dc-4108-9688-d9c72c004272))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 530 "unconnected-(U2-VINA-Pad3)") (pinfunction "VINA") (pintype "power_in") (tstamp aedd35ee-f1f7-448d-aa98-0f0039223dc0))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 531 "unconnected-(U2-EN-Pad4)") (pinfunction "EN") (pintype "input") (tstamp 2d9c0ce7-45b6-43ef-98cf-0267fd33226f))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 532 "unconnected-(U2-FB-Pad5)") (pinfunction "FB") (pintype "input") (tstamp ecd33f16-a610-41e1-a332-66b81b1a152f))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 533 "unconnected-(U2-AGND-Pad6)") (pinfunction "AGND") (pintype "passive") (tstamp 85604bed-5bf9-4e6d-928d-bd0daaf1cb6d))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 534 "unconnected-(U2-GND-Pad7)") (pinfunction "GND") (pintype "passive") (tstamp d902bd37-bf8e-4c3e-99a7-d794ab0da053))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 535 "unconnected-(U2-VINSW-Pad8)") (pinfunction "VINSW") (pintype "power_in") (tstamp e0f466dc-f7b4-41aa-87f5-ab338c571de5))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp ac92898f-6086-4986-bdb0-f4825b8f981e)
    (at 52.255 103.99)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/37a0c1b2-33b9-482f-a773-bb5dbfe1c4b4")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.43) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp afacedcc-3b0b-4bd9-accc-f34784eeed66)
    )
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fe22cf2b-f39b-490b-8d84-709b8651bfed)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 9b28a345-68c5-4480-aeda-915145005676)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 84fcb0f2-ffc6-4aa1-b9bc-e076d681ae42))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fe09b061-aef6-4395-9bff-920682994e29))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc9aa498-9650-4a04-b8bf-1aeba8c80fe0))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bfea12b3-1bfc-44a7-83fd-080f599c54bd))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bf24b02b-dc46-44fc-b1a3-330803717b58))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 109806f6-9b7f-4b67-8cc8-0aa4858ced6d))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c5588e2-5eee-4e4c-a57c-ce716f3f97fb))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 85ce0797-1399-47c6-85f7-d718189b8fc4))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7e55841-d5ab-4ae3-abfe-22b242f4b7d4))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d416219b-9e06-47ec-8ce0-6194dd585d7b))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 892fdb74-0f1c-4137-b910-882b4e51f7ae))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 44110638-f316-4226-af56-d8bd76a276f3))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "unconnected-(D1-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 7b59e5ba-6ede-4302-b910-76724a8a74ad))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "unconnected-(D1-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp d00aa147-ea75-4aa2-b399-5078f986788c))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_BGA:BGA-78_8.0x10.5mm_Layout9x12_P0.8mm" (layer "F.Cu")
    (tstamp af6535ac-feb2-426f-adfe-e7d29885e91b)
    (at 124.8 51.8)
    (property "Sheetfile" "ddr.kicad_sch")
    (property "Sheetname" "ddr")
    (path "/240fb45c-362d-4cf9-bead-d17ef15bf7d9/ab21b1c4-d997-4063-b47e-b9ae498f032b")
    (attr smd)
    (fp_text reference "U8" (at 0 -6.8 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2ea4c08-60a3-4dd3-a357-1715564750eb)
    )
    (fp_text value "~" (at 0 6.4 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a2b5f639-5b9a-4b36-81d8-6707bfe03d4f)
    )
    (fp_text user "A1" (at -5.2 -6.8 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left bottom))
      (tstamp 9eab58d2-f7d4-4ac7-a472-6ee992be71e1)
    )
    (fp_text user "${REFERENCE}" (at 0 0.4 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4d3ecfba-7aef-4873-a197-af0c460053a9)
    )
    (fp_line (start -4.8 -6.4) (end -3.2 -6.4)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 04859cd5-c7ed-458c-928b-abc7e6322e51))
    (fp_line (start -4.8 -4.8) (end -4.8 -6.4)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 37acd447-4daf-4569-8feb-d6b8d02b1a80))
    (fp_line (start -4.4 -6) (end -4.4 6)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 406c97a9-fdf1-42fc-8c8b-ddb6ee8c2a88))
    (fp_line (start -4.4 6) (end 4.4 6)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 098354ce-4ed1-41dd-86f8-3ef1d8ca6c4f))
    (fp_line (start 4.4 -6) (end -4.4 -6)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 77141f86-b3a3-46f4-877c-234504d41f41))
    (fp_line (start 4.4 6) (end 4.4 -6)
      (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 37275725-57b8-453c-af6c-17001577183c))
    (fp_line (start -4 -4.8) (end -4 5.6)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp e2650b0d-8012-4b5d-a4b4-6ae5818c2893))
    (fp_line (start -4 5.6) (end 4 5.6)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp dcb63a32-2736-48fe-a1dd-41a149f0620e))
    (fp_line (start -3.2 -5.6) (end -4 -4.8)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 13ab5918-96eb-42e9-91e1-60379f6e7c3b))
    (fp_line (start 4 -5.6) (end -3.2 -5.6)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3970dccf-5fb3-49ed-9180-6b4818b69b4d))
    (fp_line (start 4 5.6) (end 4 -5.6)
      (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c4092d1c-d2a2-4bae-9a59-f485e5af3ff0))
    (pad "A1" smd circle (at -3.2 -4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 605 "unconnected-(U8A-VSS-PadA1)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp 1a1d5f48-00e2-430e-afe7-1bf7e2987c04))
    (pad "A2" smd circle (at -2.4 -4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 606 "unconnected-(U8A-VDD-PadA2)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp e9719df3-aba5-4ec5-8596-ec24dcc985e4))
    (pad "A3" smd circle (at -1.6 -4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 607 "unconnected-(U8B-NC-PadA3)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.075) (tstamp cb76f4fb-8c81-41bd-90f7-f23297d3b8f0))
    (pad "A7" smd circle (at 1.6 -4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 608 "unconnected-(U8B-NF{slash}TDQS#-PadA7)") (pinfunction "NF/TDQS#") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 441e87af-b325-48fc-878d-81ffcbb326d9))
    (pad "A8" smd circle (at 2.4 -4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 609 "unconnected-(U8A-VSS-PadA8)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp 9e763d6b-1f87-435a-a4de-098b722c77a1))
    (pad "A9" smd circle (at 3.2 -4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 610 "unconnected-(U8A-VDD-PadA9)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp ee700f2d-6316-45d8-b311-a3ca8fd2867e))
    (pad "B1" smd circle (at -3.2 -4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 611 "unconnected-(U8A-VSS-PadB1)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp 33a6b229-0590-457e-b456-b75f5919a259))
    (pad "B2" smd circle (at -2.4 -4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 612 "unconnected-(U8A-VSSQ-PadB2)") (pinfunction "VSSQ") (pintype "passive") (solder_mask_margin 0.075) (tstamp 16fb0458-b2eb-4bce-aa69-ecab8d7661bf))
    (pad "B3" smd circle (at -1.6 -4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 613 "unconnected-(U8B-DQ0-PadB3)") (pinfunction "DQ0") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 23741704-efc4-43eb-89fd-a28b293e43ad))
    (pad "B7" smd circle (at 1.6 -4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 614 "unconnected-(U8B-DM{slash}TDQS-PadB7)") (pinfunction "DM/TDQS") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b7f758ac-5c58-46d9-b211-f5fbbb743d50))
    (pad "B8" smd circle (at 2.4 -4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 615 "unconnected-(U8A-VSSQ-PadB8)") (pinfunction "VSSQ") (pintype "passive") (solder_mask_margin 0.075) (tstamp ecfe7b07-0ccc-46b2-a959-b9ee4e4301c7))
    (pad "B9" smd circle (at 3.2 -4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 616 "unconnected-(U8A-VDDQ-PadB9)") (pinfunction "VDDQ") (pintype "power_in") (solder_mask_margin 0.075) (tstamp afce1e58-a223-4bce-880b-949a391ca8b8))
    (pad "C1" smd circle (at -3.2 -3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 617 "unconnected-(U8A-VDDQ-PadC1)") (pinfunction "VDDQ") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 4138230a-3832-41a0-9209-2a8a8e532823))
    (pad "C2" smd circle (at -2.4 -3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 618 "unconnected-(U8B-DQ2-PadC2)") (pinfunction "DQ2") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp f2c46f04-a3ee-46bc-b5fb-34cf35923a47))
    (pad "C3" smd circle (at -1.6 -3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 619 "unconnected-(U8B-DQS-PadC3)") (pinfunction "DQS") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp d225ccce-8c5c-4948-a38e-1d775c694fea))
    (pad "C7" smd circle (at 1.6 -3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 620 "unconnected-(U8B-DQ1-PadC7)") (pinfunction "DQ1") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 4186d465-dbe9-475a-a59a-86df64440d3c))
    (pad "C8" smd circle (at 2.4 -3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 621 "unconnected-(U8B-DQ3-PadC8)") (pinfunction "DQ3") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 105dd9bf-9f03-4b6a-9502-33842b1dd54f))
    (pad "C9" smd circle (at 3.2 -3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 622 "unconnected-(U8A-VSSQ-PadC9)") (pinfunction "VSSQ") (pintype "passive") (solder_mask_margin 0.075) (tstamp 16ce63b0-3b01-4fde-ad27-12e632c0ce8b))
    (pad "D1" smd circle (at -3.2 -2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 623 "unconnected-(U8A-VSSQ-PadD1)") (pinfunction "VSSQ") (pintype "passive") (solder_mask_margin 0.075) (tstamp 29b27e46-64b1-46b6-a695-232c8c2046bf))
    (pad "D2" smd circle (at -2.4 -2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 624 "unconnected-(U8B-DQ6-PadD2)") (pinfunction "DQ6") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp b0b8cb29-73b4-4008-801f-6c701c16ac25))
    (pad "D3" smd circle (at -1.6 -2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 625 "unconnected-(U8B-DQS#-PadD3)") (pinfunction "DQS#") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 1b1bec3f-a376-4330-b3f1-d156a9fe8826))
    (pad "D7" smd circle (at 1.6 -2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 626 "unconnected-(U8A-VDD-PadD7)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 889881f6-38db-49f8-bef9-7128d1554073))
    (pad "D8" smd circle (at 2.4 -2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 627 "unconnected-(U8A-VSS-PadD8)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp a2393fd2-b3d4-40b6-8512-8675f2914f87))
    (pad "D9" smd circle (at 3.2 -2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 628 "unconnected-(U8A-VSSQ-PadD9)") (pinfunction "VSSQ") (pintype "passive") (solder_mask_margin 0.075) (tstamp 83ae6565-a41f-4f9e-8bf9-cbd3db7e0a98))
    (pad "E1" smd circle (at -3.2 -1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 629 "unconnected-(U8A-VREFDQ-PadE1)") (pinfunction "VREFDQ") (pintype "input") (solder_mask_margin 0.075) (tstamp d7f23a10-553e-4ca2-93ac-01c06c8c6445))
    (pad "E2" smd circle (at -2.4 -1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 630 "unconnected-(U8A-VDDQ-PadE2)") (pinfunction "VDDQ") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 8d1f6050-b0d9-4db6-add6-61788f00189b))
    (pad "E3" smd circle (at -1.6 -1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 631 "unconnected-(U8B-DQ4-PadE3)") (pinfunction "DQ4") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 6bd3a93c-c939-4965-b1ae-3a8c6027e705))
    (pad "E7" smd circle (at 1.6 -1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 632 "unconnected-(U8B-DQ7-PadE7)") (pinfunction "DQ7") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 5507ba13-bf9e-4915-b139-e9aec29af2aa))
    (pad "E8" smd circle (at 2.4 -1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 633 "unconnected-(U8B-DQ5-PadE8)") (pinfunction "DQ5") (pintype "bidirectional") (solder_mask_margin 0.075) (tstamp 8bd50122-d97b-403e-b027-ce6c1c5b6409))
    (pad "E9" smd circle (at 3.2 -1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 634 "unconnected-(U8A-VDDQ-PadE9)") (pinfunction "VDDQ") (pintype "power_in") (solder_mask_margin 0.075) (tstamp f5986756-62a8-45d1-828e-f6d00acce5b0))
    (pad "F1" smd circle (at -3.2 -0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 635 "unconnected-(U8B-NC-PadF1)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.075) (tstamp 094209f6-3846-42ea-999a-9d776eae6d90))
    (pad "F2" smd circle (at -2.4 -0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 636 "unconnected-(U8A-VSS-PadF2)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp e21227b7-a429-496a-92ae-8052869378e6))
    (pad "F3" smd circle (at -1.6 -0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 637 "unconnected-(U8B-RAS#-PadF3)") (pinfunction "RAS#") (pintype "input") (solder_mask_margin 0.075) (tstamp 98dc12f0-7a2d-493f-be6c-f3dd888e92ff))
    (pad "F7" smd circle (at 1.6 -0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 638 "unconnected-(U8B-CK-PadF7)") (pinfunction "CK") (pintype "input") (solder_mask_margin 0.075) (tstamp af0d90c4-fd4f-4744-b771-c404b735f261))
    (pad "F8" smd circle (at 2.4 -0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 639 "unconnected-(U8A-VSS-PadF8)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp eb157d56-a253-4b41-8b56-75b3caedd416))
    (pad "F9" smd circle (at 3.2 -0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 640 "unconnected-(U8B-NC-PadF9)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.075) (tstamp 7bdcf1e5-9f48-4634-b36d-1940cc012dda))
    (pad "G1" smd circle (at -3.2 0) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 641 "unconnected-(U8B-ODT-PadG1)") (pinfunction "ODT") (pintype "passive") (solder_mask_margin 0.075) (tstamp 60f7b03f-282e-4e91-a8f6-9a496c0e9aa2))
    (pad "G2" smd circle (at -2.4 0) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 642 "unconnected-(U8A-VDD-PadG2)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 4f7e3047-d8bd-4ddb-9e9e-689af6f292ef))
    (pad "G3" smd circle (at -1.6 0) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 643 "unconnected-(U8B-CAS#-PadG3)") (pinfunction "CAS#") (pintype "input") (solder_mask_margin 0.075) (tstamp f1336702-77dc-4112-817a-032270b5af99))
    (pad "G7" smd circle (at 1.6 0) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 644 "unconnected-(U8B-CK#-PadG7)") (pinfunction "CK#") (pintype "input") (solder_mask_margin 0.075) (tstamp 07d2b1eb-d124-44a2-ae4e-7f735eb987c0))
    (pad "G8" smd circle (at 2.4 0) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 645 "unconnected-(U8A-VDD-PadG8)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 3f08a8d3-1060-4cac-87c3-092dd1c62718))
    (pad "G9" smd circle (at 3.2 0) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 646 "unconnected-(U8B-CKE-PadG9)") (pinfunction "CKE") (pintype "input") (solder_mask_margin 0.075) (tstamp 593abc9d-9c03-42bb-8fb7-089a5c9e7b81))
    (pad "H1" smd circle (at -3.2 0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 647 "unconnected-(U8B-NC-PadH1)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.075) (tstamp 353ec1a3-a135-4cb0-8bfe-0e1b48cbfdf0))
    (pad "H2" smd circle (at -2.4 0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 648 "unconnected-(U8B-CS#-PadH2)") (pinfunction "CS#") (pintype "input") (solder_mask_margin 0.075) (tstamp b60a6954-5a1a-4ef7-ba3c-c84ffdc8f09d))
    (pad "H3" smd circle (at -1.6 0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 649 "unconnected-(U8B-WE#-PadH3)") (pinfunction "WE#") (pintype "input") (solder_mask_margin 0.075) (tstamp bc2f3831-6def-4a7b-9b5b-72c8995ae8e1))
    (pad "H7" smd circle (at 1.6 0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 650 "unconnected-(U8B-A10{slash}AP-PadH7)") (pinfunction "A10/AP") (pintype "input") (solder_mask_margin 0.075) (tstamp 710ee52f-4713-432e-bf78-26587f895e0d))
    (pad "H8" smd circle (at 2.4 0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 651 "unconnected-(U8B-ZQ-PadH8)") (pinfunction "ZQ") (pintype "passive") (solder_mask_margin 0.075) (tstamp d0b8df8d-9b10-4b39-8940-5d3b71306c9e))
    (pad "H9" smd circle (at 3.2 0.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 652 "unconnected-(U8B-NC-PadH9)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.075) (tstamp 58600f6d-b4c4-4e3e-8032-10bea8d013fc))
    (pad "J1" smd circle (at -3.2 1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 653 "unconnected-(U8A-VSS-PadJ1)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp 5774e4e6-bf88-4acc-95a5-d65b1453a264))
    (pad "J2" smd circle (at -2.4 1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 654 "unconnected-(U8B-BA0-PadJ2)") (pinfunction "BA0") (pintype "input") (solder_mask_margin 0.075) (tstamp b255ba73-8dab-4dad-8348-43f2b6d252ed))
    (pad "J3" smd circle (at -1.6 1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 655 "unconnected-(U8B-BA2-PadJ3)") (pinfunction "BA2") (pintype "input") (solder_mask_margin 0.075) (tstamp c8b2e1f0-a924-49e3-b682-ae246659f15b))
    (pad "J7" smd circle (at 1.6 1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 656 "unconnected-(U8B-NC-PadJ7)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.075) (tstamp 9bebf88e-9a7c-4713-a859-d22a84c490d8))
    (pad "J8" smd circle (at 2.4 1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 657 "unconnected-(U8A-VREFCA-PadJ8)") (pinfunction "VREFCA") (pintype "input") (solder_mask_margin 0.075) (tstamp 14e70c93-44a8-4035-9394-acfb242b33dd))
    (pad "J9" smd circle (at 3.2 1.6) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 658 "unconnected-(U8A-VSS-PadJ9)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp b24aaab1-4da4-422f-bff3-917ad7a1bdea))
    (pad "K1" smd circle (at -3.2 2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 659 "unconnected-(U8A-VDD-PadK1)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 83552bf9-e50d-4989-ad68-986816b71ca6))
    (pad "K2" smd circle (at -2.4 2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 660 "unconnected-(U8B-A3-PadK2)") (pinfunction "A3") (pintype "input") (solder_mask_margin 0.075) (tstamp 2cb3a272-b555-4dc3-a9fe-a1620cae10cc))
    (pad "K3" smd circle (at -1.6 2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 661 "unconnected-(U8B-A0-PadK3)") (pinfunction "A0") (pintype "input") (solder_mask_margin 0.075) (tstamp d90703a9-a4a9-4841-b5bb-7bebec1098b3))
    (pad "K7" smd circle (at 1.6 2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 662 "unconnected-(U8B-A12{slash}BC#-PadK7)") (pinfunction "A12/BC#") (pintype "input") (solder_mask_margin 0.075) (tstamp de4ce270-2560-432c-b895-bf3efe2c8641))
    (pad "K8" smd circle (at 2.4 2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 663 "unconnected-(U8B-BA1-PadK8)") (pinfunction "BA1") (pintype "input") (solder_mask_margin 0.075) (tstamp 01618266-42cd-4d10-b179-71f82d5db8c1))
    (pad "K9" smd circle (at 3.2 2.4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 664 "unconnected-(U8A-VDD-PadK9)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp a71973e3-2836-4f90-a5bb-9a8a6418a9e7))
    (pad "L1" smd circle (at -3.2 3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 665 "unconnected-(U8A-VSS-PadL1)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp 3736b9b4-f7ab-4582-9f0a-4ccdc5470373))
    (pad "L2" smd circle (at -2.4 3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 666 "unconnected-(U8B-A5-PadL2)") (pinfunction "A5") (pintype "input") (solder_mask_margin 0.075) (tstamp f52758af-2a65-4b33-8c3a-c32cd96bd243))
    (pad "L3" smd circle (at -1.6 3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 667 "unconnected-(U8B-A2-PadL3)") (pinfunction "A2") (pintype "input") (solder_mask_margin 0.075) (tstamp 24f9cdb1-4887-4395-aa0d-b00ee631fd61))
    (pad "L7" smd circle (at 1.6 3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 668 "unconnected-(U8B-A1-PadL7)") (pinfunction "A1") (pintype "input") (solder_mask_margin 0.075) (tstamp 4ae55e0d-9031-445e-a6de-3887562bcb63))
    (pad "L8" smd circle (at 2.4 3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 669 "unconnected-(U8B-A4-PadL8)") (pinfunction "A4") (pintype "input") (solder_mask_margin 0.075) (tstamp 657ea4f0-1ccb-4986-98af-2afb6b1573a5))
    (pad "L9" smd circle (at 3.2 3.2) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 670 "unconnected-(U8A-VSS-PadL9)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp aff19193-67da-4ce1-a265-4e1c1105dd45))
    (pad "M1" smd circle (at -3.2 4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 671 "unconnected-(U8A-VDD-PadM1)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 06ea7f0e-5ed1-485c-9d9d-00e4199e02f8))
    (pad "M2" smd circle (at -2.4 4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 672 "unconnected-(U8B-A7-PadM2)") (pinfunction "A7") (pintype "input") (solder_mask_margin 0.075) (tstamp 3412226e-2ecc-4310-9543-0d1b1e0ca822))
    (pad "M3" smd circle (at -1.6 4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 673 "unconnected-(U8B-A9-PadM3)") (pinfunction "A9") (pintype "input") (solder_mask_margin 0.075) (tstamp 8f3420eb-ee7f-4af8-bc16-3b423fee57b4))
    (pad "M7" smd circle (at 1.6 4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 674 "unconnected-(U8B-A11-PadM7)") (pinfunction "A11") (pintype "input") (solder_mask_margin 0.075) (tstamp b3d07aef-0634-4a51-b754-ab1ac685c0fb))
    (pad "M8" smd circle (at 2.4 4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 675 "unconnected-(U8B-A6-PadM8)") (pinfunction "A6") (pintype "input") (solder_mask_margin 0.075) (tstamp c77ba9df-57ea-46de-b115-249ee9f42554))
    (pad "M9" smd circle (at 3.2 4) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 676 "unconnected-(U8A-VDD-PadM9)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.075) (tstamp 9580a218-a0ed-47dc-8de2-6d27c74e4833))
    (pad "N1" smd circle (at -3.2 4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 677 "unconnected-(U8A-VSS-PadN1)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp be0fb399-cf5f-419a-b4c8-19bcbb002556))
    (pad "N2" smd circle (at -2.4 4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 678 "unconnected-(U8B-RESET#-PadN2)") (pinfunction "RESET#") (pintype "input") (solder_mask_margin 0.075) (tstamp 99f11a31-faf8-420b-bf60-6326575b1652))
    (pad "N3" smd circle (at -1.6 4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 679 "unconnected-(U8B-A13-PadN3)") (pinfunction "A13") (pintype "input") (solder_mask_margin 0.075) (tstamp 17dba100-01e3-4bfe-8649-a434fd140bf5))
    (pad "N7" smd circle (at 1.6 4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 680 "unconnected-(U8B-A14-PadN7)") (pinfunction "A14") (pintype "input") (solder_mask_margin 0.075) (tstamp cbe81bdd-6464-4072-ac9f-35d9692086cf))
    (pad "N8" smd circle (at 2.4 4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 681 "unconnected-(U8B-A8-PadN8)") (pinfunction "A8") (pintype "input") (solder_mask_margin 0.075) (tstamp 07f82636-8466-4b1b-8e24-fc3654c2e0fc))
    (pad "N9" smd circle (at 3.2 4.8) (size 0.35 0.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 682 "unconnected-(U8A-VSS-PadN9)") (pinfunction "VSS") (pintype "passive") (solder_mask_margin 0.075) (tstamp ff18f184-a043-4dd5-a15c-2a8eed59ac01))
    (model ":KICAD7_3DMODEL_DIR:Package_BGA.3dshapes/FBGA78_8X10P5_MRN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Dsub:ICD15S13E4GX00LF" (layer "F.Cu")
    (tstamp b94c0c15-86e3-48e7-a7eb-a3814dc7edf8)
    (at 99.696 34.9955 180)
    (property "Sheetfile" "vga.kicad_sch")
    (property "Sheetname" "vga")
    (property "ki_description" "15-pin female D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole")
    (property "ki_keywords" "connector db15 female D-SUB VGA")
    (path "/337f91b2-5935-41a8-adab-77c6de100854/1304e346-2941-4d1f-bdd3-806c52aa2045")
    (attr through_hole)
    (fp_text reference "J1" (at -5.08 -5.08 180 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a99f71b-9ce4-45f7-9299-34df2fa81b7d)
    )
    (fp_text value "DB15_Female_HighDensity_MountingHoles" (at 0 -7.62 180 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e11b5ac-ce11-4b0c-bf1e-e168fdef476e)
    )
    (fp_text user "${REFERENCE}" (at 0 -5.08 180 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd67b241-be7d-4c1e-9506-222370c5c966)
    )
    (fp_line (start -3.302 3.302) (end -3.302 -4.572)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c38f45fa-91bf-4147-928c-044b2a649ab3))
    (fp_line (start -3.302 3.556) (end -3.302 3.302)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8983970b-3937-494a-b729-439beb819bc7))
    (fp_line (start 28.194 -4.572) (end -3.302 -4.572)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 286f4d44-9c81-4712-a5d3-82490c522763))
    (fp_line (start 28.194 -4.572) (end 28.194 2.794)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ddebc395-f4f7-46d2-a156-3eeadb9b80eb))
    (fp_line (start 28.194 3.556) (end 28.194 2.794)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ce03e96a-2134-442d-8839-8c4e9af9bba3))
    (fp_rect (start -2.91 11.43) (end 27.9 -4.1)
      (stroke (width 0.12) (type solid)) (fill none) (layer "Dwgs.User") (tstamp 34721024-3a44-44df-9020-c970ea02cda7))
    (fp_rect (start -2.25 11.43) (end 2.25 21.7)
      (stroke (width 0.12) (type solid)) (fill none) (layer "Dwgs.User") (tstamp a4644a66-26f0-4d8c-97d6-e804efb097d4))
    (fp_rect (start 4.39 11.43) (end 20.06 21.7)
      (stroke (width 0.12) (type solid)) (fill none) (layer "Dwgs.User") (tstamp b902ca1f-80a2-4c16-95db-fc42e7db0b31))
    (fp_rect (start 22.74 11.43) (end 27.24 21.7)
      (stroke (width 0.12) (type solid)) (fill none) (layer "Dwgs.User") (tstamp 0dd7ea94-9e10-4c3c-8658-ee5bb27b55a5))
    (fp_rect (start -3.302 -4.572) (end 28.194 22.098)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 6e6989eb-fdc6-475b-824d-0f6e6e724159))
    (pad "0" thru_hole circle (at 0 0 180) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J1-Pad0)") (pintype "passive") (tstamp cc22ea62-5eae-4e43-afe1-c59c027f032a))
    (pad "0" thru_hole circle (at 24.99 0 180) (size 4 4) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J1-Pad0)") (pintype "passive") (tstamp 660460da-5d1f-4314-bd9d-619f863ae218))
    (pad "1" thru_hole rect (at 16.8 -2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J1-Pad1)") (pintype "passive") (tstamp a651c2b0-d0f7-4d02-a884-bd8f6629422b))
    (pad "2" thru_hole circle (at 14.515 -2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J1-Pad2)") (pintype "passive") (tstamp 2e93e062-4bc7-429a-b7d6-f00903bab263))
    (pad "3" thru_hole circle (at 12.23 -2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J1-Pad3)") (pintype "passive") (tstamp 1fd694e3-fa99-4d5a-93fb-65acb78642d8))
    (pad "4" thru_hole circle (at 9.945 -2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(J1-Pad4)") (pintype "passive") (tstamp 0e461938-4e95-41a0-b504-1602cdfc1422))
    (pad "5" thru_hole circle (at 7.66 -2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(J1-Pad5)") (pintype "passive") (tstamp 6f0f91ff-f2bf-434a-8a66-6e68f9fed0eb))
    (pad "6" thru_hole circle (at 17.9425 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(J1-Pad6)") (pintype "passive") (tstamp ff8718d2-133c-443a-8947-189d3be227f2))
    (pad "7" thru_hole circle (at 15.6575 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(J1-Pad7)") (pintype "passive") (tstamp 62ca90c8-307f-4ad4-b64a-b5961958681e))
    (pad "8" thru_hole circle (at 13.3725 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(J1-Pad8)") (pintype "passive") (tstamp 20b1772b-bb16-4200-b61a-a629a08212c3))
    (pad "9" thru_hole circle (at 11.0875 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(J1-Pad9)") (pintype "passive") (tstamp 7d9e031e-6bf1-429f-a99f-6e970598160f))
    (pad "10" thru_hole circle (at 8.8025 0 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(J1-Pad10)") (pintype "passive") (tstamp 91caa036-6ad7-41d2-bcdb-5a395b783aae))
    (pad "11" thru_hole circle (at 16.8 2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(J1-Pad11)") (pintype "passive") (tstamp cae0fe3c-e6b4-400c-a8e4-94d571a52978))
    (pad "12" thru_hole circle (at 14.515 2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(J1-Pad12)") (pintype "passive") (tstamp 7423b662-edaf-4489-afff-8f826d3ead1c))
    (pad "13" thru_hole circle (at 12.23 2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(J1-Pad13)") (pintype "passive") (tstamp eca687dc-d570-45f9-9b05-b88301e32f13))
    (pad "14" thru_hole circle (at 9.945 2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(J1-Pad14)") (pintype "passive") (tstamp 6d96446d-bc9f-47c2-9c11-87d638b69144))
    (pad "15" thru_hole circle (at 7.66 2.54 180) (size 1.6 1.6) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(J1-Pad15)") (pintype "passive") (tstamp b64a42ff-6a04-457b-87d3-2723e45b4c99))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/sicd15s13e4gx00lf.stp"
      (offset (xyz 12.5 -11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp bc7c464f-cdcb-44b6-8554-f30c903a1703)
    (at 34 32.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/146facc4-c213-4655-9e5c-415d11349114")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 18a2edac-eeef-4148-a870-9b1c1efae55c)
    )
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f7b83e4-7a7c-4f49-af02-765f881c578a)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp cb55c0fa-f2f8-437d-a18d-924c33d41283)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c55b36a0-9155-4ebc-b722-bc2561c2ace1))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bdb31e72-905a-408b-b2ce-89d89972f58e))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 453dd0be-b9b6-490d-9a3e-505ceae0632d))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4b145817-aac2-430b-9cb9-18e6fd36cb2b))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 28b1b2a6-02f1-4752-a848-8d82849a438b))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 22dce87e-d0f3-40e0-a57b-241a345e5aae))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15b1e258-c47d-411b-acb3-0b9827f44fce))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 05f50402-d387-426a-9095-eafacbdce159))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b595b99a-8bb7-4a55-9aab-c5b43865c526))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 773d50b6-41e3-42d5-8025-b9bedcd224a0))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 572 "+3V3") (pintype "passive") (tstamp fcb462b0-28eb-40af-bab2-1c99f2a2f8e6))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 568 "/cpu/~{CPU_IRQB}") (pintype "passive") (tstamp bc36e32d-a233-4259-818b-074a519f1a76))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp bccbeb0c-8c8c-4b23-8072-ce7b89d5560e)
    (at 58.5 29.75 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "cpu.kicad_sch")
    (property "Sheetname" "cpu")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/a28bae45-a41d-48aa-8dee-a2333866db3d/4c9c1a76-2c78-4bfd-8b23-c5b16bc91541")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 58046e41-e18a-46ce-845c-98f721123129)
    )
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a64579b-6cd8-42bf-9288-6b52bc8729d9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 9bec3eba-35b9-470b-992e-a76b44912671)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5e85bf3d-2b8a-4c67-99da-d1abeaebedd8))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 730a4352-b5f4-47c1-8d4e-846c6a4dd426))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e2b8d009-27f2-48a8-988b-f66c30011641))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a311728-5178-4a8c-bc06-1e92ecad81a1))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 54889d69-dc72-4921-95c5-6236307e2d3f))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9e23fefd-36a8-423a-a30b-3c0f3c4a23b9))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp af5c6549-9a3e-4feb-a0db-9c19a3236a3a))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64b6ef33-c911-4548-87e3-0e45447d6e29))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fb002f1-3d5b-4401-9ce5-f213ac473014))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 124db5bf-7d88-4f63-96c6-942936a143cb))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 572 "+3V3") (pintype "passive") (tstamp 85838fd7-b23b-484e-a128-22d3d7788d88))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 602 "Net-(U7-~{SOB})") (pintype "passive") (tstamp 5bca09b8-bfdb-4872-abcb-a334c4c6278a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Display_7Segment:LTS-4802B" (layer "F.Cu")
    (tstamp bce76a1d-105e-452b-8a96-0099b5cab747)
    (at 83.75 90.34)
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/2479b6f1-63bd-4d7e-89df-43651605954f")
    (attr through_hole)
    (fp_text reference "U14" (at 0 -2.54 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9fbdaa22-e770-4b6b-a210-a1f6c71ac981)
    )
    (fp_text value "~" (at 3.58 13.1 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fdef4409-7325-48f1-957c-54824ddb6d6a)
    )
    (fp_text user "${REFERENCE}" (at 3.58 4.01 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bc51f72c-6ca1-488d-9027-c25ffe8c1e1f)
    )
    (fp_rect (start -1.04 -1.07) (end 8.66 11.83)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 1b909212-e0f2-422e-937d-492351dbfd4c))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 771 "unconnected-(U14-CA-Pad1)") (pinfunction "CA") (pintype "passive") (tstamp c9a95ef1-c836-4b13-88df-8e33cb346601))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 772 "unconnected-(U14-F-Pad2)") (pinfunction "F") (pintype "passive") (tstamp d031cdab-ff74-44bb-9c23-12ff12bf5d8b))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 773 "unconnected-(U14-G-Pad3)") (pinfunction "G") (pintype "passive") (tstamp 9fbabffc-a631-4279-bdfa-ecbf4b327dfa))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 774 "unconnected-(U14-E-Pad4)") (pinfunction "E") (pintype "passive") (tstamp 57d67848-babf-4537-945f-b94543175fe5))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 775 "unconnected-(U14-D-Pad5)") (pinfunction "D") (pintype "passive") (tstamp 9f6d27c0-197e-4469-b26f-4b85c782f0a4))
    (pad "6" thru_hole circle (at 7.62 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 776 "unconnected-(U14-CA-Pad6)") (pinfunction "CA") (pintype "passive") (tstamp 62176283-bac7-4ba9-b87b-9f0fe0a40684))
    (pad "7" thru_hole circle (at 7.62 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 777 "unconnected-(U14-DP-Pad7)") (pinfunction "DP") (pintype "passive") (tstamp 942043ba-6e1c-4852-a5ce-94364251bebf))
    (pad "8" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 778 "unconnected-(U14-C-Pad8)") (pinfunction "C") (pintype "passive") (tstamp d209d519-6d71-494e-bd0c-4ec199008cd2))
    (pad "9" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 779 "unconnected-(U14-B-Pad9)") (pinfunction "B") (pintype "passive") (tstamp dd150cd3-b088-4977-ad5b-51b5a26e5534))
    (pad "10" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 780 "unconnected-(U14-A-Pad10)") (pinfunction "A") (pintype "passive") (tstamp 81157c07-b572-40c1-8a23-976565726158))
    (model ":KICAD7_3DMODEL_DIR:Display_7Segment.3dshapes/LTS-4802BJR-H1_LTO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tstamp daa5e0db-a96b-42e5-93af-6f3ae680d82d)
    (at 163.5625 37.85)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Sheetfile" "power.kicad_sch")
    (property "Sheetname" "power")
    (path "/03abecec-4724-420e-920e-986ba2580308/f34d2cc9-f847-42ed-a77e-9035eec2b59f")
    (attr smd)
    (fp_text reference "U5" (at 0 -3.4) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 54808bd8-5dac-4b49-a4c5-4fdd0e110fac)
    )
    (fp_text value "~" (at 0 3.4) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e51217b-64aa-4346-819b-e0fb43f325c0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp 36f3a2e4-e805-4627-bb42-fc3a37ee5c84)
    )
    (fp_line (start 0 -2.56) (end -3.45 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8d725f77-c2c7-4ff3-9edc-6e299df90617))
    (fp_line (start 0 -2.56) (end 1.95 -2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 55ffb72a-7a84-442a-98e9-8638e251f5ff))
    (fp_line (start 0 2.56) (end -1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dcb0bdf2-c212-4799-abfc-6ce21fc86d45))
    (fp_line (start 0 2.56) (end 1.95 2.56)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 13868b21-71f9-408e-b81d-e0002de147f4))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d5c6b952-df33-4b8a-845e-9806ff6d52e5))
    (fp_line (start -3.7 2.7) (end 3.7 2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 952a4ccb-881f-4680-9e60-236c9ddbe463))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6963e5f6-ae51-4000-bf94-2fa4a3a4e0de))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 880537c3-ce0c-466b-a9e0-9be5f68061e9))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d80f814c-2b36-4fb7-a9d9-b35cd5fe31af))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d00c0da4-aa1d-4d5b-8080-ee1aeb504761))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c3aef710-340b-46ed-ba04-e04fc38c4d6e))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 62c19b7b-efce-4f27-b190-ac5002873bcf))
    (fp_line (start 1.95 2.45) (end -1.95 2.45)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b6d2122a-3b95-4e0a-9965-4ae7ba1322d9))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 552 "unconnected-(U5-SW-Pad1)") (pinfunction "SW") (pintype "power_out") (tstamp 81671f05-f2df-4d35-a49b-a86ba220405c))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 553 "unconnected-(U5-PGND-Pad2)") (pinfunction "PGND") (pintype "passive") (tstamp c6c7105b-5bae-4482-ba2e-9b0bff5e031e))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 554 "unconnected-(U5-VINA-Pad3)") (pinfunction "VINA") (pintype "power_in") (tstamp cb297392-9b5b-4ec7-a793-56f2db692bb7))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 555 "unconnected-(U5-EN-Pad4)") (pinfunction "EN") (pintype "input") (tstamp e4b9484b-1e0c-4eec-892f-9e7cfa6d11a8))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 556 "unconnected-(U5-FB-Pad5)") (pinfunction "FB") (pintype "input") (tstamp 4c61d62b-5de3-4d9b-9bc8-5491311eeace))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 557 "unconnected-(U5-AGND-Pad6)") (pinfunction "AGND") (pintype "passive") (tstamp 6956cc9e-e286-4e95-8346-40abcbdce739))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 558 "unconnected-(U5-GND-Pad7)") (pinfunction "GND") (pintype "passive") (tstamp 796eec8f-3f85-4c6f-87d9-20e8891a1550))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 559 "unconnected-(U5-VINSW-Pad8)") (pinfunction "VINSW") (pintype "power_in") (tstamp d1c5d13b-bf6d-4238-9ec2-d3c83148702a))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOP-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_USB:0672984091" (layer "F.Cu")
    (tstamp db103249-1d69-45eb-afd3-8360dc8b8a60)
    (at 141.0725 93.885)
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "usb")
    (property "ki_description" "USB Type A connector, stacked")
    (property "ki_keywords" "connector USB")
    (path "/608a5705-96be-4a71-b2b6-c4625a5aee39/86eb4b0b-0107-4d3e-86c4-d8a84cb43ca6")
    (attr through_hole)
    (fp_text reference "J6" (at 3.5 -8 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 030642c5-1972-4464-a624-1146438453f1)
    )
    (fp_text value "USB_A_Stacked" (at 3.5 3 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 30a091de-b903-4f1a-97e3-1ad30ebfe70b)
    )
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cc075cd6-a5f0-43de-aa57-db161d531031)
    )
    (fp_rect (start -6 -6.5) (end 13 15)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 2a449e0e-95ef-41ec-9e3b-73831c79c666))
    (fp_rect (start -5.5 -6) (end 12.5 14.5)
      (stroke (width 0.12) (type default)) (fill none) (layer "F.Fab") (tstamp 801de7d6-0629-455a-a31e-4ee34cd0afac))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 99 "unconnected-(J6-VBUS1-Pad1)") (pinfunction "VBUS1") (pintype "power_in") (tstamp 723f741d-3e6d-44b5-9b28-dad6afc6cd66))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 100 "unconnected-(J6-D1--Pad2)") (pinfunction "D1-") (pintype "bidirectional") (tstamp 30d89b0a-7c9b-4a23-8a2e-b42001abe32d))
    (pad "3" thru_hole circle (at 4.5 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 101 "unconnected-(J6-D1+-Pad3)") (pinfunction "D1+") (pintype "bidirectional") (tstamp 0c655cde-fc49-4e79-a849-faf0b7e0bec2))
    (pad "4" thru_hole circle (at 7 0) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 102 "unconnected-(J6-GND1-Pad4)") (pinfunction "GND1") (pintype "power_in") (tstamp 4fee1c55-bdbb-40fd-ac54-aaefabfa992d))
    (pad "5" thru_hole circle (at 0 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 103 "unconnected-(J6-VBUS2-Pad5)") (pinfunction "VBUS2") (pintype "power_in") (tstamp 13e3a39f-4bb9-45be-89f1-e4c32ff215dc))
    (pad "6" thru_hole circle (at 2.5 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 104 "unconnected-(J6-D2--Pad6)") (pinfunction "D2-") (pintype "bidirectional") (tstamp 0c710e13-fb32-4f55-9407-055f50a8f947))
    (pad "7" thru_hole circle (at 4.5 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 105 "unconnected-(J6-D2+-Pad7)") (pinfunction "D2+") (pintype "bidirectional") (tstamp 4ca26473-667e-4b86-978f-fd2082f1d05f))
    (pad "8" thru_hole circle (at 7 -2.62) (size 1.5 1.5) (drill 0.92) (layers "*.Cu" "*.Mask")
      (net 106 "unconnected-(J6-GND2-Pad8)") (pinfunction "GND2") (pintype "power_in") (tstamp 158c3cd0-28f2-4a9c-b2b6-6643a8b6877b))
    (pad "9" thru_hole circle (at -3.07 -2.97) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(J6-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp 29d6861b-12f2-4a9d-bbc2-f9adfbe99da3))
    (pad "9" thru_hole circle (at -3.07 2.71) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(J6-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp d82cc64f-bb0f-4bd9-afeb-7d776123e305))
    (pad "9" thru_hole circle (at 10.07 -2.97) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(J6-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp 7e9a7f80-70c0-4f7d-83ea-d25fdd32ef6c))
    (pad "9" thru_hole circle (at 10.07 2.71) (size 3.5 3.5) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(J6-Shield-Pad9)") (pinfunction "Shield") (pintype "passive") (tstamp c357180e-379e-4e5b-82a9-847f8b6c98aa))
    (model ":KICAD7_3DMODEL_DIR:Connector_USB.3dshapes/672984091.stp"
      (offset (xyz 3.5 -12.5 7.8))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )

  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tstamp eb094921-985f-4022-ae15-6f734e5fb75d)
    (at 77.7 55.1 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/2e5bc80e-61f2-449b-bd47-345c91fbc33a")
    (attr through_hole)
    (fp_text reference "SW3" (at 3.25 -2 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b30efae3-5794-49ff-ba07-67eb5ef60623)
    )
    (fp_text value "SW_Push" (at 3.75 6.7 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6935c6ea-6a4a-4946-920d-09e4c0ecdec8)
    )
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9ac967e0-4972-40f8-ac6f-583f90e19f33)
    )
    (fp_line (start -0.25 1.5) (end -0.25 3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4135e70-ebd8-4936-ab95-716467429289))
    (fp_line (start 1 5.5) (end 5.5 5.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c2f8c3c-b1b2-475e-9935-dfbb26201541))
    (fp_line (start 5.5 -1) (end 1 -1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 96e94f67-b7bf-47b6-9dc6-1263b6723015))
    (fp_line (start 6.75 3) (end 6.75 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 377febc7-b386-42f3-b58d-4529d8c56eb7))
    (fp_line (start -1.5 -1.5) (end -1.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0c308c89-1de3-45da-abc1-d8977401edab))
    (fp_line (start -1.5 -1.25) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7d7496f4-2e40-4981-af3a-295f52ad6825))
    (fp_line (start -1.5 5.75) (end -1.5 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd21edf4-cd9c-46c1-949e-6f722c405992))
    (fp_line (start -1.5 5.75) (end -1.5 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6e40b578-a27a-4f2e-9e9f-4aba5c9b15a7))
    (fp_line (start -1.5 6) (end -1.25 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d4363d24-550d-43cf-a367-bcddd072c0f6))
    (fp_line (start -1.25 -1.5) (end 7.75 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1cf1aa57-164c-4cbc-9bb7-813f42474613))
    (fp_line (start 7.75 -1.5) (end 8 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e862fd6d-3d99-4df0-8b4a-efe6f75acfa0))
    (fp_line (start 7.75 6) (end -1.25 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8ac15f16-4666-4106-b8a5-747ee3366af9))
    (fp_line (start 7.75 6) (end 8 6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4393a579-9580-45bc-a7e1-91aa142b21d4))
    (fp_line (start 8 -1.5) (end 8 -1.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 35c4efe1-0a14-449f-9f70-5842ec9dd68c))
    (fp_line (start 8 -1.25) (end 8 5.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cd8107c0-8d0f-4b53-846b-af845d8a4e9e))
    (fp_line (start 8 6) (end 8 5.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 631e3ccf-234b-48a2-9900-18f7e81f9444))
    (fp_line (start 0.25 -0.75) (end 3.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e1a6f2d-4827-4ba1-b8d1-5af65a6852d2))
    (fp_line (start 0.25 5.25) (end 0.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2299faca-94eb-47f1-b4f0-76ff9f8ee7d0))
    (fp_line (start 3.25 -0.75) (end 6.25 -0.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b02d5988-646f-4c7f-9b98-63e408b062d4))
    (fp_line (start 6.25 -0.75) (end 6.25 5.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91d30a44-4815-461e-bf49-87d1e68e487a))
    (fp_line (start 6.25 5.25) (end 0.25 5.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1cb2d1dc-5242-4349-854d-d2ea5eb16612))
    (fp_circle (center 3.25 2.25) (end 1.25 2.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp a84ef6a8-55a6-419e-9050-4b88919609d3))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 126 "unconnected-(SW3-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 49a58166-de72-4600-8add-69594c04663f))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 126 "unconnected-(SW3-Pad1)") (pinfunction "1") (pintype "passive") (tstamp d08386f6-9df2-49ad-b616-5bea651a8820))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 127 "unconnected-(SW3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 5ccfbb2f-2e25-4350-876a-e5a3aebe6dbe))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 127 "unconnected-(SW3-Pad2)") (pinfunction "2") (pintype "passive") (tstamp 41c4e93c-b691-4536-9130-0e15dc574d2e))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_QFP:QFP80P900X900X160-32N" (layer "F.Cu")
    (tstamp ed6834f2-3a52-4d04-a924-95ae68a61a37)
    (at 135.6 77.78)
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "usb")
    (path "/608a5705-96be-4a71-b2b6-c4625a5aee39/6a322a84-024e-46e4-a7d9-cc60be36fc15")
    (attr smd)
    (fp_text reference "U19" (at -1.825 -6.135) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d6c5f95e-c3e1-412f-b01d-7a1f2634ae2b)
    )
    (fp_text value "TUSB2046BVFR" (at 8.335 6.135) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a1f4c88-e944-42a4-b708-ef77bbfa58ad)
    )
    (fp_line (start -3.5 -3.5) (end -3.5 -3.39)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp cd934877-ee5b-4c73-8bc9-13cac812fa0a))
    (fp_line (start -3.5 -3.5) (end -3.39 -3.5)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp c5bf922a-8671-4673-a111-febac72ce7da))
    (fp_line (start -3.5 3.5) (end -3.5 3.39)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 9f8ff452-b50a-4041-a26a-9e9a01d0753a))
    (fp_line (start -3.5 3.5) (end -3.39 3.5)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 724bb066-f6b4-4784-886e-0eb9ebd9a7b6))
    (fp_line (start 3.5 -3.5) (end 3.39 -3.5)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp ab78c3f1-506b-42ec-b4ce-c43e143c13a3))
    (fp_line (start 3.5 -3.5) (end 3.5 -3.39)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 89dc6175-1a25-4132-b56b-a45b8cc3cf23))
    (fp_line (start 3.5 3.5) (end 3.39 3.5)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 726a6326-651e-4d8f-95a0-84dcd63db487))
    (fp_line (start 3.5 3.5) (end 3.5 3.39)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 063b2cbc-dd29-4a69-a052-ca47c2ca3f09))
    (fp_circle (center -5.94 -2.8) (end -5.84 -2.8)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.SilkS") (tstamp 2228e717-4eac-4244-921b-d1bd5d707d9b))
    (fp_line (start -5.21 -5.21) (end 5.21 -5.21)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 70f1d3ac-1ea1-464b-ba53-4eacda3d48f7))
    (fp_line (start -5.21 5.21) (end -5.21 -5.21)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 075868ea-a1a8-44d7-bee0-01c0b0c260bf))
    (fp_line (start -5.21 5.21) (end 5.21 5.21)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e67f939-963c-46a2-875a-a9aa3d947f77))
    (fp_line (start 5.21 5.21) (end 5.21 -5.21)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc9eb350-6107-4ec3-b744-22f4ac34b889))
    (fp_line (start -3.5 3.5) (end -3.5 -3.5)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp b3a0ef88-921e-4815-8cf2-9e7db7741927))
    (fp_line (start 3.5 -3.5) (end -3.5 -3.5)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 52974997-b160-4df4-a0fa-61a16710cc58))
    (fp_line (start 3.5 3.5) (end -3.5 3.5)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp 915012aa-17b7-4b75-a012-ecc653c2db87))
    (fp_line (start 3.5 3.5) (end 3.5 -3.5)
      (stroke (width 0.127) (type solid)) (layer "F.Fab") (tstamp ddbc241e-cc29-4413-8a00-2ce473f26cf1))
    (fp_circle (center -5.94 -2.8) (end -5.84 -2.8)
      (stroke (width 0.2) (type solid)) (fill none) (layer "F.Fab") (tstamp 32b31c51-613d-407e-b55e-975831ae87a2))
    (pad "1" smd roundrect (at -4.18 -2.8) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 831 "unconnected-(U19-DP0-Pad1)") (pinfunction "DP0") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp e2ffcf25-314f-4fc7-9bff-0fac3d6677d8))
    (pad "2" smd roundrect (at -4.18 -2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 832 "unconnected-(U19-DM0-Pad2)") (pinfunction "DM0") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 43c69cc0-d6df-4661-84af-bd2c8a780094))
    (pad "3" smd roundrect (at -4.18 -1.2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 833 "unconnected-(U19-VCC-Pad3)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 9e2214b5-347c-4eee-9215-5e6694a23534))
    (pad "4" smd roundrect (at -4.18 -0.4) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 834 "unconnected-(U19-~{RESET}-Pad4)") (pinfunction "~{RESET}") (pintype "input") (solder_mask_margin 0.102) (tstamp ed1a6159-dd7d-4c4c-b7a8-109f9c245929))
    (pad "5" smd roundrect (at -4.18 0.4) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 835 "unconnected-(U19-EECLK-Pad5)") (pinfunction "EECLK") (pintype "output") (solder_mask_margin 0.102) (tstamp 9128cea7-e9fb-408a-910e-39a457794934))
    (pad "6" smd roundrect (at -4.18 1.2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 836 "unconnected-(U19-EEDATA{slash}GANGED-Pad6)") (pinfunction "EEDATA/GANGED") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 089136df-b7fb-47b7-960c-dd067414d6c6))
    (pad "7" smd roundrect (at -4.18 2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 837 "unconnected-(U19-GND-Pad7)") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 32c9ddbe-58fe-4daa-bb8f-443c3323dd1e))
    (pad "8" smd roundrect (at -4.18 2.8) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 838 "unconnected-(U19-BUSPWR-Pad8)") (pinfunction "BUSPWR") (pintype "input") (solder_mask_margin 0.102) (tstamp ff9937ab-209b-4a76-838a-7316a06b1f43))
    (pad "9" smd roundrect (at -2.8 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 839 "unconnected-(U19-~{PWRON1}-Pad9)") (pinfunction "~{PWRON1}") (pintype "output") (solder_mask_margin 0.102) (tstamp 8d522ead-74bb-453d-8ad2-218070262552))
    (pad "10" smd roundrect (at -2 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 840 "unconnected-(U19-~{OVRCUR1}-Pad10)") (pinfunction "~{OVRCUR1}") (pintype "input") (solder_mask_margin 0.102) (tstamp f04c33ae-9248-49d1-9753-224a86bc6d87))
    (pad "11" smd roundrect (at -1.2 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 841 "unconnected-(U19-DM1-Pad11)") (pinfunction "DM1") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 683a7c42-7f5a-4647-8667-d13f83f2e30d))
    (pad "12" smd roundrect (at -0.4 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 842 "unconnected-(U19-DP1-Pad12)") (pinfunction "DP1") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 6c62ace4-34c0-42e1-b17d-65bf23c1d417))
    (pad "13" smd roundrect (at 0.4 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 843 "unconnected-(U19-~{PWRON2}-Pad13)") (pinfunction "~{PWRON2}") (pintype "output") (solder_mask_margin 0.102) (tstamp a027fee6-c723-46f7-bdde-cfef34aa545a))
    (pad "14" smd roundrect (at 1.2 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 844 "unconnected-(U19-~{OVRCUR2}-Pad14)") (pinfunction "~{OVRCUR2}") (pintype "input") (solder_mask_margin 0.102) (tstamp afc54932-56e0-44d2-b2a9-b1f353b1bffd))
    (pad "15" smd roundrect (at 2 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 845 "unconnected-(U19-DM2-Pad15)") (pinfunction "DM2") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp c1580f6d-99fd-44cf-b37c-e7c9c6e57ca7))
    (pad "16" smd roundrect (at 2.8 4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 846 "unconnected-(U19-DP2-Pad16)") (pinfunction "DP2") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 663dc8ae-918c-403d-9632-448183faf55d))
    (pad "17" smd roundrect (at 4.18 2.8) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 847 "unconnected-(U19-~{PWRON3}-Pad17)") (pinfunction "~{PWRON3}") (pintype "output") (solder_mask_margin 0.102) (tstamp d0a1cc39-e757-427d-ae62-eec19657e63d))
    (pad "18" smd roundrect (at 4.18 2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 848 "unconnected-(U19-~{OVRCUR3}-Pad18)") (pinfunction "~{OVRCUR3}") (pintype "input") (solder_mask_margin 0.102) (tstamp 96adf55b-b8e9-4569-8f38-14d613d6974c))
    (pad "19" smd roundrect (at 4.18 1.2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 849 "unconnected-(U19-DM3-Pad19)") (pinfunction "DM3") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp e0c5b699-8862-45e6-be3b-dd6e963c1a79))
    (pad "20" smd roundrect (at 4.18 0.4) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 850 "unconnected-(U19-DP3-Pad20)") (pinfunction "DP3") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp bb1cc702-57a0-4e61-b0c4-85968446b7d7))
    (pad "21" smd roundrect (at 4.18 -0.4) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 851 "unconnected-(U19-~{PWRON4}-Pad21)") (pinfunction "~{PWRON4}") (pintype "output") (solder_mask_margin 0.102) (tstamp 15f31c75-a6c7-423a-80db-8e4d6a6208f5))
    (pad "22" smd roundrect (at 4.18 -1.2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 852 "unconnected-(U19-~{OVRCUR4}-Pad22)") (pinfunction "~{OVRCUR4}") (pintype "input") (solder_mask_margin 0.102) (tstamp 5784391b-5eba-4d37-84a1-ba3ef66681d2))
    (pad "23" smd roundrect (at 4.18 -2) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 853 "unconnected-(U19-DM4-Pad23)") (pinfunction "DM4") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp d2fe1239-792e-4a89-838d-d057a1868414))
    (pad "24" smd roundrect (at 4.18 -2.8) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 854 "unconnected-(U19-DP4-Pad24)") (pinfunction "DP4") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp 728e1e1c-0071-4444-9a99-ac808dfe8a1d))
    (pad "25" smd roundrect (at 2.8 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 855 "unconnected-(U19-VCC__1-Pad25)") (pinfunction "VCC__1") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 1af3bea2-3f66-4274-a4ff-0f3c2d030b04))
    (pad "26" smd roundrect (at 2 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 856 "unconnected-(U19-~{EXTMEM}-Pad26)") (pinfunction "~{EXTMEM}") (pintype "input") (solder_mask_margin 0.102) (tstamp 5ce3f55e-1524-4596-83c0-615370f72bf3))
    (pad "27" smd roundrect (at 1.2 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 857 "unconnected-(U19-TSTPLL{slash}48MCLK-Pad27)") (pinfunction "TSTPLL/48MCLK") (pintype "bidirectional") (solder_mask_margin 0.102) (tstamp c671bb3f-8c48-4895-a086-f0b313457aa0))
    (pad "28" smd roundrect (at 0.4 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 858 "unconnected-(U19-GND__1-Pad28)") (pinfunction "GND__1") (pintype "power_in") (solder_mask_margin 0.102) (tstamp 67b434b3-f3ed-47db-9b35-1b134f088151))
    (pad "29" smd roundrect (at -0.4 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 859 "unconnected-(U19-XTAL2-Pad29)") (pinfunction "XTAL2") (pintype "output") (solder_mask_margin 0.102) (tstamp 9f03db47-f7b7-4694-a5ac-9c71d5a4ccc8))
    (pad "30" smd roundrect (at -1.2 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 860 "unconnected-(U19-XTAL1-Pad30)") (pinfunction "XTAL1") (pintype "input") (solder_mask_margin 0.102) (tstamp c194653b-25ed-4b0d-a16c-22c9a6e256ec))
    (pad "31" smd roundrect (at -2 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 861 "unconnected-(U19-TSTMODE-Pad31)") (pinfunction "TSTMODE") (pintype "input") (solder_mask_margin 0.102) (tstamp 3f2f6b03-6579-462a-a774-30f52fbebdb9))
    (pad "32" smd roundrect (at -2.8 -4.18 90) (size 1.56 0.54) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 862 "unconnected-(U19-SUSPND-Pad32)") (pinfunction "SUSPND") (pintype "output") (solder_mask_margin 0.102) (tstamp c3e70ce3-8eb2-439a-bb39-3508ca14b09f))
    (model ":KICAD7_3DMODEL_DIR:Package_QFP.3dshapes/TUSB2046BVFR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "Display_7Segment:LTS-4802B" (layer "F.Cu")
    (tstamp f10275a5-2fdd-4600-a983-db7ed6936648)
    (at 94.5 90.34)
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/54d244b9-38de-4dbb-b74e-677d10e595c2")
    (attr through_hole)
    (fp_text reference "U15" (at 0 -2.54 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9a6ab636-0b22-4a80-8087-c89cad7d9504)
    )
    (fp_text value "~" (at 3.58 13.1 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp df227234-b464-4f2b-8c82-68044db42ced)
    )
    (fp_text user "${REFERENCE}" (at 3.58 4.01 unlocked) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 257f937f-1847-4e66-93e7-269b8e892b41)
    )
    (fp_rect (start -1.04 -1.07) (end 8.66 11.83)
      (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 0ae6b439-58b6-4371-a973-6ee9458b5130))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 781 "unconnected-(U15-CA-Pad1)") (pinfunction "CA") (pintype "passive") (tstamp eb533cee-3ddd-48f9-9473-8c5b490523fe))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 782 "unconnected-(U15-F-Pad2)") (pinfunction "F") (pintype "passive") (tstamp e6c07d01-9743-4e41-88d9-975126ee7724))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 783 "unconnected-(U15-G-Pad3)") (pinfunction "G") (pintype "passive") (tstamp 38bff38c-e3d6-4b72-b458-c3d49f7c0f91))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 784 "unconnected-(U15-E-Pad4)") (pinfunction "E") (pintype "passive") (tstamp dc8f6b4b-0bf1-4b55-853b-f217e3e7cb11))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 785 "unconnected-(U15-D-Pad5)") (pinfunction "D") (pintype "passive") (tstamp 22f3faab-3aff-48dd-96f4-26efc108671f))
    (pad "6" thru_hole circle (at 7.62 10.16) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 786 "unconnected-(U15-CA-Pad6)") (pinfunction "CA") (pintype "passive") (tstamp d3d71493-3571-4deb-bbd1-68abe0a423b2))
    (pad "7" thru_hole circle (at 7.62 7.62) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 787 "unconnected-(U15-DP-Pad7)") (pinfunction "DP") (pintype "passive") (tstamp 7a1e089a-7146-447f-8932-87e7d3cf03ff))
    (pad "8" thru_hole circle (at 7.62 5.08) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 788 "unconnected-(U15-C-Pad8)") (pinfunction "C") (pintype "passive") (tstamp a8b11024-90e5-4188-b147-2263f19b681d))
    (pad "9" thru_hole circle (at 7.62 2.54) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 789 "unconnected-(U15-B-Pad9)") (pinfunction "B") (pintype "passive") (tstamp d74020aa-0b34-4e27-b734-3750ce46f803))
    (pad "10" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 790 "unconnected-(U15-A-Pad10)") (pinfunction "A") (pintype "passive") (tstamp 4a431c50-ef24-482f-978f-271f33f356f8))
    (model ":KICAD7_3DMODEL_DIR:Display_7Segment.3dshapes/LTS-4802BJR-H1_LTO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tstamp f75011ad-829e-42f9-9db8-8fdfc4d3b2b9)
    (at 80.32 62.625 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "board_io.kicad_sch")
    (property "Sheetname" "board_io")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/97b7ebae-6d0e-40d9-8e3a-8f6a0baafdc2/3010f977-fe60-4c95-88eb-4a33b03d6cee")
    (attr smd)
    (fp_text reference "D6" (at 0 -1.43 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a09b7f05-7ed5-4adb-8f64-e578842f27fe)
    )
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 781c0253-6371-4f5e-a532-c13d83cdc5d9)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp d34ef06a-3db7-411e-b4ff-6af9e8baf5f1)
    )
    (fp_line (start -1.66 -0.735) (end -1.66 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66abfb99-5182-41fd-aebf-66dd45285c34))
    (fp_line (start -1.66 0.735) (end 0.8 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c323d24f-316d-4dbd-a663-c5edb42db2dc))
    (fp_line (start 0.8 -0.735) (end -1.66 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3afb6010-4cdc-45d5-9bc4-462d952f54c1))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dc91587c-7961-4ce0-a233-5f5cc59a8844))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a2d6d676-224c-4328-933b-60d57f947ebd))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ed13dfa1-201e-4dee-994e-7fdccf203b9c))
    (fp_line (start 1.65 0.73) (end -1.65 0.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ecd59ddb-a08f-4ebf-9347-3256de8ff618))
    (fp_line (start -0.8 -0.1) (end -0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bd246aac-98c8-436e-9fe4-a752b25e61b7))
    (fp_line (start -0.8 0.4) (end 0.8 0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e6601092-50c9-4b23-9246-cff468eb5a3c))
    (fp_line (start -0.5 -0.4) (end -0.8 -0.1)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3302bfae-fbd1-4fd4-af6e-fa95fab978cf))
    (fp_line (start 0.8 -0.4) (end -0.5 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1d94d45-8e3f-4e9b-bd60-c1e3ad6a2bee))
    (fp_line (start 0.8 0.4) (end 0.8 -0.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92120080-dc07-4a2b-9468-cbb27c3ee9fe))
    (pad "1" smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "unconnected-(D6-K-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 6c37aabb-cf5c-4dc1-afd8-d075f9bafa7a))
    (pad "2" smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "unconnected-(D6-A-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 3274f1c9-7ec0-4c6d-a334-28f8d7b0fca9))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

)
